arXiv:1209.1120v1 [physics.ins-det] 5 Sep 2012

The MINERνA Data Acquisition System and Infrastructure

G. N. Perdue^{p,∗}, L. Bagby^c, B. Baldin^c, C. Gingu^c, J. Olsen^c, P. Rubinov^c, E. C. Schulte^{h,1}, R. Bradford^{p,2}, W. K. Brooks^k, D. A. M. Caicedo^a, C. M. Castromonte^a, J. Chvojka^p, H. da Motta^a, I. Danko^n, J. Devan^b, B. Eberly^n, J. Felix^i, L. Fields^f, G. A. Fiorentini^a, A. M. Gago^g, R. Gran^o, D. A. Harris^c, K. Hurtado^{a,j}, H. Lee^p, E. Maher^e, S. Manly^p, C. M. Marshall^p, K. S. McFarland^p, A. Mislivec^p, J. Mousseau^m, B. Osmanov^m, J. Osta^c, V. Paolone^n, R. D. Ransome^h, H. Ray^m, D. W. Schmitz^c, C. Simon^l, C. J. Solano Salinas^j, B. G. Tice^h, T. Walton^d, J. Wolcott^p, D. Zhang^b, B. P. Ziemer^l

aCentro Brasileiro de Pesquisas Físicas, Rua Dr. Xavier Sigaud 150, Urca, Rio de Janeiro, RJ, 22290-180, Brazil bDepartment of Physics, College of William & Mary, Williamsburg, Virginia 23187, USA cFermi National Accelerator Laboratory, Batavia, Illinois 60510, USA dHampton University, Dept. of Physics, Hampton, VA 23668, USA eMassachusetts College of Liberal Arts, 375 Church Street, North Adams, MA 01247, USA fNorthwestern University, Evanston, Illinois 60208, USA gSección Física, Departamento de Ciencias, Pontificia Universidad Católica del Perú, Apartado 1761, Lima, Perú hRutgers, The State University of New Jersey, Piscataway, New Jersey 08854, USA iUniversidad de Guanajuato. Lascuraín de Retana No. 5. Col. Centro. Guanajuato 37150, Guanajuato. México jUniversidad Nacional de Ingeniería, Tupac Amaru Avenue 210, Lima, Perú kDepartamento de Física, Universidad Técnica Federico Santa María, Avda. España 1680 Casilla 110-V Valparaíso, Chile lDepartment of Physics and Astronomy, University of California – Irvine, Irvine, California 92697-4575, USA mDepartment of Physics, University of Florida, Gainesville, FL 32611,USA nDepartment of Physics and Astronomy, University of Pittsburgh, Pittsburgh, Pennsylvania 15260, USA

∗Corresponding Author Email address: perdue@fnal.gov (G. N. Perdue) 1Present Address: Temple University, Philadelphia, PA 19122-6099, USA 2Present Address: Argonne National Laboratory, 9700 S. Cass Avenue, Lemont, IL 60439, USA

Preprint submitted to Nucl. Instrum. Methods A July 9, 2022 oDepartment of Physics, University of Minnesota – Duluth, Duluth, Minnesota 55812, USA pUniversity of Rochester, Rochester, New York 14610 USA

Abstract

MINERνA (Main INjector ExpeRiment ν-A) is a new few-GeV neutrino cross section experiment that began taking data in the FNAL NuMI (Fermi National Accelerator Laboratory Neutrinos at the Main Injector) beam-line in March of 2010. MINERνA employs a fine-grained scintillator detector capable of complete kinematic characterization of neutrino interactions. This paper describes the MINERνA data acquisition system (DAQ) including the read-out electronics, software, and computing architecture.

Keywords: DAQ, Data Acquisition, Minerva, Neutrinos

1. Introduction 1 MINERνA (Main INjector ExpeRiment ν-A) is a low-to-medium energy 2 neutrino-nucleus scattering experiment at FNAL (Fermi National Accelerator 3 Laboratory). It utilizes the high-intensity NuMI (Neutrinos at the Main 4 Injector) beamline and sits in the MINOS (Main Injector Neutrino Oscillation 5 Search) Near Detector Hall, directly in front of the MINOS Near Detector 6 and 105 meters below grade. MINERνA does not extend far enough in the 7 beam direction to range out muons with momentum over about 2 GeV/c, 8 so the MINOS Near Detector is directly employed as a muon spectrometer. 9 The references contain more detailed information on the physics program 10 and general details of MINERνA^1, MINOS^2, and the NuMI beam^3. 11 This document discusses the MINERνA data acquisition system (DAQ) 12 in two steps. First, the custom electronics are described, followed by a de- 13 scription of the DAQ software and computing architecture. 14 The initial specifications for the DAQ readout system asked for a readout 15 rate of ∼100 kB/s with a duty factor defined by one ∼ 10 microsecond beam 16 spill every 2.2 seconds^4. Fortunately, those specifications were surpassed as 17 our initial estimate for required data throughput was low by about a factor 18 of five. 19

2. Overview of the Readout Scheme in MINERνA 20 The DAQ, slow controls (SC), and near-online monitoring (“nearline”) 21 systems are built around MINERνA-specific readout electronics. MINERνA 22 utilizes plastic scintillator as its fundamental detector technology. Light 23 is delivered via wavelength shifting fiber to Hamamatsu R7600 64-channel 24 multi-anode photomultiplier tubes (PMTs)^5. A small number of single-anode 25 PMTs are also mounted for a “Veto Wall” detector that sits in front of the 26 main MINERνA detector. 27 Each PMT is read out by a Front End Board (FEB)^6 mounting six 28 Application-Specific Integrated Circuit (ASIC) chips (TriP-t chips)^7 that dig- 29 itize and store charge using pipeline ADCs. Input charges from the PMT an- 30 odes are divided into high, medium, and low gain channels using a capacitive 31 divider to increase the dynamic range. The high gain is 1.25 fC/ADC, the 32 medium is 4 fC/ADC, and the low is 15.6 fC/ADC. The FEBs generate the 33 high voltage for most of the PMTs using an on-board Cockroft-Walton (CW) 34 generator. The control circuitry resides on the FEB, while the CW chain it- 35 self resides on the base, with appropriate taps for each dynode. A small 36 number of the PMTs are single-anode and use resistor-base technology for 37 voltage control. These PMTs are used to read out the Veto Wall and employ 38 a separate voltage control system discussed below. All FEB operations are 39 controlled by a Spartan 3E Field-Programmable Gate Array (FPGA) chip. 40 The FPGAs decode timing signals received over the unshielded twisted pair 41 (UTP) cables, sequence the TriP-t chips and decode and respond appropri- 42 ately to communication frames received over the data link. The FPGA also 43 controls the CW and other aspects of FEB operation. For data collection, 44 the boards are daisy-chained together (into “chains”) using standard UTP 45 ethernet networking cables with a custom protocol and Low Voltage Differ- 46 ential Signaling (LVDS). Of the four pairs in the cable, one is dedicated to 47 timing, including clock and encoded signals, one is dedicated for data, one 48 is used to indicate the sync-lock status of the data Serializer/Deserializer 49 (SERDES) and one for a test pulse. 50 The readout chain is connected at both ends to a custom VME mod- 51 ule called the Chain ReadOut Controller (CROC)^8. A CROC supports four 52 Front End (FE) channels, each serving one chain of up to fifteen FEBs, 53 though no chain is longer than ten FEBs in MINERνA. Each of the four 54 CROC channels contains a 6 kB dual-port memory for storing messages 55 (called “frames”) from the FEBs. The CROCs in turn receive timing and 56

trigger commands from another custom VME module, the CROC Interface 57 Module (CRIM)^8, each of which distributes timing to up to four CROCs. 58 MINERνA uses two VME crates, each containing a CAEN V2718 crate con- 59 troller^9, two CRIMs, and roughly a half-dozen CROCs. There is no hit-based 60 trigger but rather a timing-based integration gate synchronized to the FNAL 61 Main Injector (MI) timing signals. Finally, the CRIMs receive information 62 from the timing system of the MINOS experiment (used for event match- 63 ing) and the state of the MI via the MINERνA Timing Module (MvTM)^{10}. 64 The MvTM does not have a VME interface, but uses the VME crate for 65 power. The start time in MINOS detector timing coordinates is logged as 66 a 28-bit number in the DAQ Header bank data. See Table 1 for a com- 67 plete module and card accounting. Only one MvTM is required to service all 68 timing needs. Each individual crate is readout by a computer (PC) mount- 69 ing a CAEN A2818 PCI card^{11} that communicates with the crate controller 70 module via optical cable. 71 Era VME Crates CROCs FEBs Total Channels Fall 2009 2 8 272 17,408 Spring 2010 2 14 491 31,424 Summer 2010 + 2 15 509 32,576

Table 1: MINERνA read-out hardware installations.

An integration gate on the FEBs is opened synchronously with the de- 72 livery of neutrino beam spills. Beam spills delivered by the MI are approx- 73 imately 10 microseconds long, and are delivered every 2.2 or 2.06 seconds, 74 depending on the MI operating mode. Our readout gate opens 500 nanosec- 75 onds before the arrival of the spill and remains open 5.5 microseconds af- 76 ter the end. During normal data-taking, one additional calibration gate is 77 recorded between neutrino spills, either a random sampling of the detector 78 noise (a pedestal gate) or in coincidence with LEDs flashing the PMTs (a 79 “light-injection” gate). Pedestals are used to establish baseline readout lev- 80 els and light-injection to monitor gain drifts in the PMTs by studying the 81 photo-statistics of the LED signals. 82 At the end of the gate, the readout system runs a software loop over all 83 of the FEBs and collects data in the form of device “frames” (well-defined 84 and formatted byte data with attached headers) one at a time for the state 85 of the high-voltage, hit timing, and finally the hit blocks themselves. Each 86

frame is passed through a chain to a CROC FE channel where it is stored 87 briefly before being passed to a readout computer for archival and monitoring 88 processes. 89 Readout of the electronics is done in pairs of nested loops. Requests for 90 data are sent to the first FEB on each FE channel before looping back to 91 retrieve the data from the CROC memory. Then the next set of FEBs are 92 handled in another dual loop over FE channels, etc. This allows the DAQ 93 computers to communicate with the next CROC while the previous one is 94 fetching data from the FEBs on one of its readout chains. 95 In normal data-taking MINERνA reads out in a “zero suppression” mode. 96 In this mode, the DAQ first reads the discriminator frame data for each 97 board and stores frames that contain hits above the discriminator threshold 98 (about 70 fC). It then loops over those boards and reads the FPGA registers 99 and all time-stamped ADC hit block frames. The FEBs are configured to 100 enable readout of up to eight ADC blocks: seven time-stamped hits and 101 one “un-timed” hit at the end of the integration gate. The un-timed hit 102 carries no discriminator timing information and contains all the integrated 103 charge between the last timed hit and the end of the gate. The FPGA 104 registers contain configuration data, high-voltage read-back, and the local 105 “gate time stamp” - the time the gate was opened for integration in the local 106 FEB counter time coordinates. Boards without hits above threshold are not 107 read out in this loop and neither are un-time-stamped ADC frames (charge 108 collected below threshold and stored until the end of the integration gate). 109 All seven available time-stamped hits are read out. During construction 110 and early low-energy configuration running, a configuration with five time- 111 stamped hits and one “un-timed” end-of-gate hit was used. See Table 2 for 112 a listing of the sizes of each data type. 113 Despite using more than 32,000 active channels in MINERνA, the quan- 114 tity of data per neutrino spill is not large due to low interaction cross-sections. 115 With a 2.2 second MI cycle and 35 × 10^{12} protons on target per spill, roughly 116 1 MB per spill for the entire detector in zero-suppression mode running in 117 the NuMI low-energy configuration is collected, where the most frequent neu- 118 trino energy is ∼3 GeV. About half of those data are beam spill data and 119 half are calibration data. 120 Readout time for a single frame is approximately 500 microseconds. Most 121 of that time is in message preparation and in setting up a block transfer; for 122 our data the readout speeds per frame are largely insensitive to the size of the 123 frame. Physics gate readouts typically require 1200 frames on average, while 124

Frame Type Size (bytes) Comments FPGA Programming 66 Spartan 3E control registers.

ADC 444 Hit data.

Discriminator 16 + 40 per Time stamps for each hit. TriP-t per hit TriP Programming 652 (read) TriP-t internal registers. 758 (write) DAQ Header 48 Not a true “frame.” → End of gate marker.

Table 2: Frame sizes per FEB for MINERνA data objects. The FPGA programming frames track configuration details and provide data on the high voltage, gate initiation time, and some useful error-checking bits. The TriP-t chips were originally designed for the D0 experiment^{12} and so carried timing data that is not usable by MINERνA. These data were trimmed in the packing algorithm for more efficient use of space. This reduced storage bloat, but did not meaningfully impact speed. Only discriminator frames are of variable size. The TriP-t programming frames are not read or written to during data acquisition. They are only accessed during configuration stages by the slow controls.

calibration gate readouts require 1600 (channel occupancy is lower in physics 125 gates). Therefore, reading a typical “cycle” (single physics gate plus single 126 calibration gate) requires 1.4 seconds. Calibration readout times are very 127 stable, but physics gate readout times vary with the level of activity in the 128 detector. The DAQ is programmed to protect the integrity of physics gates 129 above all else. It will only attempt a calibration readout in the case where 130 the physics readout is accomplished in under 0.9 seconds. If the subsequent 131 calibration readout extends beyond 0.9 seconds, the DAQ will dump that 132 readout and simply arm for the next physics spill. However, the DAQ will 133 not interrupt readout of a physics gate. Propagation of the start gate signal 134 is blocked in hardware and only unlatched after readout is complete. 135 3. System-Wide Timing Signals 136 Time-stamps are recorded for the MINERνA experiment using a single 137 53.1 MHz crystal on the MvTM which is distributed to all of the electronics 138 components - from MvTM to the CRIMs, from the CRIM to the CROCs, 139 from the CROCs to the FEBs. See Fig. 1 for an illustration of the timing 140 signals loop. Each board regenerates the clock using phase-locked loop (PLL) 141

circuits. The 53.1 MHz clock is distributed on the readout cable, but the 142 FEBs use the onboard PLL to multiply the frequency by two. All times in 143 MINERνA are defined in units of system ticks, or clock ticks. A clock tick 144 is equal to 145 1/f = 1/(2 × 53.1 × 10^6 Hz) = 9.4 ns (1) Additionally the FPGA on the FEB uses a quadrature circuit, providing a 146 granularity of ∼2.4 ns for the discriminator time stamps. Throughout the 147 remainder of this document, the term “clock tick” will refer to the unit used 148 by the FEBs (∼9.4 ns) unless explicitly noted otherwise. 149

Figure 1: The DAQ Loop Timing Signals.^{13}

The FEBs, CROCs and CRIMs can operate using on board oscillators, 150 but FEBs and CROCs in MINERνA are always operated by synchronizing 151 their clocks to a radio frequency (RF) signal provided by the CRIMs. The 152 CRIMs are typically operated in “MvTM Mode,” and locked to the MvTM 153 clock, but in certain situations are placed in “Internal Mode,” where the 154 clock is supplied by the internal crystal oscillator. See Table 3. MINERνA 155 electronics were designed to operate without a trigger, so the cosmic and 156 Test-Beam modes are special. In those cases, a coincidence between a live 157 gate (≈ 16 μs wide) and an external logic pulse is searched for in order to 158 make readout decisions. Because of dead-time between gates, the live-time 159 is low in those operating modes (∼ 10%). 160

Data-Taking Mode CRIM Clock Mode Pedestal Internal Cosmic Rays Internal FTBF (Test-Beam) Beam Internal NuMI Beam MvTM Light Injection (LI) MvTM Mixed Mode (Beam with LI or Pedestal) MvTM

Table 3: CRIM timing modes for different data-taking modes. “FTBF” refers to the Fermilab Test Beam Facility.

When operating in the internal timing mode, each CRIM supplies its own 161 clock and either the DAQ system sends a new open-gate command after each 162 successful readout or the CRIM opens the gates independently at a frequency 163 set by the user ranging between 0.5 Hz and 52 kHz. The first sort of internal 164 clock mode operation is used for standalone pedestal runs and the second 165 requires an external trigger in coincidence to initiate readout (cosmic or test 166 beam). 167 Encoded clock and trigger signals enter the CROCs over LVDS via RJ-45 168 input connectors: 169 1. RF - Radio Frequency 170 2. SGATE - Start Gate (open an integration gate) 171 3. CNRST - Counter Reset 172 4. FCMND - Fast Command (special commands) 173 5. TCALB - Timing Calibration Pulse 174 See Fig. 2 for the structure of the encoded commands on the clock line. 175 In either Internal or MvTM timing mode, the CRIM can receive exter- 176 nal signals via a set of LEMO connectors on its front panel or via an RJ-45 177 connector. The MvTM is able to recieve timing signals from the MINOS 178 Master Timing Module over UTP Cat5e using LVDS. The MvTM addition- 179 ally can send and relay Low Voltage Transistor-Transistor Logic (LVTTL) 180 signals through the pairs of in-and-out LEMO connectors. One LEMO in- 181 put is used to receieve a LVTTL signal providing MI cycle status from the 182 Accelerator Division (this signal ultimately detemines the start-gate time). 183 The other two LEMO connectors are used to fire the light injection system 184 (discussed later). 185

Figure 2: The Timing Encoder Signals.^{13}

During normal operation, the CRIM clock is derived from the MvTM. In 186 principle, the MvTM can sync to the MINOS clock signal but it runs free 187 against that clock and the MvTM internal oscillator is used to synchronize 188 all of the clocks. The arrival time of the MINOS start-gate signal is recorded 189 in a register in the CRIM, however. The MINOS and MINERνA clocks are 190 therefore running in sync with an unknown phase shift. When in MvTM 191 mode, the CRIM will raise an interrupt when an external trigger pulse is 192 detected - for example, when the spill signal comes from the MI. This inter- 193 rupt begins the readout sequence and blocks until it is reset after readout is 194 complete. Fig. 3 illustrates the timing module logic. 195 The CRIM interprets Start-gate (SGATE), trigger (TRIG), timing cali- 196 bration (TCALB), and counter-reset (CNRST) LVTTL signals and generates 197 corresponding output in a slightly different way for each of the different tim- 198 ing modes. 199 1. SGATE is sent through SGATE OUT in all timing modes. 200 2. TRIG is sent only in MvTM mode, and only in case of a software 201 command to open a gate. 202 3. TCALB is sent synchronously with SGATE in most CRIM firmware 203 versions. It can be configured to only send this signal when an external 204 TRIG is supplied. 205 4. CNRST is sent synchronously with SGATE in most CRIM firmware 206 versions. The FEBs interpret this as a “Counter Load” signal and set 207 their counters to a value specified in the FPGA programming registers. 208 This is part of the timing synchronization scheme for the FEBs. 209

Figure 3: The CRIM (timing module) block diagram.^{14}

The clock and data travel only in one direction over the readout chains- from 210 the CROC to each of the FEBs in turn and arriving back at the CROC. The 211 CROC checks that the clock is present at the receiving end and will set an 212 error flag if it is not. Further data acquisition is not possible until this error 213 is cleared. 214 Our configuration for data-taking in the NuMI hall is: 215 1. A LEMO cable from the accelerator division rack is attached to LEMO 216 input 1 on the MvTM. A signal synchronized with the MI operational 217 cycle arrives ∼215 μs before a spill. A delay is programmed into the 218 FEB FPGA’s to account for the offset. This signal is sent to the CRIM 219 from the MvTM via a CAT3 cable, and propagated from there through 220 the CROCs to the FEBs. The FEBs use only the rising edge of the 221 SGATE signal to open a gate. The falling edge is ignored. 222 2. A dedicated CAT3 cable is routed from the MINOS clock rack into 223 the Master Clock Interface connector on the MvTM. This cable car- 224 ries CNRST, TCALB, and SGATE encoded clock signals. The CRIM 225 receives those signals as: 226 • MINERνA CNRST - MINOS CNRST. Set by the MINOS GPS 227 clock to reset asynchronous to the other signals at a rate of 1 Hz. 228 This signal is currently masked from the FEBs, but used to reset 229 the counter on the CRIM. 230 • MINERνA TCALB - The MINOS SGATE signal is mapped here 231 in the MvTM. The clock time is recorded (using on-board coun- 232 ters) for the arrival of this signal and stored on a register in the 233 CRIM that is read at the end of the acquisition cycle. 234 • MINERνA SGATE - This receiver is masked within the MvTM 235 and the CRIM never sees a signal of this type. 236 3. All of the CRIMs are daisy-chained together via the TRIG port, going 237 out from the “Master CRIM” (the CRIM with the lowest address in 238 the VME crate with the lowest address) and then in and out of all sub- 239 sequent CRIMs (incrementing by CRIM address before crate address) 240 until the input on the last CRIM (the CRIM with the highest address 241 in the VME crate with the highest address) is reached. This chain is re- 242 sponsible for propagating the start signal in light injection data taking. 243 A software command is sent to the Master CRIM only and propagated 244 to the others via this electrical connection. Additionally a signal is sent 245

from the Master CRIM SGATE connector to the light injection box. 246 This output is passed through the MvTM itself for shaping and delay. 247 4. The CRIM is run in one of two timing modes (see Table 3). In the 248 Internal and MvTM modes a sequencer that sends SGATE, TRIG, 249 and CNRST to the FEBs is employed. If running in “cosmic” mode for 250 the MINERνA Test Beam Experiment, TCALB is additionally sent if 251 an interrupt was raised. 252 4. Hit Timing 253 The MINERνA FEBs mount six TriP-t chips. Four are dedicated to the 254 high and medium gain and two are dedicated to the low gain. Due to this 255 division, the TriP-t chips must be grouped together when storing hits in order 256 to avoid some potential ambiguities. This has important consequences for 257 hit timing. 258 4.1. TriP-t “Push” Behavior 259 Understanding hit storage is important for understanding hit timing. The 260 TriP-t has a 48-cell deep analog pipeline and integrated charge is pushed into 261 this pipeline when the discriminator fires according to a process described be- 262 low. Each cell of charge corresponds to a “hit.” This behavior is not internal 263 to the TriP-t chip, but is controlled but the FPGA firmware. The readout 264 depth (number of total allowed hits) is limited by the internal memory of 265 the FPGA and the way digitized data from the hits is stored in the FPGA. 266 There is flexibility in the maximum number of hits that may be stored, but 267 in standard configurations prior to 2012, MINERνA stored up to eight hits. 268 Charge is integrated over a time window set by the user. The whole 269 window is referred to as a “gate.” Activity is separated in time inside this 270 gate by latching the system counter when the integrated charge goes over 271 a user-defined threshold and then storing the charge integrated up to that 272 time (this process is called “pushing the pipeline”). After storing the hit, 273 the integrators are reset and re-opened. At the end of the gate, the analog 274 information stored in the pipeline is digitized into RAM with one ADC block 275 (or “hit”) for each stored set of charges in the pipeline (for each “pipe”). 276 The different times associated with these processes are tunable by the user. 277 In MINERνA, the standard gate length is 1702 clock ticks (≈16 μs). The 278 integration time after a discriminator fires is 16 clock ticks (≈150 ns), and 279 the reset requires 20 clock ticks (≈188 ns). 280

The six TriP-t chips on each FEB are numbered 0-5, and each carries 32 281 channels. TriP-t chips 0-3 each operate 16 channels in the high gain mode 282 and 16 channels in the medium gain mode. TriP-t chips 4 & 5 each operate 283 32 channels in the low gain mode. There are 64 channels on each multi- 284 anode PMT, so TriP-t chips 0, 1, and 4 serve one half of the PMT, and 285 TriP-t chips 2, 3, and 5 serve the other. Note this means any given pixel on 286 a PMT is serviced by two separate TriP-t chips - one chip with one channel 287 operating in a low-gain mode (low amplification of signal), and one chip 288 with two channels, one in a medium-gain mode and one in a high-gain mode 289 (large amplification of signal). All three channels operate simultaneously and 290 independently of each other, each recording a value proportional to the gain 291 times the charge. In principle, every channel on a TriP-t chip supports a 292 discriminator, but only the discriminators on the high gain TriP-t channels 293 are active. This is because the high gain channels are the most sensitive 294 and low and medium-gain channels cannot be over threshold without their 295 corresponding high-gain channel also being over threshold. The channel map 296 ties two high and medium-gain TriP-t chips to each low gain TriP-t chip. In 297 order to associate data in the low gain with data in the high or medium 298 for a given channel, the low-gain TriP-t for that channel must be pushed 299 with the high gain TriP-t chip. To avoid ambiguous hit assignment for the 300 other channels serviced by the low-gain TriP-t chip that are not shared with 301 the firing high-gain chip, the “parallel” high-gain chip must also be pushed. 302 Thus, there are effectively two logical units, 32 channels in size, on each 303 board that are used to fill the analog pipelines. 304 4.2. Clock Ticks and Time 305 Time on the FEBs is set relative to a free-running counter that counts 306 up in clock ticks until it reaches the 32-bit unsigned integer maximum, at 307 which point it simply rolls over to zero. The counters are reset to the value 308 stored in the programming registers of the FPGA control chips when the 309 FEBs receive a CNRST signal. By tuning this start value to account for 310 signal propagation time, it is possible to synchronize the local counter values 311 on the FEBs to within one clock tick. 312 After a gate-open signal, the FEB loads its Timer register value and starts 313 a counter that counts up to the 16-bit unsigned integer maximum. This delay 314 is used to synchronize with beam activity and as a ”quiet” period to blank 315 charge pulses to the CW voltage system just before SGATE (at least 15 316 microseconds is required). At the counter maximum the FEB gate opens 317

and the time on the free-running counter is latched as our gate start time. 318 It is an offline software convention to subtract this time from all subsequent 319 calculations on a board. 320 Because the low gain channels are shared across two high and medium 321 gain sets of channels, when the discriminators fire charge is pushed and stored 322 in groups of 32 channels. This means a hit in a given channel creates a 323 timestamp T_0 for the whole TriP-t chip via the high gain. That timestamp 324 is further shared across the “TriP-t Chip Group” (0, 1, and 4 share the same 325 base time, and 2, 3, and 5 share a separate base time). Subsequent hits 326 within the 16-tick integration window have differing delay and quarter ticks. 327 Crossing a discriminator threshold causes all three associated TriP-t chips to 328 push 16 FEB clock ticks later, regardless of subsequent hits. 329 When a discriminator fires, it sets its whole TriP-t chip group (0+1+4 330 or 2+3+5) to push 20 system ticks later. The entire group shares the base 331 integer time stamp for the earliest channel to fire on the group, and the 332 initiating channel also stores a quarter-tick for fine resolution. The system 333 clock continues to run and provides delay and quarter ticks to timestamp 334 subsequent hits (prior to the push) to 1/4 of a tick accuracy in other channels 335 (pixels) in the group. 336 4.3. Dead Time 337 Coupling pairs of high gain TriP-t chips implies dead time impacts 32 338 channels at a time. The reset after a push requires 20 clock ticks to complete. 339 During the reset period, all three TriP-t chips that pushed are essentially dead 340 to incoming signals. Hits during the reset period are un-timed and the charge 341 recorded is either greatly attenuated or zero. For illustration, consider Fig. 342 4. When there is a hit on one half of a discriminator-active TriP-t pair at 343 time T_0 and another hit at a later time T_1, the second hit is latched in time 344 as long as it arrives before the push. If the second hit on either pair of TriP- 345 t chips arrives more than 16 ticks after the initiating hit, the later hit is not 346 recorded. Time on both TriP-t chips is relative to T_0, the first threshold cross 347 between the two. Fig. 5 shows a typical bank structure for a gate and Fig. 348 6 shows the memory structure of a discriminator bank. 349 There is another form of dead time due to hit saturation. This occurs 350 when the number of “pushes” allowed by the pipeline depth are exhausted. 351 In this case, charge continues to integrate, but additional hits are no longer 352 time-stamped. 353

Figure 4: A specific dead-time illustration on one FEB. Consider a hit on TriP-t 0. This hit will set a timestamp, T_0 here, and cause a pipeline push 16 clock ticks later for TriPt chips 0, 1, and 4. A later hit at time T_1 above does not initiate a new pipeline push and the time is stamped relative to T_0. The ADCs are effectively dead between T_0 + 16 and T_0 + 36 clock ticks. After that point, the ADCs on those TRiPs are fully live again and new hits over threshold will be timestamped.

Figure 5: A generic example of the organization of data within the discriminator and ADC banks. The columns (“Hit X”) denote hit RAM Functions - all of the data in the column is read at once and partial pipeline reads cannot be performed. In this case, there was a hit on either TriP-t 0 or 1, another independent hit on either TriP-t 2 or 3, and a final hit on TriP-t 0 or 1. The ADCs cannot distinguish which TriP-t in the two pairs contained the initial hit for that pair. Again, this diagram does not distinguish which TriP-t had the channel hit first, and it cannot distinguish which of the hits in the “Hit 1” RAM Function was earlier - the discriminator bank must be decoded for that information. The end of integration “hit” is not included in the set of ADC banks shown here. It would appear in a new column titled “Hit 2” and would appear in all TriP-t ’s. For each FEB read out, the following RAM Functions: ReadDiscr, ReadHit0, ..., ReadHit7 are looped through.

Figure 6: A visualization of the discriminator bank for a single TriP-t chip. The system tick is stored in the 32 bits at the “bottom” of the figure. Quarter ticks for each channel are stored in the 32 bits above that at 2 bits per channel. Finally, the delay ticks are stored in 16 bits for each channel above the quarter ticks.

4.4. FEB Timing Synchronization 354 When the CRIM sends an open-gate command (SGATE) through the 355 CROCs to the FEBs, the actual signal arrives at different times to the dif- 356 ferent FEBs on the chain due to cable delays. This is accounted for in two 357 steps: 358 1. The FEB loads the value recorded in the Timer register of the FPGA. 359 By staggering the time loaded to account for the finite signal propaga- 360 tion time down the chain, all of the boards can synchronize the values 361 on their local counters. 362 2. Once the FEBs receive an open-gate signal they begin counting up 363 to a pre-set open-gate time value, beginning not with zero, but with 364 the Timer value mentioned in the previous step. This additional delay 365 is meant to provide the PMT with time to settle into a stable high 366 voltage in the case the Cockroft-Walton adjusted the voltage period 367 just before the gate is opened. Once they reach this time, they open 368 their integration gates. All the FEBs will physically open their gates 369 at the same local time. 370

5. DAQ Software 371 5.1. Readout Control 372 The DAQ is a system built out of three computers running 64-bit Scientific 373 Linux Fermi^{15} - one readout node for each VME crate and one master node. 374 Data transfer between the readout nodes and master node is handled via the 375 Event Transfer (ET) software package (part of CODA^{16}), discussed further 376 below. The head node initiates a run and creates a memory-mapped file to 377 store data. It provides instructions to the readout nodes on when to begin 378 the readout sequence. When readout begins, each of the slave nodes passes 379 data frame-by-frame to the master for collation. At the end of a run, the head 380 node converts the memory-mapped file into a flat binary and releases it. One 381 feature of this approach is that if the DAQ fails during readout, the collected 382 data are already stored on disk and are not lost. The DAQ is written in C++ 383 to run on Scientific Linux Fermi^{15}, but should run with minimal modifications 384 on most major Linux distributions. The code is divided into four libraries: 385 1. Hardware access: Our hardware access libraries are built on top of a 386 set of proprietary (closed-source) libraries provided by CAEN to access 387 the V2718 VME crate controller^9 using the A2818 PCI optical bridge 388 card^{11}. Functions from the libraries CAEN makes freely available for 389 this hardware on its website are used to format command and control 390 messages to the CROCs and CRIMs as required during readout. 391 2. Event structure: Another set of libraries that define the types and 392 structures of the MINERνA data types. 393 3. Acquisition control: These libraries and executables run the acquisition 394 and interface with the Run Control software described in Section 5.2. 395 4. Buffer management and interprocess communication (IPC): Like the 396 hardware access libraries, the buffer management and IPC code uses 397 external libraries. In particular, the open-source Event Transfer (ET) 398 system version 9.0, based on CODA,^{16} developed at the Thomas Jef- 399 ferson Lab National Accelerator Facility (JLab)^{17} is used. 400 5.2. Run Control 401 The run control is written in Python for flexibility and platform-independence. 402 There are two external Python libraries (in addition to the DAQ software, 403 described in section 5.1) needed for various components of the run control to 404 work: 405

1. wxPython^{18}, chosen as our graphics toolkit because of its ease of use 406 and maturity; 407 2. pySerial^{19}, which provides a convenient RS-232 interface. 408 6. Computing Architecture 409 6.1. Overview of Data Handling 410 MINERνA uses two networks of server-class computers: one for physics 411 data collection and one for data quality monitoring and run control. The 412 data collection PCs are detailed in Section 7. For monitoring, MINERνA 413 uses two remote clusters of computers at Fermilab: one in the Feynman 414 Computing Center (FCC), and the other at Wilson Hall (WH). These systems 415 are discussed in Sections 8 and 9 416 Data are collected and logged underground independently of above-ground 417 computing clusters. The DAQ can run without input from or a connection 418 to any above-ground network with local storage for physics data, metadata, 419 and logs sufficient for about a month of normal operations. The above- 420 ground computers manage long-term data archival, log file metadata into 421 SAM (Sequential Access Method - a metadata database application)^{20}, pro- 422 duce histograms for monitoring, and provide run control options. 423 6.2. Data acquisition coordination 424 The run control software manages connections between most of the com- 425 puters used in the data acquisition and monitoring process such that they 426 remain synchronized throughout. Kerberos-authenticated^{21} SSH tunnels are 427 used to connect clients (i.e., user shift consoles) to a master DAQ server pro- 428 cess and the master DAQ server to the other slave machines, as described 429 below. 430 The heart of the run control is a central server process on the master 431 DAQ node. It maintains communication with “dispatcher” processes running 432 on each of the relevant slave remote nodes so as to instruct them to start 433 or stop their various tasks as the state of data acquisition changes. It is 434 also the entry point for communication from the graphical end client used 435 by operators to interact with the DAQ. This “DAQ manager” process can 436 coordinate data taking irrespective of the number of clients connected; once 437 started, it will run through to completion of the data acquisition sequence 438 even if the controlling client is disconnected. 439

The DAQ manager connects to a collection of remote nodes in various 440 locations. Among these are readout nodes that insert the digitized data 441 into the data stream and the monitoring nodes that run slow monitoring 442 processing jobs and serve the data to the operator. 443 Operators control the DAQ using a graphical client (also contained in the 444 run control package) that connects to the DAQ manager over the network 445 using a custom thin-client TCP protocol. This design accommodates both 446 the Fermilab control room and collaborator institutions located around the 447 world. 448 7. Physical Organization of the Readout Equipment in NuMI 449 All relevant MINERνA electronics equipment is mounted in racks sitting 450 on a deck beside the detector. All racks are equipped with smoke detection 451 and interlocked power, with rack protection and slow monitoring built into 452 the overall online scheme. 453 Racks are labeled according to their primary hardware electronics com- 454 ponents and there are four primary racks: 455 1. The VME Rack (also sometimes called the DAQ Rack) 456 2. The Light Injection (LI) Rack 457 3. The Veto Rack 458 4. The Spares Rack 459 Our racks all consume less than 2500W each, meeting the FNAL require- 460 ments for air cooling. See Fig. 7 for an overview of the arrangement of and 461 connections between the three racks. 462 7.1. The VME Rack 463 The VME Rack contains the two VME crates that hold the MINERνA 464 readout electronics. It additionally mounts a pair of PCs and network sup- 465 port components. Access control for devices that cannot be configured to use 466 Kerberos is provided by a very restrictive ACL (Access Control List). See 467 Fig. 8 for the rack layout and connection types. Insofar as the readout ar- 468 chitecture is concerned, it contains (roughly in mechanical installation order 469 from top to bottom): 470 1. A custom Temperature and Environment Monitor (TEM) device (la- 471 beled the “Slow Monitor”) that supports eight temperature probes that 472

Figure 7: Connection map for the MINERνA readout system, ignoring AC distribution, FESB power, and safety systems. Network connections are also suppressed - every device with an internet name is linked to the network switch housed in the VME rack.

may be deployed throughout the racks and over the detector surface. 473 The device also logs humidity, pressure, and temperature at the end of 474 six cabled sensors deployed on the detector. 475 2. Two CAEN VME 8011 crates^{22}. The crates are indexed as 0 and 1. 476 Crate 0 contains a controller module, two CRIM modules, and eight 477 CROC modules. Crate 1 contains a controller module, two CRIM 478 modules, seven CROC modules, and a MvTM module. See Figs. 9 479 and 10 for the VME module assignment in Crates 0 and 1 respectively. 480 3. An APC 120VAC Masterswitch III Switched Rack PDU (Power Distri- 481 bution Unit), Model # AP7900. This PDU is a networked device that 482 provides remote power control for the VME crates and all PCs in the 483 rack. 484 4. A 48 port Cisco C2960G switch, designated S-S-MINERVA-1.^{23} 485 5. Three 48VDC power supplies to power the FEB’s (not pictured in the 486 figures). 487 6. Three networked fuse panels for the 48VDC power supplies, networked 488 to S-S-MINERVA-1. These fuse panels host a web interface with self- 489 documented power control of the FESBs mounted on the MINERνA 490 detector (not pictured in the figures). 491 7. A 1U Linux PC serving as a back-up for the master DAQ node in the 492 Veto Rack (see Section 7.3). 493 8. A 1U Windows PC running control and monitoring software for the 494 LeCroy High Voltage Power System (HVPS) located in the Veto Rack. 495 Not currently installed. Space, power, and networking resources are 496 reserved. 497 9. An APC Smart-UPS 2200VA (2000W Un-interruptible Power Supply) 498 supporting the switch and PCs. The primary function of this UPS is 499 power filtering. In the event of a full power failure, the system will 500 remain live for more than thirty minutes. 501 7.2. The LI Rack 502 The LI rack contains the MINERνA custom-built Light Injection (LI) 503 boxes^{24}. The rack is intentionally kept sparse to provide sufficient space to 504 route and store the optical fibers that connect from the back of the LI boxes 505 to the PMTs mounted on top of MINERνA. See Fig. 11 for the rack layout 506 and connection types. For our purposes, it contains (roughly in mechanical 507 installation order from top to bottom): 508

Figure 8: Connection map for the VME Rack. Power architecture is not shown, including the three networked fuse panels.

Figure 9: The connection and layout diagram for VME Crate 0.

Figure 10: The connection and layout diagram for VME Crate 1. The V1720 CAEN Waveform Digitizer is not currently installed.

1. A BiRa Rack Protection System (RPS). The RPS deploys a variety 509 of monitoring cables into the VME Rack: voltage-monitoring cables 510 to the VME crates, and airflow and temperature sensors. The RPS is 511 connected to the S-S-MINERVA-1 switch located in the VME rack by 512 ethernet. 513 2. A PIN diode box. The PIN is optically connected to the LI box to 514 monitor the stability of the LED light output. The PIN box is addi- 515 tionally connected via BNC and specialized cables to a CAEN V1720 516 waveform digitizer^{25} mounted in VME Crate 0 in the VME Rack. 517 3. The primary LI box. This box contains control electronics and LEDs 518 that service optical connectors on the back of the box. From those 519 connectors light is piped via optical fiber to the PMT boxes mounted 520 on top of the detector. It is interfaced via a 9-pin serial RS-232 socket 521 on the front of the box. This serial cable is connected to the MINERνA 522 DAQ PC cluster for configuration commands. It additionally accepts 523 a LEMO connection for the external trigger signal. 524 4. A secondary (smaller) LI box to service the most forward detector 525 modules. It uses the same electronics and connections as the larger 526 box, but mounts fewer LEDs. 527 7.3. The Veto Rack 528 The Veto rack derives its name from the LeCroy High Voltage Power 529 System mounted there that controls the high voltage on the resistor-base 530 PMTs deployed to readout the ”Veto Wall” sitting in front of the MINERνA 531 detector. It also contains the main readout PCs for the DAQ system. See 532 Fig. 12 for the rack layout and connection types. For our purposes, its 533 important contents are: 534 1. Two MINERνA FEBs attached to a special custom breakout board 535 in a 2U chassis. The FEBs are standard MINERνA boards, but the 536 breakout board is required to interface the single-anode PMTs (resistive 537 base) used to monitor the scintillator panels in the veto wall. 538 2. A LeCroy Model HV4032A High Voltage Power System (HVPS). The 539 HVPS connects to the readout PC located in the VME Rack via a 540 special custom serial cable. It also connects to the Veto Wall PMTs. 541 3. A 1U Linux PC running the DAQ Master software. This PC is identical 542 to the logger PC in the VME Rack. The DAQ Master node connects 543 to the Slave Readout nodes via direct ethernet. 544

Figure 11: Connection map for the LI Rack.

4. Two 3U Linux PCs serving as DAQ Readout Slave nodes. Each PC 545 mounts a CAEN a2818 PCI Optical Bridge card^{11} and interfaces with 546 one of the VME crates located in the VME Rack. 547 5. An APC 120VAC Masterswitch III Switched Rack PDU (Power Distri- 548 bution Unit), Model # AP7900. This PDU is a networked device that 549 provides remote power control for the VME crates and all PCs in the 550 rack. 551 6. An APC Smart-UPS 2200VA (2000W Un-interruptible Power Supply) 552 supporting the PCs. The primary function of this UPS is power filter- 553 ing. In the event of a full power failure, the system will remain live for 554 over thirty minutes. 555

Figure 12: Connection map for the Veto Rack.

7.4. The Spares Rack 556 The final rack in the MINERνA electronics installation sits across the hall 557 from the detector on the West side of the enclosure. It contains a number of 558 spare components: 559 1. A 3U Linux PC configured to serve as a spare readout node. 560 2. A 48 port Cisco C2960G switch, designated S-S-MINERVA-2.^{23} 561 3. A 1U Linux PC running logging software for the slow monitoring de- 562 vices. This machine also serves as the head node for a pool of servers 563 running a Condor^{26} queue for batch processing jobs used to support 564 monitoring activities in the control room. 565 4. Spare AC distribution and smoke protection units. 566 7.5. Power Infrastructure 567 7.5.1. DC Power Distribution 568 The large number of Front End boards and their location atop the de- 569 tector makes conventional low-voltage power distribution impractical. A dis- 570 tributed power architecture is employed where 48 VDC power equipment 571 is located in the electronics racks and intermediate low voltage regulation is 572 performed on the detector near the FEBs. Finally, low-noise linear regulators 573 on each FEB produce the final 3.3 V power required. 574 Each FEB readout chain (up to ten FEBs) is powered by a Front End 575 Support Board (FESB) which contains an isolated DC-DC converter to step 576 down 48 VDC to approximately 4 VDC at 20 A. FESBs are passively cooled 577 and use the FEB/PMT steel mounting bracket as a heat sink. 578 Three 48 VDC power supplies operate in parallel and support “hot swap” 579 and dynamic load sharing. Two supplies are required to meet the design 580 specification of 3000W. The extra power supply allows for “N+1” redundant 581 operation, which makes it simple to remove and replace a supply without 582 interruption. Each power supply is rated for 1900 W and provides an interface 583 by which the health of the supply may be monitored remotely (through the 584 Rack Protection System (RPS) interface board and Environmental Monitor). 585 Through the Fuse Chassis the main 48 VDC 120 A bus is fanned out into 586 six 20 A connections. Two of these 20 A connections feed a Network Fuse 587 Panel (NFP), which fans out into twenty 2 A busses going to the FESBs. 588 Each NFP offers independent control and monitoring of the FESBs through 589 a web interface. 590

The actual power supply consumption is 1500 W when the FEBs are 591 idle. The redundant “N+1” power supply configuration has been robust and 592 reliable and has operated continuously without problems since commissioning 593 in 2008. See Fig. 13 for a schematic. 594

Figure 13: Power distribution for MINERνA.

7.5.2. Rack Protection System and AC Power Distribution 595 Rack protection is provided by the BiRa Systems RPS unit model 8884^{27}, 596 which monitors a smoke detector in each of the three racks on the platform. 597 If smoke is detected, the RPS unit drops the interlock signal, disabling the 598 AC distribution chassis. The RPS also generates an emergency power output 599 (EPO) signal that immediately disconnects the internal batteries on the UPS. 600 The Environmental Monitor reads various temperature sensors located 601 around the detector. In addition, this monitor records and logs humidity and 602 ambient light conditions. It is accessed through a web and FTP interface on 603 the DAQ network. 604 8. Interface to the MINERνA Control Room 605 8.1. The MINERνA Control Room 606 The MINERνA control room is located in Wilson Hall at FNAL, in the 607 north-west corner room on the 12th floor (WH12). See Fig. 14 for a map 608 of building locations at Fermilab. MINERνA services our control room with 609

a total of eight PCs, with four in the Control Room and four in the Feyn- 610 man Computing Center (FCC) at FNAL. The PCs kept in FCC run more 611 processor-intensive tasks using a private Condor batch queue system^{26}. 612

Figure 14: Buildings and sites at Fermilab.

8.2. Controlling the DAQ System 613 As noted above in section 6.2, the DAQ system is controlled via a graphi- 614 cal thin client delivered with the run control software. The client runs locally 615 on the operator’s terminal. Control of the DAQ is via a custom TCP thin- 616 client protocol that is transmitted over a Kerberos-enabled SSH tunnel to 617 the master DAQ node. Inbound connections are filtered both via the firewall 618 provided by the NuMI router and by an access list of Kerberos principals 619 allowed to log into the machine. 620 Commands sent via a successful tunnel to the DAQ manager process 621 (running on the DAQ master node) are interpreted based on a notion of client 622 “control” of the DAQ. At most one (though possibly zero) client(s) can be in 623 control of the DAQ at any given time; only commands that originate from a 624 node which is currently “in control” are ultimately acted upon. An unlimited 625

3 number of clients are allowed to connect as observers. Any observer is 626 allowed to request control at any time; however, if another client is in control 627 at the time the request is made, the client in control is given a configurable 628 length of time to veto the request or approve transfer of control. In addition, 629 the run control package contains a client manager program that can revoke or 630 assign control to or from any client that is currently connected after proper 631 credentials are submitted, currently a password. 632 Once connected and in control, the operator is presented with a graphi- 633 cal interface containing details about the current data acquisition sequence 634 and status as well as controls allowing him/her to start, manually advance, 635 or stop data acquisition. When the DAQ is stopped the operator can also 636 adjust a handful of simple configuration options pertaining to the data ac- 637 quisition sequence he/she would like to begin. The bulk of the configuration 638 operations, however, is accessible only to experts directly on the DAQ head 639 node so as to avoid accidental misconfiguration. 640 Once initiated, data acquisition requires no intervention from the oper- 641 ator. The run control system can even operate unsupervised by any clients 642 at all (as would happen, for example, in the case where the network connec- 643 tion to a remote site is interrupted). Under these circumstances warnings 644 about the system state are queued and delivered in bulk to every client who 645 reconnects until they are acknowledged. 646 9. Data Handling Paths 647 The MINERνA electronics are capable of monitoring a wide variety of 648 configuration states: high voltage on the (Cockcroft-Walton) PMTs deployed 649 on the detector, whether individual boards are dead or live, and the temper- 650 ature of the FEBs. A separate system monitors the resistive base PMTs used 651 for the MINERνA Veto Wall. For cost-saving reasons MINERνA uses the 652 same communications chain for electronics configuration and slow controls 653 as it does for data handling. As a consequence, these monitoring data are 654 packaged with the physics data directly and exist as part of that stream. 655 For monitoring purposes, the MINERνA near-online, or “Nearline,” clus- 656 ter runs an ET client that is notified about the beginning and end of runs. 657

3Unlimited at least in principle. Network bandwidth and CPU time saturation, of course, will create an operational ceiling, though the actual maximum will depend on the environmental conditions.

During a run, it reads data from the DAQ head node frame-by-frame. When 658 it completes an event (signified by reading the DAQ event header frame) 659 it converts the binary data into MINERνA “RawDigits” (the most basic 660 analysis data format) for monitoring. Other tasks running on the Nearline 661 cluster decode the RawDigits and process them through the MINERνA soft- 662 ware framework - producing monitoring quantities ranging from high voltage 663 status to event displays. These are published to control room PCs for exper- 664 imenters to study. 665

Figure 15: Flow-chart diagram for physics data through the MINERνA acquisition chain. Not shown are the archival data handling beyond the near-online cluster or the metadata handling.

After each run a copy of the raw binary data file is pushed to the disk 666 and tape for permanent storage. See Fig. 15 for a flowchart of the scheme. 667 A long-term rolling copy of recent raw data is kept on the DAQ system itself 668 (extending back approximately two months). With the raw data the DAQ 669 additionally pushes metadata about the run for entry into SAM. Finally, a 670 “keep-up” processing that uses raw data copied directly from the DAQ (not 671 from the Nearline system) is also run to produce the RawDigits of record. In 672 the end, there are three copies of the “raw” data at the end of this process: 673 a copy of the raw data on the DAQ storage disks, a copy of the raw data in 674

permanent storage, and a copy of the RawDigits (raw data reformatted for 675 MINERνA software consumption) for general use. 676 10. Summary and Performance 677

Figure 16: Protons on target delivered and recorded for MINERνA.

MINERνA began its official physics run on March 23, 2011 with the DAQ 678 system described above. Since that time, live-time for the whole period was 679 96.4% (not counting beam down-times). See Fig. 16 for a summary of the 680 protons on target delivered and recorded for MINERνA. During normal op- 681 erations the live-time is over 99% and inefficiencies are almost entirely due 682 to change-over between runs. Our integrate live-time is most impacted by 683 electronics failures and simple operator error or inattention. There are ideas 684 for removing losses due to run change-overs (pre-starting the subsequent run 685 and putting it into a wait state to speed up the change) and our run control 686 system is constantly being improved to minimize the opportunity for exper- 687

imenters to make mistakes when running the system while still providing 688 flexible operational control. 689 References 690 1. The MINERvA Conceptual Design Report. MINERvA Doc-DB 482; 691 2006. 692 2. The MINOS Experiment. http://www-numi.fnal.gov/Minos/; 2011. 693 3. The NuMI Beamline. http://www- 694 numi.fnal.gov/numwork/numiwk.html; 2011. 695 4. The MINERvA Technical Design Report. MINERvA Doc-DB 700; 2006. 696 5. Hamamatsu M64 PMT. http://sales.hamamatsu.com/en/products/electron- 697 tube-division/detectors/photomultiplier-tubes/part-r7600-00-m64.php; 698 2011. 699 6. C.Gingu , P.Rubinov . Minerva Master/Slave Data Acquisition Board 700 Description and Measurement Result. 2005. 701 7. Rubinov P. AFEII Analog Front End Board Design Specifications. 2005. 702 8. Baldin B. VME Data Acquisition Modules for MINERvA Experiment. 703 FERMILAB-TM-2458-PPD; 2010. 704 9. The CAEN v2718 VME Crate Controller. 705 http://www.caen.it/nuclear/product.php?mod=V2718; 2008. 706 10. T.Fitzpatrick , C.Rotolo . MINOS Master Clock System Preliminary 707 Design Specification. NUMI-NOTR-ELEC-827, Fermilab; 2000. 708 11. The CAEN a2818 PCI Optical Bridge. 709 http://www.caen.it/nuclear/product.php?mod=A2818; 2008. 710 12. http://www-d0.fnal.gov/; 2011. 711 13. Baldin B. MINERvA Chain Readout Controller. MINERvA Doc-DB 712 1516; 2007. 713 14. Baldin B. MINERvA CROC Interface Module. MINERvA Doc-DB 714 1238; 2009. 715

15. Fermi Linux. http://fermilinux.fnal.gov/; 2011. 716 16. CODA. https://coda.jlab.org/wiki/index.php/Main Page; 2011. 717 17. http://www.jlab.org; 2011. 718 18. http://wxpython.org; 2011. 719 19. http://pyserial.sourceforge.net/; 2011. 720 20. http://d0dbweb.fnal.gov/sam pyapi; 2011. 721 21. http://web.mit.edu/kerberos/; 2011. 722 22. The CAEN 8011 VME Crate. http://www.caen.it/nuclear/syproduct.php?mod=VME8011; 723 2008. 724 23. Cisco Systems. http://www.cisco.com/en/US/products/ps6406/index.html; 725 2011. 726 24. Dytman S. LI Summary. MINERvA Doc-DB 4033; 2009. 727 25. The CAEN v1720 Waveform Digitizer. 728 http://www.caen.it/nuclear/product.php?mod=V1720; 2008. 729 26. http://www.cs.wisc.edu/condor/; 2011. 730 27. http://www.bira.com/; 2011. 731