arXiv:2307.06634v1 [eess.SP] 13 Jul 2023

Coherent Compensation based ISAC Signal Processing for Long-range Sensing

(Invited Paper)

Lin Wang^*, Zhiqing Wei^*, Liyan Su^†, Zhiyong Feng^*, Huici Wu^‡ and Dongsheng Xue^*

* Key Laboratory of Universal Wireless Communications, Ministry of Education Beijing University of Posts and Telecommunications, Beijing 100876, China †Huawei Technologies Co., Ltd, Beijing 100085, China ‡National Engineering Lab for Mobile Network Technologies Beijing University of Posts and Telecommunications, Beijing 100876, China Email:{wlwl, weizhiqing, fengzy, dailywu, xuedongsheng}@bupt.edu.cn, suliyan1@huawei.com

Abstract—Integrated sensing and communication (ISAC) will greatly enhance the efficiency of physical resource utilization. The design of ISAC signal based on the orthogonal frequency division multiplex (OFDM) signal is the mainstream. However, when detecting the long-range target, the delay of echo signal exceeds CP duration, which will result in inter-symbol interference (ISI) and inter-carrier interference (ICI), limiting the sensing range. Facing the above problem, we propose to increase useful signal power through coherent compensation and improve the signal to interference plus noise power ratio (SINR) of each OFDM block. Compared with the traditional 2D-FFT algorithm, the improvement of SINR of range-doppler map (RDM) is verified by simulation, which will expand the sensing range.

Index Terms—Integrated sensing and communication, OFDM, echo delay exceeds cyclic prefix duration, coherent compensation, long-range sensing

I. INTRODUCTION

6G wireless communication applications (autonomous driving, smart factory, etc) not only require communication but also require sensing the surrounding environment. It is necessary to integrate communication and sensing in the same system, which is called the integrated sensing and communication (ISAC). The ISAC will greatly improve the efficiency of physical resource utilization [1]–[3].

The ISAC technical routes include communication-centric design, radar-centric design and joint design. In which, the communication-centric ISAC refers to integrate sensing into communication system without influencing communication performances. The orthogonal frequency division multiplex (OFDM) widely used in the mobile communication system is the mainstream in ISAC signal design [4]. While transmitting communication information, the range and velocity of the target can be estimated [5]–[7]. However, the sensing range of the OFDM signal is limited by the cyclic prefix (CP). For long-range target, there will be inter-symbol interference (ISI) and inter-carrier interference (ICI) in the echo signal [8]. According to the CP duration defined in 3GPP TS 38.211, the maximum sensing range without ISI and ICI is only 88.5 meters, which greatly restricts the application of ISAC.

Therefore, it is urgent to design an interference suppression method to expand the sensing range.

Facing the above-mentioned challenges, Tigrek et al. [8] removed the CP and transmitted the adjacent elementary OFDM symbols continuously to reduce the Doppler ambiguity of long-range targets. Due to the absence of CP, OFDM signal is susceptible to multipath, which affects the communication. Hakobyan et al. [9], [10] proposed repeated symbols OFDM (RS-OFDM), which only retains the CP of the first OFDM symbol and transmits the identical symbol consecutively. This scheme causes no ISI and ICI in the echo signal, and the maximum unambiguous speed is increased. But the repeated symbols limit the data rate. Tang et al. [11] studied IEEE 802.11ad based sensing. When the delay of echo signal exceeds one OFDM symbol duration, the coherent superposition of adjacent symbols is used to accumulate energy. Then a small amount of interference-free OFDM symbols at the end of frame can be used for sensing. But it is necessary to insert additional pilots to assist sensing. Wu et al. [12] proposed to re-segment the echo signal and transmitted signal into elementary sub-blocks in the time domain and adjacent subblocks can overlap. For echo signal, some samples called virtual cyclic prefix (VCP) after each sub-block are added onto the front of this sub-block to form a cyclic shift signal. The channel information matrix can be obtained by a pointwise division between fast fourier transformation (FFT) of resegmented sub-block of echo signal and the transmitted signal. This scheme can flexibly re-segment the sub-blocks according to the sensing requirement. But these two schemes are not fully applicable to ISAC base station (BS): 1) echo delay exceeding one OFDM duration is not considered in ISAC BS; 2) the re-segmented sub-blocks will devastate the original OFDM symbol structure and increase the number of FFT.

In this paper, ISAC BS is considered, which utilizes the 3GPP TS 38.211 based OFDM waveform. For the case where the echo delay exceeds CP duration but does not exceed one OFDM symbol duration, the ISI and ICI are modeled. Then, some samples after each elementary OFDM interval are added to the front through coherent compensation to increase power of the useful signal and improve the signal to interference plus noise power ratio (SINR) of each OFDM block. Since the data is processed within elementary OFDM symbol interval, the OFDM structure is kept and the number of FFT will not be increased. The simulation results verify that the proposed coherent compensation scheme can improve the SINR of the range-doppler map (RDM) compared with the traditional 2D- FFT algorithm and VCP algorithm.

The rest of this paper is organized as follows. Section II introduces the OFDM signal model based on 3GPP TS 38.211 and models the ISI and ICI when the echo delay exceeds CP duration. Section III presents the proposed coherent compensation algorithm and derives the optimal compensation length. Section IV verifies the improvement of the proposed algorithm to the sensing performance through simulation. Section V concludes this paper.

II. SIGNAL MODEL

Fig. 1: OFDM echo signal and coherent compensation for target with echo delay exceeding CP duration. The samples (red part) after each elementary OFDM interval can be added to the front to improve the SINR.

The baseband signal of M OFDM symbols (including CP) in the transmitter is

x (t) = 1 √ N_c M−1∑ m=0

N_c−1∑

k=0 S_m (k) e^{j2πkΔf (t−mT )}u (t − mT ), (1) where N_c represents the number of subcarriers. S_m (k) represents the normalized modulation symbol (e.g. QAM, PSK) transmitted on the kth subcarrier of the mth OFDM symbol. Δf is the subcarrier spacing. B = N_cΔf is the bandwidth. T =T_{CP} +T_D is the duration of the entire OFDM symbol. T_{CP} and T_D are the duration of CP and elementary OFDM symbol, respectively. u (t) is the pulse shaping function, generally using a rectangular function as follows.

u (t) = { 1 −T_{CP} ≤ t < T_D 0 else . (2) Then the received echo baseband signal is y (t) =α̃x (t − τ ) e^{j2πfdt}+w (t) . (3) where τ and f_d represent the time delay and Doppler shift caused by target. α̃ = αe^{−j2πfc τ} , where α represents the radar cross-section (RCS) of target, path loss and gain of antennas. w (t) represents additive noise, which follows a stationary Gaussian random process. Since x (t) is normalized, we can define the received SINR as γ_0 =^{|α̃|2}_{σ2} , where |∗| represents the modulus operator and σ^2 is the power of noise.

We consider that the radar receiver and transmitter are colocated and synchronized. For the case where the echo delay exceeds CP duration but is less than one OFDM symbol duration, i.e. T_{CP} < τ < T , the ith sampling point with sampling interval T_s = 1/B in the nth elementary OFDM symbol interval is (4), where w_n (i) = w (nT + iT_s), i = 0, 1, · · · , N_c − 1. From (2), it can be seen that −T_{CP} ≤ nT + iT_s − mT − τ < T_D needs to be satisfied. Then we have n +^{iTs −τ −TD}_T < m ≤ n +^{iTs −τ +TCP}_T . Since T_{CP} < τ < T , we can get m = n − 1, n. So there will be ISI in nth elementary OFDM interval, as shown in Fig. 1. Doppler frequency shift will compromise the orthogonality between subcarriers. However, when the subcarrier spacing is considerably larger than Doppler frequency shift (usually satisfying Δf > 10f_d), the Doppler frequency shift on different subcarriers is considered to be equivalent, which ensures the orthogonality between subcarriers [10]. Therefore, (4) can be transformed into (5).

y_n(i) = 1 √ N_c N_c−1∑

k=0 α̃S_{n−1} (k) e^{j2πkΔf (T +iTs−τ )}e^{j2πfdnT} • u (T + iT_s − τ) + 1 √ N_c N_c−1∑

k=0 α̃S_n (k) e^{j2πkΔf (iTs −τ)}e^{j2πfd nT} u (iT_s − τ ) + w_n (i) . (5)

Let N_s = ⌊τ/T_s⌉ denote the sample offset corresponding to the delay of echo signal, where ⌊∗⌉ denotes rounding to the nearest integer. N_{cp} = ⌊T_{CP} /T_s⌉ is the sample length of CP. It can be known from (2) that when i = 0, 1, · · · , N_s − N_{cp} − 1, u (T + iT_s − τ) is non-zero, and when i = N_s − N_{cp}, · · · , N_c − 1, u (iT_s − τ ) is non-zero. Performing FFT on (5), the frequency domain symbol on the pth subcarrier in the nth elementary OFDM symbol interval can be obtained as (6), where W_n (p) is the FFT of w_n (i). It can be seen from (6) that the average power of the useful signal, ISI and ICI are

P_u = (1 − N_s − N_{cp} N_c )^2|α̃|^2, (7)

P_{ISI} = |α̃|^2 N_c (N_s − N_{cp}) , (8)

P_{ICI} = |α̃|^2 N^2_c

(N_c − N_s + N_{cp}) (N_s − N_{cp}) . (9)

The SINR of the received frequency domain signal is

Υ_f = (1 −^{Ns−Ncp}_{Nc} )^2 2^{Ns−Ncp}_{Nc} − (^{Ns−Ncp}_{Nc} )^2 +^1_{γ0} . (10)

Therefore, as the echo delay (or N_s) increases, the frequency domain SINR decreases when the γ_0 is fixed.

y_n (i) = y (nT + iT_s) = 1 √ N_c M−1∑ m=0

N_c−1∑

k=0 α̃S_m (k) e^{j2πkΔf (nT +iTs −mT −τ)}e^{j2πfd (nT +iTs )}u (nT + iT_s − mT − τ )+w_n (i) . (4)

Y_n (p) = (1 − N_s − N_{cp} N_c )α̃S_n (p) e^{−j2πpτN}c^Ts e^{j2πfd nT} + 1 N_c N_c−1∑

k=0 [α̃S_{n−1} (k) e^{j2πk(TCP −τ )} NcTs ( N_s−N_{cp}−1 ∑ i=0 e^{j2π(k−p)iN}c )]e^{j2πfd nT}

+ 1 N_c N_c−1∑

k=0,k≠p [α̃S_n (k) e^{−j2πkτNcTs} ( N_c−1∑

i=N_s−N_{cp} e^{j2π(k−p)iNc} )]e^{j2πfd nT} + W_n (p) . (6)

III. COHERENT COMPENSATION BASED ISAC SIGNAL PROCESSING

When the echo delay exceeds CP duration, the SINR of the received frequency domain symbol decreases due to the existence of ISI and ICI. In which, the power of useful signal attenuates with the increase of the delay, while the ISI sees the same tendency along with delay. When the delay is τ = T_D/2 + T_{CP} , orthogonality between subcarriers is most severely damaged, which leads to the most serious ICI. The orthogonality between subcarriers is destroyed due to not receiving a complete OFDM symbol. In order to improve the SINR, the N^′ samples after the elementary OFDM symbol interval can be added to the front of this interval, as shown in Fig. 1. The lth sample after nth elementary OFDM symbol is (11), where l = 0, 1, · · · , N^′ − 1.

It can be seen from (11) that when N^′ ≤ N_s, the samples come from the nth OFDM symbol. Therefore, the sample compensation can realize the coherent combination of the energy and increase the SINR. When N^′ > N_s, the interference from the (n + 1)th OFDM symbol will be introduced. The ith sample in the nth elementary OFDM symbol interval after coherent compensation when N^′ ≤ N_s is (12). The noise of different samples is i.i.d, so the sample compensation is an incoherent combination for noise. The noise distribution after compensation is

w̃_n (i) ∼ { N(0, 2σ^2) 0 ≤ i ≤ N^′ − 1 N(0, σ^2) N^′ ≤ i ≤ N_c − 1 (13)

Performing FFT on (12), the frequency domain symbol after coherent compensation on the pth subcarrier in the nth elementary OFDM symbol interval is (14), where W̃_n (p) is the FFT of w̃_n (i). From (14), we can get the average power of the useful signal, ISI, ICI, and noise after coherent compensation as follows.

P_u = (1 − N_s − N_{cp} N_c + N^′ N_c )^2|α̃|^2, (15)

P_{ISI} = |α̃|^2 N_c (N_s − N_{cp}) , (16)

P_{ICI} = |α̃|^2 N^2_c |N_s − N_{cp} − N^′| (N_c − |N_s − N_{cp} − N^′|) , (17)

P_w =

N_c + N^′ N_c σ^2. (18)

Then the SINR of the received frequency domain symbol after coherent compensation is (19).

Comparing (8) and (16), it can be seen that when N^′ ≤ N_s, coherent compensation does not affect the power of ISI. This is because the ISI comes from previous OFDM symbol, which is not affected during coherent compensation. It can be seen from (17) that the ICI disappears when N^′=N_s−N_{cp}. Because a complete OFDM symbol is formed. When N^′ continues to increase, the extra samples cannot maintain orthogonality in the FFT interval, causing ICI to appear again. But the extra samples can still increase the power of useful signal through coherent compensation, which can be seen from (15). When N^′ > N_s, since the adjacent OFDM symbols are independent, the compensated samples of the next OFDM symbol will not increase the power of useful signal, but will increase the power of ISI. Therefore, the SINR will be lower compared with the case when N^′ = N_s. Next, we try to analyze the optimal sample compensation length.

Let N_e =^{Ns−Ncp}_{Nc} , N_a =^{N ′}_{Nc} , then (19) can be expressed as Υ_f =

(1 − N_e + N_a)^2 N_e + |N_e − N_a| (1 − |N_e − N_a|) + (1 + N_a)^1_{γ0} . (20)

A. N_a ≤ N_e, i.e. N^′ ≤ N_s − N_{cp}

When N_a ≤ N_e (i.e. N^′ ≤ N_s−N_{cp}), (20) can be expressed as Υ_f =

(1 − N_e + N_a)^2 (2N_e − N_a) − (N_e − N_a)^2 + (1 + N_a)^1_{γ0}

. (21)

Deriving (21) with respect to N_a, we can get^∂_{∂Na} Υ_f > 0. That is to say, when the number of compensated samples is in the range of [0, N_s −N_{cp}], Υ_f reaches maximum by compensating N_s − N_{cp} samples.

y (nT + (l + N_c) T_s) ≈ 1 √ N_c N_c−1∑

k=0 α̃S_n (k) e^{j2πkΔf (lTs−τ)}e^{j2πfdnT} u (lT_s + N_cT_s − τ ) (11)

+ 1 √ N_c N_c−1∑

k=0 α̃S_{n+1} (k) e^{j2πkΔf (lTs−TCP −τ)}e^{j2πfd nT} u (lT_s + N_cT_s − T − τ ) + w_n (l) .

ỹ_n(i) = 1 √ N_c N_c−1∑

k=0 α̃S_{n−1} (k) e^{j2πkΔf (T +iTs −τ)}e^{j2πfd nT} u (T + iT_s − τ ) + w̃_n (i) (12)

+ 1 √ N_c N_c−1∑

k=0 α̃S_n (k) e^{j2πkΔf (iTs−τ)}e^{j2πfdnT} u( T i N^′ − 1

− T_{CP} ) + 1 √ N_c N_c−1∑

k=0 α̃S_n (k) e^{j2πkΔf (iTs −τ)}e^{j2πfd nT} u (iT_s − τ )

Ỹ_n (p) = (1 − N^s − N^{cp} N_c + N^′ N_c )α̃S_n (p) e^{−j2πpτNcTs} e^{j2πfd nT} + 1 N_c N_c−1∑

k=0 [α̃S_{n−1} (k) e^{j2πk(TCP −τ )} NcTs ( N_s−N_{cp}−1 ∑ i=0 e^{j2π(k−p)iNc} )]e^{j2πfdnT}

+ 1 N_c N_c−1∑

k=0,k≠p [α̃S_n (k) e^{−j2πkτN}c^Ts ( N^′ −1∑

i=0 e^{j2π(k−p)iN}c + N_c−1∑

i=N_s−N_{cp} e^{j2π(k−p)iN}c )]e^{j2πfd nT} + W̃_n (p) (14)

Υ_f = (1 −^{Ns−Ncp}_{Nc} +^{N ′}_{Nc} )^2 N_s−N_{cp} N_c + 1 N^2_c |Ns − Ncp − N ′| (N_c − |N_s − N_{cp} − N^′|) +^{Nc+N ′}_{Nc}^1_{γ0} (19)

B. N_a > N_e, i.e. N_s − N_{cp} < N^′ ≤ N_s

When N_a > N_e (i.e. N_s − N_{cp} < N^′ ≤ N_s), (20) can be expressed as

Υ_f =

(1 − N_e + N_a)^2 N_a − (N_a − N_e)^2 + (1 + N_a)^1_{γ0}

. (22)

Deriving (22) with respect to N_a, we can get ∂ ∂N_a Υ_f =

(1 − N_e + N_a) g (N_a) [ N_a − (N_a − N_e)^2 + (1 + N_a)^1_{γ0}

]_2 (23)

where

g (N_a) = N_a(3 + 1 γ_0

) + (1 + N_e) 1 γ_0

− (1 + N_e) . (24)

Since g (N_a) is an increasing function with respect to N_a, Υ_f is maximal when N^′ = N_s − N_{cp} or N^′ = N_s and can be expressed as in (25) and (26), respectively.

Υ_f (N_a=N_e) = N_c (N_s − N_{cp}) + (N_c + N_s − N_{cp})^1_{γ0}

. (25)

Υ_f (N_a= N_s N_c ) = (N_c + N_{cp})^2 N_cN_s − N^2_{cp} + N_c (N_c + N_s)^1_{γ0}

. (26)

• Υ_f (N_a=^{Ns}_{Nc} ) > Υ_f (N_a=N_e)

When d > d_0, where

d_0 =

T^2_D + T_DT_{CP} + T^2_{CP} 2T_D + T_{CP} c_0 2 , (27)

Υ_f (N_a=^{Ns}_{Nc} ) > Υ_f (N_a=N_e) is always satisfied. For d < d_0, the received SINR needs to satisfy γ_0 < γ, where γ= (N_c + N_{cp}) (N_c + N_s − N_{cp}) + N_c (N_s − N_{cp}) (N_c + N_{cp})^2 − N_s (N_c + N_{cp}) − N_c (N_s + N_{cp}) . (28) • Υ_f (N_a=^{Ns}_{Nc} ) < Υ_f (N_a=N_e)

When d < d_0, the received SINR needs to satisfy γ_0 > γ.

Remark 1:

(a) When the compensated sample 0 < N^′ ≤ N_s − N_{cp}, the SINR increases with increasing N^′.

(b) When the target distance d > d_0, regardless of the received SINR γ_0, the SINR after coherent compensation is the largest when N^′ = N_s.

(c) When the target distance d < d_0, the SINR after N^′ = N_s coherent compensation is the largest when γ_0 < γ. If γ_0 > γ, the SINR is the largest when compensating N^′ = N_s − N_{cp} samples.

After point-wise dividing S_n (p) in (14), the channel information can be obtained. The index corresponding to the peak in the RDM can be obtained in (29) and (30) through the 2D-FFT algorithm, as shown in Fig. 2. k̂=⌊ τ T_s ⌉. (29) l̂=⌊f_dMT ⌉. (30) Then, we can get the range and speed of the target as follows. r = c_0k̂ 2B . (31) v = c_0l̂ 2f_cM(N_c + N_{cp})T_s . (32)

Fig. 2: Sensing signal processing for target with echo delay exceeding CP duration.

IV. SIMULATION RESULTS

TABLE I: Simulation parameters [13]

Parameter Value Carrier frequency f_c 28 GHz Subcarrier spacing Δf 120 kHz Number of subcarriers N_c 4096 Number of OFDM symbols M 160 Elementary OFDM symbol duration T_D 8.33 μs CP duration T_{CP} 0.59 μs Entire OFDM symbol duration T 8.92 μs Modulation 16QAM

The simulation parameters are shown in TABLE I, which come from 3GPP TS 38.211. The speed of the target is not our main concern, so it is set to 20 m/s in this paper. For BS-based communication, there will be no ISI and ICI if the maximum delay extension doesn’t exceed the CP duration. But for BS-based sensing, it is required that the echo delay doesn’t exceed the CP duration. Due to the two-way characteristic, the coverage of sensing is much smaller than that of communication. So there will be a higher probability of the occurrence of ICI and ISI in BS-based sensing. It can be seen from TABLE I that under this configuration, the sensing range corresponding to the CP duration is only 88.5 m. If there is no special statement, the received SINR of echo signal of the 500 m target is set to 2 dB, and the received SINR of echo signal of target at other distance is calculated by the LOS path loss model in urban macro scenario as follows [14].

Pathloss [dB] = 28.0 + 22log_{10}(d) + 20log_{10}(f_c). (33)

where f_c is in GHz and the distance d between the transmitting and receiving antennas is in meters. In the following simulations, we use the SINR of RDM as a metric of performance.

(a) 300 m target (b) 500 m target

Fig. 3: The SINR of RDM of target at 300 m and 500 m vs. The number of compensated samples.

Fig. 3 shows the SINR of RDM versus the number of compensated samples when the target is located at 300 m with received SINR γ_0 = 11.76 dB and 500 m with received SINR γ_0 = 2 dB. It can be seen from Fig. 3(a) and Fig. 3(b) that the SINR of RDM increases as the number of compensated samples increases when N^′ ≤ N_s − N_{cp}, which verifies the Remark 1(a). When the number of compensated samples is N^′=N_s − N_{cp}, SINR of 300 m target’s RDM is maximized. But for 500 m target, the best length of compensated samples is N^′=N_s, verifying the Remark 1(c). Fig. 4 depicts the comparison of two compensation lengths for 800 m target at different received SINR. From Fig. 4 we can see, no matter what the received SINR is, the SINR of 800 m target’s RDM is maximized when N^′=N_s, which verifies the Remark 1(b).

Fig. 4: Comparison of two compensated sample lengths for 800 m target at different received SINR.

Fig. 5: SINR of targert’s RDM at different ranges.

Fig. 5 depicts the SINR of RDM obtained by 2D-FFT, coherent compensation for N^′ = N_s −N_{cp} and N^′ = N_s when the target is located at different ranges (echo delay exceeds CP duration). It can be seen from Fig. 5 that the SINR of RDM obtained by compensating N^′ = N_s − N_{cp} samples is better than that of traditional 2D-FFT algorithm. Because there is no ICI at this case, and the power of useful signal (i.e. peak of RDM) is increased through coherent compensation. When the target is relatively close, compensating N^′ = N_s samples will reduce the SINR of RDM. Because the received SINR of the echo is high, and the sample compensation will greatly enlarge the noise of RDM, which lowers the SINR of RDM. When the target is far away, the SINR of RDM obtained by compensating N^′ = N_s samples is better than that by compensating N^′ = N_s − N_{cp} samples.

Fig. 6: SINR of RDM of target at 500 m under different sensing algorithms

Fig. 6 demonstrates the SINR of RDM of target at 500 m obtained by 2D-FFT, VCP, and coherent compensation under different received SINR. The VCP scheme re-segments each sub-block into 12 OFDM symbols, and 4 OFDM symbols overlap between adjacent sub-blocks. The length of VCP is the sample offset corresponding to the echo delay. It can be seen from the figure that compared with the traditional 2D-FFT algorithm, the coherent compensation scheme improves the SINR of RDM by 2 ∼ 4 dB. However, it’s worth mentioning that the VCP scheme is less efficacious when constellation symbols are transmitted in the frequency domain. This is because the re-segmentation of the echo signal destroys the original OFDM structure, causing the symbols recovered by FFT to roughly follow the Gaussian distribution. Therefore, the probability of recovered frequency domain symbols with smaller amplitudes is higher. The noise will be amplified in the process of point-wise division, thus worsening the SINR of RDM.

Fig. 7: Range profile of target at 500m.

Fig. 7 plots the range profile obtained by coherent compensation and 2D-FFT when the target is located at 500 m. Compared with 2D-FFT scheme, coherent compensation scheme increases the peak power, which eventually enlarges the SINR in the range profile, albeit with the noise floor slightly raised simultaneously.

V. CONCLUSION

This paper studies ISAC BS, which utilizes the 3GPP TS 38.211 based OFDM waveform. When the echo delay exceeds CP duration, there will be ISI and ICI. The impaired SINR will limit sensing range. We propose to add some samples after each elementary OFDM interval to the front through coherent compensation to improve the SINR of each OFDM block. The simulation results show that the proposed algorithm improves the SINR of RDM compared with traditional 2D- FFT algorithm, which will expand the sensing range.

ACKNOWLEDGMENT

This work was supported in part by the National Natural Science Foundation of China (NSFC) under Grant U21B2014, 62271081, and 92267202, and in part by the National Key Research and Development Program of China under Grant 2020YFA0711302.

REFERENCES

[1] F. Liu et al., “Integrated sensing and communications: Toward dualfunctional wireless networks for 6G and beyond,” IEEE J. Sel. Areas Commun., vol. 40, no. 6, pp. 1728-1767, Jun. 2022.

[2] J. A. Zhang et al., “An overview of signal processing techniques for joint communication and radar sensing,” IEEE J. Sel. Top. Sign. Proces., vol. 15, no. 6, pp. 1295-1315, Nov. 2021.

[3] Z. Feng, Z. Fang, Z. Wei, X. Chen, Z. Quan and D. Ji, “Joint radar and communication: A survey,” China Communications, vol. 17, no. 1, pp. 1-27, Jan. 2020.

[4] Z. Wei et al., “Integrated sensing and communication signals toward 5G-A and 6G: A Survey,” IEEE Internet Things J., vol. 10, no. 13, pp. 11068-11092, 1 Jul., 2023.

[5] W. Zhou, R. Zhang, G. Chen and W. Wu, “Integrated sensing and communication waveform design: A survey,” IEEE open J. Commun. Soc., vol. 3, pp. 1930-1949, Oct. 2022.

[6] M. Braun, C. Sturm and F. K. Jondral, “On the single-target accuracy of OFDM radar algorithms,” in IEEE Int. Symp. Person Indoor Mobile Radio Commun. (PIMRC), 2011, pp. 794-798.

[7] C. Sturm and W. Wiesbeck, “Waveform design and signal processing aspects for fusion of wireless communications and radar sensing,” Proc. IEEE, vol. 99, no. 7, pp. 1236-1259, Jul. 2011.

[8] R. F. Tigrek, W. J. A. de Heij and P. van Genderen, “Multi-carrier radar waveform schemes for range and Doppler processing,” in IEEE Nat. Radar Conf. Proc., 2009, pp. 1-5.

[9] G. Hakobyan, M. Girma, X. Li, N. Tammireddy and B. Yang, “Repeated symbols OFDM-MIMO radar at 24 GHz,” in Euro. Radar Conf. (EuRAD), 2016, pp. 249-252.

[10] G. Hakobyan and B. Yang, “A novel intercarrier-interference free signal processing scheme for OFDM radar,” IEEE Trans. Veh. Technol., vol. 67, no. 6, pp. 5158-5167, Jun. 2018.

[11] A. Tang, S. Li and X. Wang, “Self-interference-resistant IEEE 802.11adbased joint communication and automotive radar design,” IEEE J. Sel. Top. Sign. Proces., vol. 15, no. 6, pp. 1484-1499, Nov. 2021.

[12] K. Wu, J. A. Zhang, X. Huang and Y. J. Guo, “Integrating lowcomplexity and flexible sensing into communication systems,” IEEE J. Sel. Areas Commun., vol. 40, no. 6, pp. 1873-1889, Jun. 2022.

[13] 3GPP, TS 38.211 (V17.3.0), “Physical channels and modulation,” Sep.

2022.

[14] 3GPP, TR 38.901 (V17.0.0), “Study on channel model for frequencies from 0.5 to 100 GHz,” Mar. 2022.