arXiv:2308.09489v2 [cs.IT] 17 Jul 2024

STAR-RIS Aided MISO SWIPT-NOMA System with Energy Buffer: Performance Analysis and Optimization

Kengyuan Xie, Guofa Cai, Jiguang He, Senior Member, IEEE, Georges Kaddoum, Senior Member, IEEE

Abstract—In this paper, we propose a simultaneous transmitting and reflecting reconfigurable intelligent surface (STAR-RIS) and energy buffer aided multiple-input single-output (MISO) simultaneous wireless information and power transfer (SWIPT) nonorthogonal multiple access (NOMA) system, which consists of a STAR-RIS, an access point (AP), and reflection users and transmission users with energy buffers. In the proposed system, the multi-antenna AP can transmit information and energy to several single-antenna reflection and transmission users simultaneously by the NOMA fashion in the downlink, where the power transfer and information transmission states of the users are modeled using Markov chains. The reflection and transmission users harvest and store the energy in energy buffers as additional power supplies, which are partially utilized for uplink information transmission. The power outage probability, information outage probability, sum throughput, and joint outage probability closed-form expressions of the proposed system are derived over Nakagami-m fading channels, which are validated via simulations. Results demonstrate that the proposed system achieves better performance as compared to the proposed system with discrete phase shifts, the STAR-RIS aided MISO SWIPT-NOMA buffer-less, conventional RIS and energy buffer aided MISO SWIPT-NOMA, and STAR-RIS and energy buffer aided MISO SWIPT-time-division multiple access (TDMA) systems. Furthermore, a particle swarm optimization-based power allocation (PSO-PA) algorithm is designed to maximize the uplink sum throughput with a constraint on the uplink joint outage probability and Jain’s fairness index (JFI). Simulation results illustrate that the proposed PSO-PA algorithm can achieve an improved sum throughput performance of the proposed system.

Index Terms—Simultaneous transmitting and reflecting reconfigurable intelligent surface (STAR-RIS), energy buffer, simultaneous wireless information and power transfer (SWIPT), non-orthogonal multiple access (NOMA), Markov chains.

I. INTRODUCTION

Internet of Things (IoT) has been considered one of the key and enabling paradigms for a plethora of applications in healthcare, smart cities, and smart homes [1]. In the IoT era, various low-power wireless sensor devices are connected to the network and interact with each other. However, the everincreasing of wireless electronics inevitably imposes challenges on the power supply of devices and massive multiple access,

K. Xie and G. Cai are with the School of Information Engineering, Guangdong University of Technology, China (e-mail: xiekengyuan@126.com, caiguofa2006@gdut.edu.cn).

J. He is with the Technology Innovation Institute, Abu Dhabi, United Arab Emirates, and also with Centre for Wireless Communications, University of Oulu, Oulu 90014, Finland (e-mail: jiguang.he@tii.ae).

G. Kaddoum is with the Department of Electrical Engineering, University of Québec, Québec, QC G1K 9H7, Canada, and also with the LaCIME Laboratory, École de Technologie Supérieure (ÉTS), Montreal, QC H3C 1K3, Canada (email: georges.kaddoum@etsmtl.ca).

owing to the limited battery lifespans of devices and scarce spectral resources [2].

Regarding the limited battery challenge although several energy harvesting methods, such as solar and wind energy harvesting, can capture energy from the environment, their availability is out of control [3]. To prolong the operational lifetime of the energy-constrained and low-power devices, simultaneous wireless information and power transfer (SWIPT) has been proposed, which offers a controllable way to charge devices by utilizing the ubiquitous radio-frequency (RF) signals [4]. SWIPT enables devices to receive power and information simultaneously. In addition, to tackle the aforementioned massive connectivity issue, non-orthogonal multiple access (NOMA) technology has been proposed [5]. In contrast to orthogonal multiple access (OMA), NOMA allows multiple users to share the same time-frequency resource, therefore providing better spectrum efficiency [6]. Recent studies have combined NOMA and SWIPT to prolong the lifetime of energy-constrained IoT networks and support massive connectivity [7]–[9]. In [7], a downlink coordinated multipoint SWIPT-NOMA network was proposed. To further improve the performance, multiple antennas have been introduced into the SWIPT-NOMA system. In [8], a multiuser multiple-input single-output (MISO) SWIPT-NOMA network was studied, where a novel hybrid user pairing scheme was proposed. In [9], a millimeter-wave multiple-input multiple-output (MIMO) SWIPT-NOMA system was investigated. The above works assumed that all harvested energy is consumed in one time slot and energy harvesting is performed with the harvest-use (HU) architecture. However, in practice, the harvested energy is small and random, which limits the performance of SWIPT-NOMA systems. Therefore, the energy buffer with the harvest-store-use (HSU) architecture was considered for storing the harvested energy, which can improve the performance of self-sustaining nodes [10]–[12]. In [10], a wireless-powered cooperative NOMA relay network was considered, where the relay was provisioned with an energy buffer to improve energy efficiency. In [11], an adaptive multiuser cooperative NOMA scheme was studied, where the nearuser was equipped with an energy buffer to harvest energy from the ambiance, thus improving the system throughput. In [12], a MISO wireless-powered NOMA network was investigated, which considers the utilization of a data buffer and energy storage at sources to achieve both a higher sum rate and improved fairness.

Recently, reconfigurable intelligent surfaces (RISs) have received extensive attention from both academia and industry, which can bring enhanced spectrum and energy efficiencies [13]. A RIS is composed of massive reflecting elements that are energy efficient and cost-effective [14], which has been introduced into SWIPT-NOMA systems for improved system performance. On the one hand, the efficiency of SWIPT highly depends on the existence of a line-of-sight (LoS) link [15] which may be blocked by various obstacles due to long distance transmissions. On the other hand, the far-field user in NOMA may experience poor performance due to path loss. RISs are not only capable of building virtual LoS links when LoS links are blocked [16], but can also bring outstanding performance gains in SWIPT [17]. Hence, tremendous research efforts have been devoted to RIS aided SWIPT-NOMA systems [18]–[24]. A RIS assisted cooperative SWIPT-NOMA system was investigated in [18], [19], where [18] focused on improving the achievable rate of the strong user while guaranteeing the weak user’s quality of service, and [19] is devoted to maximizing the data rate of the cell-edge user. The age of information minimization problem of the RIS aided SWIPT-NOMA system was investigated in [20]. The max-min energy efficiency problem of the active RIS aided multi-cluster cooperative SWIPT-NOMA system was studied in [21]. A RIS aided SWIPT-wireless-powered communication network NOMA system was found to ameliorate transmission efficiency in [22]. A cooperative NOMA mobile edge computing (MEC) network aided by RIS and SWIPT was analyzed in [23]. A RIS aided MISO SWIPT-NOMA system was proposed in [24], which is considered a cooperative transmission scheme to improve the performance of cell-edge users. However, in [18]–[24], the HU architecture was utilized to harvest energy, where energy harvesting nodes do not buffer the energy for use in future time slots. Moreover, the conventional RIS only reflects the signal to users, which makes it necessary for the transmitter and receiver to be on the same side.

To overcome the limitation of user distribution in conventional RIS aided systems, the novel concept of simultaneous transmitting and reflecting RIS (STAR-RIS) has been recently proposed [25]. Different from the conventional RIS, STAR-RIS provides full-space service coverage and a more flexible deployment [26], which can not only reflect but also transmit (also known as refract) the incident signal. Specifically, the incident signal on the STAR-RIS is divided into two parts. One part is reflected to the same space as the transmitter, i.e., the reflection space, and the other part is transmitted to the opposite space, i.e., the transmission space [27]. Moreover, three practical protocols of STAR-RIS have been proposed in [27], i.e., time-switching, mode-switching, and energy-splitting. Because the STAR-RIS would divide the incident signal into two portions in the energysplitting protocol and mode-switching protocol, a multiple access scheme is necessary to distinguish these two parts to decode them successfully [28]. NOMA has been considered to be a promising multiple-access technique due to its ability to provide enhanced spectral efficiency and connectivity [29]. Recently, STAR-RIS aided NOMA networks have been investigated in several works [30]–[32]. In [30], a STAR-RIS aided NOMA system was investigated to maximize the achievable sum rate. In [31], a STAR-RIS assisted downlink MISO-NOMA network was considered for maximizing the system energy efficiency. In [32], a STAR-RIS assisted downlink MIMO-NOMA network was considered to investigate the energy-efficient resource allocation. To study the potential benefits of deploying STAR- RIS in wireless-powered transmission, there have been some initial works on STAR-RIS aided wireless-powered systems [33]–[36]. In [33], a STAR-RIS aided wireless-powered MEC system was investigated. In [34], a STAR-RIS assisted wirelesspowered IoT network was proposed, which adopts the time division multiple access (TDMA) scheme. In [35], a STAR- RIS aided wireless-powered NOMA system was investigated, where the time-switching protocol and energy-splitting protocol of STAR-RIS are utilized to improve the sum throughput. In [36], a STAR-RIS aided SWIPT system was proposed, where STAR-RIS employs the time-switching protocol. However, in [33]–[36], only single-antenna access points (APs) with the HU architecture were considered.

In light of the aforementioned motivations, we propose a STAR-RIS and energy buffer aided MISO SWIPT-NOMA system in this paper. The HSU architecture for users with energy buffers is adopted to achieve energy management, thus ensuring better performance. The main contributions of this paper can be summarized as follows:

• We consider a STAR-RIS and energy buffer aided MISO SWIPT-NOMA system, where a multi-antenna AP transmits the superimposed signals to several single-antenna users via the direct link and reflection/transmission links assisted by STAR-RIS in the downlink, and the users transmit their data to the AP in the uplink. Successive interference cancellation (SIC) is considered for information decoding. Moreover, the reflection and transmission users are equipped with energy buffers to enhance the system’s sustainability, where the power transfer and information transmission states are modeled using Markov chains. In this system, the sustainability is studied from the perspectives of both energy acquisition and consumption.

• By exploiting the moment-matching approach, the proposed system’s power outage probability, information outage probability, and sum throughput performances are derived in closed-form over Nakagami-m fading channels^1. The power and information outage probabilities are combined into a closed-form joint outage probability. Simulations are carried out to verify the accuracy of the theoretical analysis and demonstrate that the proposed system offers improved performance compared to baseline schemes.

• To achieve the maximization of uplink sum throughput while ensuring a certain uplink joint outage probability and Jain’s fairness index (JFI) for users, a low-complexity particle swarm optimization-based power allocation (PSO-PA) algorithm is proposed to find the optimal energy-splitting ratios of the STAR-RIS and the transmit power allocation factors. Results unveil that the proposed PSO-PA algorithm provides an improved sum throughput performance for the proposed system.

The rest of this paper is organized as follows. In Section

1Nakagami-m fading channels have been adopted in RIS or STAR-RIS aided communication systems due to their generic property [37], [38], which can characterize wireless signal propagation in a variety of environments. It should be noted that Nakagami-m fading channels can be reduced into other channels, such as Rayleigh and Rician, by changing the value of m [38], [39].

Fig. 1: STAR-RIS and energy buffer aided MISO SWIPT-NOMA system.

II, we introduce the system model. In Section III, we analyze the performance of the proposed system. In Section IV, we propose the resource allocation method. Simulation results and discussions are summarized in Section V. Finally, we conclude the paper in Section VI.

Notations: Matrices and vectors are denoted by uppercase bold and lowercase bold, respectively. C^{M×1} denotes the space of M × 1 complex vectors. j^2 = −1 and j denotes the imaginary unit. diag(x) denotes a diagonal matrix with the elements of vector x on the main diagonal. The complex Gaussian distribution is denoted by CN ( μ, σ^2 ) with mean μ and variance σ^2. K_α (·) denotes the modified Bessel function of the second kind. I_α (·) is the α-th order Bessel function of the first kind. γ (·, ·) is the upper incomplete Gamma function. Γ (·) is the Gamma function. E (·) and Var (·) represent the expectation and variance operations, respectively. max (a, b) returns the maximum of a and b.

II. SYSTEM MODEL This section first describes the proposed system and its downlink signal model, and then presents the energy consumption model and the uplink signal model.

A. STAR-RIS and Energy Buffer Aided MISO SWIPT-NOMA System

Fig. 1 illustrates the proposed STAR-RIS and energy buffer aided MISO SWIPT-NOMA system, consisting of an L-antenna AP, a STAR-RIS, reflection users, and transmission users. The L-antenna AP can communicate with single-antenna reflection users and transmission users with the aid of the STAR-RIS that is composed of N low-cost reflective elements. It is assumed that the direct link from the AP to the user is available. In this paper, it is assumed that AP has a fixed energy supply, while U_r and U_t are powered by harvested energy due to energy constraints. Time-division duplex (TDD) communication is adopted. First, the AP simultaneously transmits the energy and information to U_r and U_t in the downlink using NOMA. Then, U_r and U_t use the harvested energy to power the signal processing circuit and transmit signals to AP in the uplink. The information transmission and energy transfer between AP and U_k, k ∈ {t, r} are assisted by STAR-RIS.

Remark 1: Considering the complexity of SIC at the user, NOMA is applied between a pair of users, i.e., two users, which is a basic case studied in previous works [32]. In fact, AP performs user pairing based on the channel gains of different users in NOMA systems [8], [40], [41]. In the proposed system, user pairing depends on the channel gains of the users in the reflection and transmission spaces. Specifically, similar to [8], [40], [41], the channel gains of the users in the reflection and transmission spaces are ranked from smallest to largest, respectively. To enlarge the channel gains difference between two users from different spaces, the unmatched user with the highest channel gain in the reflection space is paired with the unmatched user with the lowest channel gain in the transmission space. Similar to [42], [43], multiple NOMA-pairs can be served via TDMA to avoid interference between them. For simplicity of presentation and revealing fundamental insights, we consider one of NOMA-pairs^2, i.e., one reflection user U_r and one transmission user U_t.

B. Downlink Signal Model

The STAR-RIS works using the energy-splitting protocol^3, where the AP can simultaneously communicate with users located on opposite sides of the STAR-RIS using NOMA. In the energy-splitting protocol, each element of the STAR-RIS operates simultaneously in transmission and reflection modes, where √ β_r, √ β_t ∈ [0, 1] denote the energy-splitting ratios. β_r +β_t = 1 holds based on the law of energy conservation [29]. Let φ_r^Δ= [√ β_re^{jφr1} , . . . , √ β_re^{jφrN} ] and φ_t^Δ= [√ β_te^{jφt1} , . . . , √ β_te^{jφtN} ] denote the STAR-RIS’s reflection and transmission coefficient vectors, where φ^r_i , φ^t_i ∈ [0, 2π) , i ∈ {1, 2, . . . , N} denote the phase-shift adjustments at the i-th element.

1) Downlink Information Transmission: The quasi-static flatfading channels were assumed [11], [44]. Let H̃ ∈ C^{N×L} be the complex channel coefficients matrix, g̃_k ∈ C^{1×N} be the complex channel coefficients vector, h̃^0_k ∈ C^{1×L} be the complex channel coefficients vector of the direct link between the AP and STAR-RIS, the STAR-RIS and U_k, and the AP and U_k. The AP uses NOMA to form a superimposed signal s = √ P_{AP}/L (√ α_rs_r + √ α_ts_t ) , where P_{AP}/L is the transmit power of each antenna at the AP, α_r and α_t are the transmit power allocation factors for U_r and U_t with α_r + α_t = 1, and s_r and s_t are the unit-energy information signals of U_r and U_t, i.e., E ( |s_r|^2 ) = E ( |s_t|^2 ) = 1.

In the proposed system, the power-splitting mode is adopted in the SWIPT, with θ being the power-splitting factor, which indicates the portion of the received signal used for information decoding. The received signal for information decoding at U_k can be expressed as

y_k = √ θ ( h̃^0_k w + g̃_kdiag(φ_k)H̃w ) s + n_k = √ θβ_k L∑ ℓ=1 ( h̃^0_{k,ℓ}e^{−jϖ}ℓ +^N ∑ i=1 h̃_{ℓ,i}g̃_{k,i}e^j(^{φk}i^{−ϖ}ℓ) ) s+n_k, (1)

where w = [ e^{−jϖ1} , . . . , e^{−jϖL} ] is the beamforming vector, and n_k is the additive white Gaussian noise (AWGN) with n_k ∼ CN (0, N_0).

2The derived results can be extended to multiple transmission and reflection users’ scenario. In addition, the development of a more efficient user pairing mechanism for multiple users scenarios in STAR-RIS can be an interesting future work.

3In fact, since the mode-switching protocol is a special case of the energy splitting protocol [27], the energy-splitting protocol is considered in this paper.

2) Energy Harvesting: Both users receive the superimposed signal s, which includes the signals √ α_rs_r and √ α_ts_t. Since α_r + α_t = 1, the harvested energy for U_k can be calculated as

E_k = η (1 − θ) β_k | | | | | L∑ ℓ=1 h̃^0_{k,ℓ}e^{−jϖ}ℓ +^N ∑ i=1 h̃_{ℓ,i}g̃_{k,i}e^j(^{φk}i^{−ϖ}ℓ) | | | | | 2 αr PAP L Ts

+ η (1 − θ) β_k | | | | | L∑ ℓ=1 h̃^0_{k,ℓ}e^{−jϖ}ℓ +^N ∑ i=1 h̃_{ℓ,i}g̃_{k,i}e^j(^{φk}i^{−ϖ}ℓ) | | | | | 2 αt PAP L Ts

= η (1 − θ) β_k | | | | | | L∑ ℓ=1 h̃^0_{k,ℓ}e^{−jϖ}ℓ +^N ∑ i=1 h̃_{ℓ,i}g̃_{k,i}e^j(^{φk}i^{−ϖ}ℓ) | | | | | | 2 PAP L Ts, (2) where η denotes the energy conversion efficiency factor, and T_s is the symbol duration.

The complex channel coefficients are represented by polar coordinates as h̃^0_{k,ℓ} = h^0_{k,ℓ}e^{−jξℓ} , h̃_{ℓ,i} = h_{ℓ,i}e^{−jμℓ,i} , g̃_{k,i} = g_{k,i}e^{−jσi} , where h^0_{k,ℓ}, h_{ℓ,i}, g_{k,i} denote the magnitudes of

the channel coefficients with | | |h̃^0_{k,ℓ} | | | = h^0_{k,ℓ}, | | |h̃ℓ,i | | | = hℓ,i, | g̃_{k,i} | = g_{k,i}, and ξ_ℓ, μ_{ℓ,i}, σ_i, {ξ_ℓ, μ_{ℓ,i}, σ_i} ∈ [0, 2π], denote the phases of h̃^0_{k,ℓ}, h̃_{ℓ,i}, g̃_{k,i}. The magnitudes of the channel coefficients follow the Nakagami-m distributions. Hence h^0_{k,ℓ} ∼

Nakagami ( m^0_{k,ℓ}, Ω^0_{k,ℓ} ) , h_{ℓ,i} ∼ Nakagami (m_{ℓ,i}, Ω_{ℓ,i}), g_{k,i} ∼ Nakagami (m_{k,i}, Ω_{k,i}), where m^0_{k,ℓ} > 0, m_{ℓ,i} > 0, m_{k,i} > 0 denote the shape parameters, and Ω^0_{k,ℓ}, Ω_{ℓ,i}, Ω_{k,i} denote the spread parameters of the Nakagami-m distributions. The spread parameters are given as Ω^0_{k,ℓ} = l_{AP,Uk} , Ω_{ℓ,i} = l_{AP,S-R}, and Ω_{k,i} = l_{S-R,Uk} , where l_{X,Y} = τ/d^ϑ_{X,Y} denotes the path-loss coefficient and is integrated into the spread parameters with ϑ being the path-loss exponent, τ the path-loss at a reference distance of 1 meter, d_{X,Y} the distance between X and Y with X ∈ {AP, S-R (STAR-RIS)} and Y ∈ {S-R, U_t, U_r}. Hence, (2) can be expressed as

E_k = η (1 − θ) β_k | | | | | L∑ ℓ=1 h^{0k,ℓ}e^{−j(ξℓ+ϖℓ)} + N∑ i=1 h_{ℓ,i}g_{k,i} ×e^j(^{φki −ϖℓ−μℓ,i−σi})

| | | | | 2 PAP L Ts. (3) Considering perfect channel state information (CSI)^4 [27], [29], the maximum available energy can be obtained by the semidefinite relaxation (SDR) technique with the optimal phase-shift value ϖ_ℓ of the beamforming vector and φ^k_i of the STAR-RIS [44]. To avoid the high computational complexity of SDR, we consider a lower complexity suboptimal scheme. Specifically, first, the phase-shift value ϖ_ℓ of the beamforming vector is fixed at the AP, where its value is opposite to the phase of the direct link, i.e., ϖ_ℓ = −ξ_ℓ. Then, the maximum available energy can be obtained by the phase-shifts φ^k_i of the STAR-RIS, i.e., φ^k_i = ϖ_ℓ + μ_{ℓ,i} + σ_i. Hence, (3) can be re-expressed as

E_k = η (1 − θ) β_k | | | | | L∑ ℓ=1 ( h^0_{k,ℓ} + N∑ i=1 h_{ℓ,i}g_{k,i} )| | | | 2 PAP L Ts. (4) C. Energy Consumption Model

The energy consumption of each user mainly includes two components, i.e., the circuit power and the transmission power consumption [45]. Specifically, the circuit power consumption for transmitting and receiving one bit is E_c (nJ/bit), while the transmission power consumption per bit is E_{tp} ( pJ/bit/m^2). Moreover, according to [46], the computing module power

4The impact of imperfect CSI on the performance of the proposed system is examined in Sect. V. In addition, the design of more efficient CSI estimation methods for STAR-RIS is an interesting but challenging future work.

Fig. 2: The Markov chain model of power states with a rechargeable energy buffer (S_0: Outage, and S_1: Sufficient power).

consumption is E_{comp} (nJ/bit). Hence, the overall power consumption of the user for receiving and transmitting M bits over a distance d_{AP,Uk} can be calculated as Es = 2MEc + Md^2_{AP,Uk} Etp + Ecomp, (5) where both the circuit power consumption for receiving and transmitting M bits at each user consumes ME_c energy. In particular, typical values for E_c and E_{tp} are 50 nJ/bit and 100 pJ/bit/m^2, respectively [45]. In addition, the power consumption of the computing module is about 8% of the total power consumption [46], [47], i.e., E_{comp} ≈ 8.7% ( 2ME_c + Md^2_{AP,Uk} E_{tp} ) . D. Uplink Signal Model

Both users simultaneously send their signals to AP by utilizing the transmission power of the energy consumption model. The received signal at the AP can be expressed as yAP = √ Ptβt L∑ ℓ=1 ( h̃^0_{t,ℓ}e^{−jϖ}ℓ +^N ∑ i=1 h̃_{ℓ,i}g̃_{t,i}e^j(^{φt}i^{−ϖ}ℓ) ) st

+ √ Prβr L∑ ℓ=1 ( h̃^0_{r,ℓ}e^{−jϖ}ℓ +^N ∑ i=1 h̃_{ℓ,i}g̃_{r,i}e^j(^{φr}i^{−ϖ}ℓ) ) sr + Ln_k , (6) where P_k =^{Md2AP,Uk Etp}_{Ts} .

III. PERFORMANCE ANALYSIS

This section presents the proposed system’s closed-form power outage probability expression over Nakagami-m fading channels. Moreover, the downlink and uplink closed-form information outage probability and sum throughput expressions are derived. Based on power and information outage probabilities, the downlink and uplink closed-form joint outage probabilities of the proposed system are obtained.

A. Power Outage Probability

The power states of U_k are modeled by a Markov chain, as shown in Fig. 2. In each time slot, U_k can either be in the power sufficient state S_1 or the power outage state S_0^5. The states of U_k at the (q − 1)-th, q-th, and (q + 1)-th time slots are illustrated in Fig. 2. The transition probabilities between two power states are represented by P^{k,po}_{uv} , where u, v ∈ {0, 1} with 0 corresponding to state S_0 and 1 corresponding to state S_1. Specifically, the transition probabilities from a given state at q-th

5In this paper, we aim to determine if there is a power outage in the energy buffer, which affects the downlink and uplink information transmission. In this paper, two states, i.e., power sufficient and outage states, are used to model the energy buffer [46], where the energy buffer is modeled as two energy levels. In fact, there will be a power outage when the energy is below the second energy level, and vice versa. Thus, two energy levels are enough to model the energy buffer in the proposed system. In addition, simulation of more energy levels [48], [49] is presented in Sect. V.

time slot to the states at (q + 1)-th time slot are expressed as P^{k,po}_{00} (q), P^{k,po}_{01} (q), P^{k,po}_{10} (q), and P^{k,po}_{11} (q) [46]. It is assumed that there are Q consecutive time slots, q denotes the q-th time slot (q = 1, 2, . . . , Q), and C is the initial state of the battery. The residual energy of q = 1 and q = 2 can be expressed as, respectively B_k (1) = E_k (1) + C − Es, (7) B_k (2) = B_k (1) + E_k (2) − Es. (8)

Hence, the residual energy of q-th time slot can be summarized as B_k (q) = B_k (q − 1) + E_k (q) − Es = B_k (q − 2) + E_k (q − 1) − Es + E_k (q) − Es . . = q∑ l=1 E_k (l) + C − qEs, (9)

where E_k (l)=η (1 − θ)β_k | | |^L∑ ℓ=1 ( h^0_{k,ℓ,l} +^N ∑ i=1 h_{ℓ,i,l}g_{k,i,l} )| | 2 P_{AP} L T_s, h^0_{k,ℓ,l}, h_{ℓ,i,l}, g_{k,i,l} denote the time-varying channel magnitudes at time slot l with l ∈ {1, 2, . . . , q}.

To ensure that no power outage occurs at the q-th time slot, B_k (q) should be greater than or equal to 0. Thus, we can calculate the transmission probability P^{k,po}_{11} (q) to ensure that the power is sufficient at the q-th time slot (i.e., the cumulative harvested energy of the energy buffer should not be less than the consumption). P^{k,po}_{11} (q) is given by

P^{k,po}_{11} (q) = Pr (_q ∑ l=1 E_k (l) + C ≥ qEs )

= Pr (_q ∑ l=1 η (1 − θ) β_k PAP L TsZ^2_l + C ≥ qEs )

= Pr (_q ∑ l=1 Z^2_l ≥ L (qEs − C) η (1 − θ) β_kPAPTs ) , (10)

where Z_l =^L ∑ ℓ=1 ( h^0_{k,ℓ,l} +^N ∑ i=1 h_{ℓ,i,l}g_{k,i,l} ) . We first derive the probability density function (PDF) of q∑ l=1 Z^2_l . Let V_{ℓil} = h_{ℓ,i,l}g_{k,i,l}, and the n-th moment of V_{ℓil}

can be expressed as shown in (11) [39]. μV_{ℓil} (n) = λ^{−n}_{ℓi} Γ (m_{ℓ,i} + n/2) Γ (m_{k,i} + n/2) Γ (m_{ℓ,i}) Γ (m_{k,i})

, (11)

where λ_{ℓi} = √_{mℓ,i} Ω_{ℓ,i} m_{k,i} Ω_{k,i} .

Let G_{ℓl} = ∑_N i=1 V_{ℓil}. Using multinomial expansion [50], the n-th moment of G_{ℓl}, i.e., μ_{Gℓl} (n)^Δ= E (G^n_{ℓl}), can be obtained as μG_{ℓl} (n) = n∑ n1 =0 n1∑ n2=0 · · · nN −2∑

nN −1=0 ( n n1 ) ( n1 n2 ) · · · ( nN−2 nN−1 )

× μV_{ℓil} (n − n1) μV_{ℓil} (n1 − n2) · · · μV_{ℓil} (nN−1) . (12) From (11) and (12), the first and second moments of G_{ℓl} is obtained as

μG_{ℓl} (1) = N∑ i=1 μV_{ℓil} (1), (13)

μG_{ℓl} (2) = N∑ i=1 μV_{ℓil} (2) + 2 N∑ i=1 μV_{ℓil} (1) N∑ i′ =i+1 μV_{ℓi′ l} (1) . (14)

Since h^0_{k,ℓ,l} ∼ Nakagami ( m^0_{k,ℓ}, Ω^0_{k,ℓ} ) , one has μ_h0_{k,ℓ,l} (n) = Γ ( m^0_{k,ℓ} + n/2 ) Γ ( m^0_{k,ℓ} ) ( m^0_{k,ℓ} Ω^0_{k,ℓ} )_{−n/2} . (15)

Let P_{ℓl} = h^0_{k,ℓ,l}+G_{ℓl}. The n-th moment of P_{ℓl} can be expressed as μ_{Pℓl} (n)^Δ= E (P^n_{ℓl}) = E (( h^0_{k,ℓ,l} + G_{ℓl} )_n) , where h^0_{k,ℓ,l} and G_{ℓl} are mutually independent. Using the binomial theorem, μ_{Pℓl} (n) is calculated as

μP_{ℓl} (n) = E [_n ∑ ε=0 ( n ε ) h^{0,ε}_{k,ℓ,l}G^{n−ε}_{ℓl} ]

= n∑ ε=0 ( n ε ) μ_h0_{k,ℓ,l} (ε) μG_{ℓl} (n − ε). (16) Hence, one has

μP_{ℓl} (1) = μ_h0_{k,ℓ,l} (1) + μG_{ℓl} (1) , (17)

μP_{ℓl} (2) = μ_h0_{k,ℓ,l} (2) + μG_{ℓl} (2) + 2μ_h0_{k,ℓ,l} (1) μG_{ℓl} (1) . (18)

The distribution of P_{ℓl} can be approximated with a Gamma distribution by the moment-matching approach [51], [52], i.e., P_{ℓl} ∼ Gamma (χ, ϕ) , (19) where χ = [E (P_{ℓl})]^2 Var (P_{ℓl}) = [μP_{ℓl} (1)]^2 μP_{ℓl} (2) − [μP_{ℓl} (1)]^2

, (20) ϕ = E (P_{ℓl}) Var (P_{ℓl}) = μP_{ℓl} (1) μP_{ℓl} (2) − [μP_{ℓl} (1)]^2

. (21)

Since Z_l =^L ∑ ℓ=1 P_{ℓl}, one has Z_l ∼ Gamma (Lχ, ϕ). The mean

and variance of Z_l are E (Z_l) = Lχ/ϕ and Var (Z_l) = Lχ/ϕ^2,

respectively. Let^q ∑ l=1 Z^2_l = T . T follows the non-central chi-

square distribution with q degrees of freedom. Therefore, the PDF of T is expressed as fT (x) = 1 2σ^2 ( x s^2 ) q−2_4 e^{− s} 2+x 2σ2 I q_{2 −1} ( s σ^2 √ x ) , (22)

where σ^2 = Var (Z_l) and s = √ q(E (Z_l))^2. Thus, P^{k,po}_{11} (q) can be calculated as

P^{k,po}_{11} (q) = ∫_∞ L(qEs −C) η(1−θ)βk PAPTs fT (x)dx

= ∞∑ ς=0

q 2 −1+ς ∑ p=0 s^{2ς} e^{− s} 2 2σ2 (2σ^2)^{ς+p}ς! e^− L(qEs−C) 2σ2 η(1−θ)βk PAP Ts (_{L(qEs−C)} η(1−θ)βk PAPTs )_p p! . (23)

The detailed derivation of (23) is given in Appendix A. When β_k = 0, one has lim_{βk =0}^{L(qEs −C)}

η(1−θ)β_k P_{AP} T_s = ∞. Using

lim_{x→∞} e^{−x}x = 0, (23) can be expressed as P^{k,po}_{11} (q) = 0. To

ensure P^{k,po}_{11} (q) > 0, β_k should be greater than zero.

It is noted that q ≥ 2 in (23) satisfies (_q 2 − 1 + ς ) ≥ 0. For the special case of q = 1, one has

P^{k,po}_{11} (q = 1) = Pr ( Z^2_l ≥ L (qEs − C) η (1 − θ) β_kPAP Ts ) . (24)

Since Z_l ∼ Gamma (Lχ, ϕ), the CDF of Z_l can be expressed as FZ_l (x) = 1 Γ (Lχ) γ (Lχ, ϕx) . (25) For Y = X^2, the CDF of Y can be calculated as F_Y (y) = F_X (√ y ) . The CDF of Z^2_l is computed as F_Z2_l (x) = 1 Γ (Lχ) γ ( Lχ, ϕx^{12} ) . (26)

Fig. 3: The CDF and PDF of P_{ℓl} for the true distribution and the approximate Gamma distribution.

The PDF of Z^2_l is obtained as

f_Z2_l (x) = ϕ^{Lχ}e^{−ϕx} 1 2 x^{Lχ−22} 2 (Lχ − 1)!

. (27)

Thus, (24) can be calculated as

P^{k,po}_{11} (q = 1) = 1− 1 Γ (Lχ) γ ( Lχ, ϕ ( L (qEs − C) η (1 − θ) β_k PAPTs )1_2) . (28)

According to the Markov model presented in Fig. 2, the power outage probability P^{k,po} of U_k over Q time slots is calculated as P^{k,po} = 1 − Q∏ q=1 P^{k,po}_{11} (q). (29)

Remark 2: For the buffer-less system, P^{k,po}_{11} (q) degenerates to P^{k,po}_{11} (q = 1) at each time slot. The power sufficient proba-

bility of a buffer-less system is^Q ∏ q=1 P^{k,po}_{11} (1). Hence, the overall

power outage P^{k,po}_{bl} of a buffer-less system over Q time slots

can be expressed as P^{k,po}_{bl} = 1 − ( P^{k,po}_{11} (1) )_Q . Remark 3: Fig. 3 presents the cumulative distribution function (CDF) and PDF of P_{ℓl} for the true distribution and the approximate Gamma distribution. The true distribution is generated through Monte Carlo simulations. It can be observed that the approximate CDF and PDF are consistent with true CDF and PDF, respectively, which validates the correctness of our analysis. The fitted Gamma distribution becomes more accurate with a larger number of STAR-RIS elements [28]. In addition, from the simulation and theory analysis results in Sect. V, it can be also seen that the simulated curves match with the theoretical ones.

Proposition 3.1: The minimum power outage probability can be achieved when the initial state of the battery satisfies the overall power consumption over Q time slots, i.e., C = QE_s.

Proof: We take the derivative of P^{k,po}_{11} (q). One has ∂P^{k,po}_{11} (q) ∂C = ∞∑ ς=0 s^{2ς} e^{− s} 2 2σ2 (2σ^2)^ς ς! e^− L(qEs−C) 2σ2 η(1−θ)βk PAPTs L 2σ^2η (1 − θ) β_k PAPTs

× q 2 −1+ς ∑ p=0

(_{L(qEs−C)} η(1−θ)βk PAPTs )_p p! − q 2 −1+ς ∑ p=1

(_{L(qEs−C)} η(1−θ)βk PAPTs )_{p−1} (p − 1)!

= ∞∑ ς=0 s^{2ς} e^{− s} 2 2σ2 (2σ^2)^ς ς! e^− L(qEs −C) 2σ2 η(1−θ)βk PAP Ts L 2σ^2η (1 − θ) β_kPAPTs (_{L(qEs−C)} η(1−θ)βk PAPTs ) q_{2 −1+ς} (_q 2 − 1 + ς ) ! . (30)

By assigning^{∂P k,po11 (q)}_{∂C} = 0, one has C = qE_s. Considering Q time slots, we have that if C = QE_s, the power outage probability is minimized over Q time slots.

Proposition 3.2: The average residual energy after Q time slots is given by C_R = η (1 − θ) β_kP_{AP}T_sQ^{χ(Lχ+1)}_{ϕ2} + C − QE_s. Only if η (1 − θ) β_kP_{AP}T_s^{χ(Lχ+1)}_{ϕ2} ≥ E_s, a sustainable wireless node is possible. Otherwise, the system will gradually deteriorate to a buffer-less system.

Proof: We perform the expectation operation on the residual energy after Q time slots. One has CR = E (_Q ∑ l=1 E_k + C − QEs )

= E (_Q ∑ l=1 η (1 − θ) β_k PAP L TsZ^2_l + C − QEs )

= η (1 − θ) β_k PAP L TsQE ( Z^2_l ) + C − QEs = η (1 − θ) β_kPAPTsQ χ (Lχ + 1) ϕ^2 + C − QEs. (31) To provide more useful insights, the asymptotic P^{k,po}_{11} (q) against P_{AP} is investigated.

Lemma 1: An asymptotic expression for P^{k,po}_{11} (q) at high P_{AP} values can be expressed as

P^{k,po}_{11} (q) = ∞∑ ς=0 s^{2ς} e^{− s2}2σ^2 (2σ^2)^ς ς!

. (32)

Proof: At high P_{AP} values, one can get^{L(qEs−C)}_{η(1−θ)βk PAPTs} → 0. Thus, in (23), the inner summation makes sense only for p = 0.

The inner summation becomes^{s2ς e−} s2 2σ2 (2σ^2 )^ς ς! .

Remark 4: Using the asymptotic P^{k,po}_{11} (q), the asymptotic power outage probability P^{k,po} can be obtained as P^{k,po} = 1− Q∏ q=1 ∞∑ ς=0 s^{2ς} e^{− s} 2 2σ2 (2σ^2 )^ς ς! . The diversity order of P k,po can be calculated

as lim

P_{AP} →∞

−^{log}(^{P k,po(PAP)})

log(P_{AP}) = 0, since P k,po is independent

with P_{AP}.

B. Downlink Information Outage Probability and Sum Throughput

The primary goal of energy collection is to provide the energy for exchanging information. When only part of the received power is available for information communication, it is crucial to assess the probability of communication outages. According to the principle of NOMA, the user with better channel conditions performs SIC decoding^6, while the other user decodes its signal directly [52]. In this paper, based on

6In this paper, perfect SIC is considered, which brings an upper bound for the information outage probability of the proposed system. Due to unavoidable error propagation and quantization error in practical hardware implementation, imperfect SIC is more realistic [53], [54]. Hence, simulation results are presented in Sect. V to investigate the impact of imperfect SIC on the system performance.

Fig. 4: The Markov chain model of information transmission states (T_0: Outage, and T_1: Successful transmission).

the path loss [52], [55], [56]^7, it is assumed that U_t experiences better channel conditions, and there is a fixed decoding order^8 (U_r, U_t) at U_t.

According to (1) and the decoding order (U_r, U_t), U_t first decodes the signal of U_r before decoding its own signal. The signal-to-interference plus noise ratio (SINR) at U_t is given by

γ^d_s = θβt | | | | L∑ ℓ=1 ( h^0_{t,ℓ} +^N ∑ i=1 h_{ℓ,i}gt,i )| | | 2 αr PAP θβt | | | | L∑ ℓ=1 ( h^0_{t,ℓ} +^N ∑ i=1 h_{ℓ,i}gt,i )| | | 2 αtPAP + LN0 . (33)

Then, U_t performs SIC to remove the interference from the signal of U_r and decodes its signal. The SNR at U_t can be expressed as

γ^d_t = θβt | | | | L∑ ℓ=1 ( h^0_{t,ℓ} +^N ∑ i=1 h_{ℓ,i}gt,i )| | | 2 αtPAP LN0 . (34)

Meanwhile, U_r treats the signal of U_t as interference and decodes its own signal directly. The SINR at U_r is obtained as

γ^d_r = θβr | | | L∑ ℓ=1 ( h^0_{r,ℓ} +^N ∑ i=1 h_{ℓ,i}gr,i )| | | 2 αr PAP θβr | | | L∑ ℓ=1 ( h^0_{r,ℓ} +^N ∑ i=1 h_{ℓ,i}gr,i )| | | 2 αtPAP + LN0 . (35)

Similar to the power outage analysis in section III-A, the information transmission states can also be modeled with a Markov chain, as illustrated in Fig. 4. The Markov chain can achieve a steady state, defined as { π^k_{0,d}P^{k,io}_{00,d} + π^k_{1,d}P^{k,io}_{10,d} = π^k_{0,d}, π^k_{0,d}P^{k,io}_{01,d} + π^k_{1,d}P^{k,io}_{11,d} = π^k_{1,d}, (36)

where π^k_{0,d} and π^k_{1,d} are the steady state probabilities for two states T_0 and T_1, π^k_{0,d} + π^k_{1,d} = 1, P^{k,io}_{00,d} + P^{k,io}_{01,d} = 1, and P^{k,io}_{10,d} + P^{k,io}_{11,d} = 1. Thus, one has

π^k_{0,d} =^P k,io 10,d P k,io 01,d +P k,io 10,d , π^k_{1,d} =^P k,io 01,d P k,io 01,d +P k,io 10,d . (37)

1) Downlink Information Outage Probability of U_r: The transition probability P^{r,io}_{10,d} denotes the outage probability of U_r, which is calculated as P^{r,io}_{10,d} = Pr ( γ^d_r < γ_{th} )

7In this paper, it is assumed that d_{S-R,Ut} < d_{S-R,Ur} . This causes more severe path loss for U_r compared to U_t. To ensure user fairness, more transmit power is allocated to U_r, i.e., α_r > α_t.

8In this paper, we can adopt other decoding orders, such as [57]. The simulation result is presented in Sect. V to show the impact of decoding order on information outage probability performance.

= Pr θβr | | |^L∑ ℓ=1 ( h^0_{r,ℓ} +^N ∑ i=1 h_{ℓ,i}gr,i )| | 2 αr PAP θβr | | |^L∑ ℓ=1 ( h^0_{r,ℓ} +^N ∑ i=1 h_{ℓ,i}gr,i )| | 2 αtPAP + LN0 < γ_{th}

= Pr ( Z^2_l < LN0γ_{th} θβr PAP (αr − αtγ_{th}) )

= 1 Γ (Lχ) γ ( Lχ, ϕ ( LN0γ_{th} θβr PAP (αr − αtγ_{th}) ) 1_2 )

, (38)

where γ_{th} = 2^R − 1 and R is the target rate. P^{r,io}_{01,d} = Pr ( γ^d_r ≥ γ_{th} ) = 1 − P^{r,io}_{10,d}. Hence, the steady-state probability π^r_{1,d} = P^{r,io}_{01,d} = 1 − P^{r,io}_{10,d}. After Q time slots, the overall information outage probability of U_r can be calculated as P^{r,io}_d = 1 − Q∏ q=1 π^r_{1,d} = 1 − ( π^r_{1,d} )_Q . (39)

2) Downlink Information Outage Probability of U_t: Similarly, the P^{t,io}_{10,d} of U_t can be expressed as

P^{t,io}_{10,d} = 1 − Pr ( γ^d_s > γ_{th}, γ^d_t > γ_{th} )

= 1 − Pr θβt | | | | | L∑ ℓ=1 ( h0t,ℓ+ N∑ i=1 hℓ,igt,i )| | | | 2 αr PAP

θβt | | | | L∑ ℓ=1 ( h0t,ℓ + N∑ i=1 hℓ,igt,i )| | | | 2 αtPAP+LN0 > γ_{th}, θβt | | | | | L∑ ℓ=1 ( h0t,ℓ + N∑ i=1 hℓ,igt,i )| | | | 2 αtPAP LN0 > γ_{th} = 1 − Pr ( Z^2_l >^{γth LN0} θβtPAP(αr −αt γth ) , Z^2_l >^{γth LN0} θβtαt PAP )

= 1 Γ (Lχ) γ ( Lχ, ϕ(γ̂_t)^{12} ) , (40)

where γ̂_t = max (_{γth LN0} θβ_tP_{AP}(α_r −α_tγ_{th} ) , γ_{th} LN_0 θβ_tα_t P_{AP} ) . The steady-

state probability π^t_{1,d} = 1−P^{t,io}_{10,d}. After Q time slots, the overall information outage probability of U_t can be calculated as P^{t,io}_d = 1 − Q∏ q=1 π^t_{1,d} = 1 − ( π^t_{1,d} )_Q . (41)

When β_k = 0, one has γ (Lχ, ∞) in both (38) and (40). Since

γ (m, x) = (m − 1)! ( 1 − e^{−x m−1} ∑ n=0 x^n n! ) , using lim_{x→∞} e^{−x}x =

0, γ (Lχ, ∞) = (Lχ − 1)!. Hence P^{r,io}_{10,d} = 1 and P^{t,io}_{10,d} = 1. To prevent the user from a complete information outage, β_k should be greater than zero.

Lemma 2: The asymptotic expressions for P^{r,io}_{10,d} and P^{t,io}_{10,d} at high P_{AP} values can be expressed as P^{r,io}_{10,d} = P^{t,io}_{10,d} = 0. (42) Proof: At high P_{AP} values, one can get^{LN0γth}

θβ_r P_{AP}(α_r −α_tγ_{th} ) →

0 and γ̂_t → 0. Since γ (Lχ, 0) = 0, (42) can be obtained.

The sum throughput of downlink transmission can be expressed as Ψ_d = RTs ( 1 − P^{r,io}_d ) + RTs ( 1 − P^{t,io}_d ) . (43)

C. Uplink Information Outage Probability and Sum Throughput Different from downlink transmission, the received signal strength of U_t may be higher due to the shorter distance from the AP, resulting in a decoding order (U_t, U_r) at the AP. According to (6), the SINR at the AP is given by γ^u_s = Ptβt | | |^L∑ ℓ=1 ( h^0_{t,ℓ} +^N ∑ i=1 h_{ℓ,i}gt,i )| | 2

Prβr | | |^L∑ ℓ=1 ( h^0_{r,ℓ} +^N ∑ i=1 h_{ℓ,i}gr,i )| | 2 + LN0 . (44)

After performing successful SIC, AP then decodes U_r. The received SNR for decoding U_r is given by

γ^u_r = Prβr | | | L∑ ℓ=1 ( h^0_{r,ℓ} +^N ∑ i=1 h_{ℓ,i}gr,i )| | | 2

LN0 . (45)

1) Uplink Information Outage Probability of U_t: Similar to (38), one has

P^{t,io}_{10,u} = Pr (γ^u_s < γ_{th}) ≈ 1 − Lχ−1∑

m=0 ϕ^{Lχ+m} 2m! (Lχ − 1)! W∑ w=1 ψw e^{−ϕ} ( Pr βr euw γth +LN0γth Pt βt ) 1 2

× ( Prβr e^{uw} γ_{th} +LN0γ_{th} Ptβt )m_2 e^{−ϕe} uw 2 e^{uw Lχ−22} e^{uw +u2w} −OW . (46) The detailed derivation of (46) is given in Appendix B.

2) Uplink Information Outage Probability of U_r: P^{r,io}_{10,u} = 1 − Pr (γ^u_s > γ_{th}, γ^u_r > γ_{th}) ≈ F_Z2_{l,r} (B) + F_Z2_{l,t} (A) + Lχ−1∑

m=0 ϕ^{Lχ+m} 2m! (Lχ − 1)! W∑ w=1 ψw

× e^{−ϕ} ( Pt βt(euw +A)−γth LN0 γth Pr βr ) 1 2 ( Ptβt (e^{uw} + A) − γ_{th}LN0 γ_{th}Prβr ) m_2

× e^{−ϕ(euw +A)} 1 2 (e^{uw} + A)^{Lχ−22} e^{uw +u2w} + OW , (47)

where A =^{γth LN0}_{Pt βt} and B =^{γth LN0}_{Pr βr} . The detailed derivation of (47) is given in Appendix B.

For both users, the overall information outage probability is given by P^{k,io}_u = 1 − Q∏ q=1 π^k_{1,u} = 1 − ( π^k_{1,u} )_Q , (48)

where π^k_{1,u} = 1 − P^{k,io}_{10,u}.

The sum throughput of uplink transmission can be expressed as Ψu = RTs ( 1 − P^{r,io}_u ) + RTs ( 1 − P^{t,io}_u ) . (49)

D. Joint Outage Probability

To combine the information outage probability and power outage probability^9, the downlink and uplink joint outage probabilities can be obtained. For U_k, the downlink and uplink joint outage probabilities are expressed as, respectively P^{k,d}_{out} = 1 − ( 1 − P^{k,po} ) ( 1 − P^{k,io}_d ) , (50)

P^{k,u}_{out} = 1 − ( 1 − P^{k,po} ) ( 1 − P^{k,io}_u ) . (51)

Both the downlink and uplink joint outage probabilities are associated with power outage probability. Hence, if a power outage occurs in the downlink joint outage probability, then the uplink joint outage probability occurs.

IV. RESOURCE ALLOCATION In this section, we propose a low-complexity power allocation scheme for solving the uplink sum throughput maximization problem with the uplink joint outage probability and JFI

9If there is a power outage, a delay occurs, which will be explored in the future.

constraint. According to (34) and (35), the downlink users’ achievable rate is given by R_k = log_2 ( 1 + γ^d_k ) . The JFI can be expressed as JF I =^{(Rt +Rr )2}_{2(R2t +R2r )} [58].

A. Problem Formulation

Our goal is to maximize the uplink sum throughput in the proposed system via jointly optimizing the energy-splitting ratios of the STAR-RIS and the transmit power allocation factors, subject to the uplink joint outage probability and JFI requirements of U_r and U_t. The uplink sum throughput optimization problem can be formulated as^{10} P1 : {β^∗_r , β^∗_t , α^∗_r , α^∗_t } = arg max_{βr ,βt,αr ,αt}Ψu (βr , βt, αr , αt) (52) s.t. C1 : 0 < βr , βt < 1, (52a) C2 : βr + βt = 1, (52b) C3 : P^{r,u}_{out} < P^{r,th}_{out} , (52c)

C4 : P^{t,u}_{out} < P^{t,th}_{out} , (52d) C5 : JF I > JF I^{th}, (52e) C6 : 0 < αr , αt < 1, (52f) C7 : αr + αt = 1. (52g)

Constraint (52a) ensures that the amplitude coefficients of transmission and reflection for the STAR-RIS are between 0 and 1. Constraint (52b) is given to meet the law of energy conservation. Constraint (52c) and constraint (52d) guarantee that the uplink joint outage probabilities at U_r and U_t are less than the present thresholds P^{r,th}_{out} and P^{t,th}_{out} , respectively. Constraint (52e) ensures that JFI is more than the preset threshold JF I^{th}. Constraint (52f) and constraint (52g) specify the range of α_r, α_t and their summation, respectively.

B. Proposed PSO-PA Algorithm

Since the sum throughput expression in (49) is intractable, we consider a derivative-free optimization method to obtain the optimal solution, which is practical without the computation of gradients [59]. It is difficult to solve the optimization problem using the exhaustive search method in an acceptable time with the increase in network scale. In this context, there are lowcomplexity optimization algorithms, such as genetic algorithm (GA) and particle swarm optimization (PSO), which have been shown to reach the global optimal solution [60]. Although the GA could work as effectively as PSO, PSO offers a superior computational cost and speed of convergence [60], [61]. Hence, PSO is considered to optimize the energy-splitting ratios β_r, β_t and the transmit power allocation factors α_r, α_t for maximizing the sum throughput.

The proposed PSO-PA method first initializes the particles’ positions and velocities. Here, there are four parameters for optimization. The particles’ position and velocity can be denoted as d^w_b = [ d^w_{b,1}, d^w_{b,2}, d^w_{b,3}, d^w_{b,4} ] and v^w_b = [ v^w_{b,1}, v^w_{b,2}, v^w_{b,3}, v^w_{b,4} ] , where b denotes the particle index and w denotes the iteration index. Let N_p denote the number of particles, and N_i denote the number of iterations. One has D^w = { d^w_1 , . . . , d^w_{Np} } . Each particle updates the velocity v^{w+1}_{b,ζ} based on its current position d^w_{b,ζ} , best record p̂^w_{b,ζ} and global best record ĝ^w_ζ , where

10Different from (49), we explicitly write Ψ_u as a function of variables β_r, β_t, α_r , and α_t, which are to be optimized.

ζ ∈ {1, 2, 3, 4}. Similarly, one has P̂^w = { p̂^w_1 , . . . , p̂^w_{Np} } and Ĝ = { ĝ^1, . . . , ĝ^{Ni} } . The iterative equation is expressed as v^{w+1}_{b,ζ} = ω̄v^w_{b,ζ} +C1r1 ( p̂^w_{b,ζ} − d^w_{b,ζ} ) +C2r2 ( ĝ^w_ζ − d^w_{b,ζ} ) , (53)

where ω̄ is an inertia weight, r_1 and r_2 are chosen independently and uniformly at random to increase the search randomness, and C_1 and C_2 are acceleration instants to control the direction of convergence of the PSO. For example, a larger value of C_1 tends to converge to a personal best solution, leading to a local optimal solution. Correspondingly, a larger value of C_2 tends to converge to the global optimum, where the particles tend to move further distances and increase their exploration of search space. Each particle updates the position based on its current position d^w_{b,ζ} , and the velocity v^{w+1}_{b,ζ} , as follows d^{w+1}_{b,ζ} = d^w_{b,ζ} + v^{w+1}_{b,ζ} . (54)

Each particle evaluates its penalty fitness function based on its positions at each iteration. The penalty fitness function is given as follows

P_f = Ψu −λ̄1 max ( 0, P^{r,u}_{out} −P^{r,th}_{out} ) −λ̄1 max ( 0, P^{t,u}_{out} −P^{t,th}_{out} )

+ λ̄2 min ( 0, JF I − JF I^{th} ) , (55)

where λ̄_1 and λ̄_2 denote the penalty factors for joint outage probability and JFI, respectively. The proposed PSO-PA scheme is presented in Algorithm 1.

Algorithm 1 Particle Swarm Optimization Based Power Allocation (PSO-PA) Input: Np, Ni, C1, and C2. Output: The optimal β^∗_r , β^∗_t , α^∗_r , α^∗_t .

1: Randomly initialize the particle positions d^1_b and velocities v^1_b , where b = 1, ..., Np. 2: Set P̂^1 = D^1 and ĝ^1 = arg max_{p̂1} b ∈P̂1 P_f .

3: for w = 1 : N_i do 4: for b = 1 : N_p do 5: Calculate particle velocity v^{w+1}_b via (53). 6: Update particle position d^{w+1}_b via (54). 7: if P_f ( d^{w+1}_b ) > P_f (p̂^w_b ) 8: then p̂^{w+1}_b = d^{w+1}_b . 9: else p̂^{w+1}_b = p̂^w_b . 10: end if 11: end for 12: Set ĝ^{w+1} = arg max

p̂w+1 b ∈P̂w+1 P_f .

13: end for 14: (ĝ^w )^∗ = arg max_{ĝw ∈Ĝ} P_f .

The time complexity of PSO-PA can be calculated as follows. In PSO-PA, given the N_p and N_i, the time complexity for initializing the particles’ positions and velocities can be expressed as O (N_p). The time complexity for searching for the global best record is given by O (N_i × N_p). Hence, the overall time complexity is approximated as O (N_i × N_p) + O (N_p) ≈ O (N_i × N_p).

V. RESULTS AND DISCUSSION In this section, power outage probability, information outage probability, sum throughput, and joint outage probability of the proposed system over Nakagami-m fading channels are evaluated. The main simulation parameters are listed in Table I; the other parameters are specified in figure caption. We consider a two-dimensional Cartesian coordinate location

TABLE I: SYSTEM PARAMETERS

The transmit power at the AP P_{AP} = 1 Watt (W) The Nakagami-m fading

channel parameters m_{0,k} = m_{i,ℓ} = m_{k,i} = 2 The symbol duration

T_s = (1/256000) s [46] The energy conversion

efficiency factor η = 0.9

The initial state of the battery C = 1 μJ The number of time slots Q = 5 The path-loss at a reference

distance of 1 meter τ = −2 dB

The path-loss exponent ϑ = 2 The number of antennas L = 2

setup as follow. The AP is located at the origin (0, 0), and the STAR-RIS is located at (16, 0). The location of U_t is (16, 2), and that of U_r is (16, −3). We assume that the inter-distance between the adjacent elements of STAR-RIS is half-wavelength. Accordingly, reflecting/transmitting channels through the adjacent elements are regarded as independent channels [26]. To verify the effectiveness of the proposed system, the following benchmarks are considered for comparison: i) conventional RIS case. More specifically, we deploy the transmitting-only RIS and the reflecting-only RIS at the same location as the STAR- RIS for full-space coverage, where each reflecting/transmittingonly RIS is equipped with^N_2 elements for fairness comparison [26]; ii) TDMA case. More specifically, the STAR- RIS adopts the time-switching protocol; iii) buffer-less case; iv) discrete phase-shift case. Because of hardware limitations, discrete phase-shift adjustment is practical and realistic for STAR-RIS [62], [63]. Specifically, discrete phase-shift values are obtained by uniformly quantizing the feasible region [62], i.e., φ^r_i , φ^t_i ∈ ℑ = { 0,^{2π}_{2e} , . . . ,^{2π(2e −1)}_{2e} } , where e denotes the number of quantization bits and is set to 4 in this paper. Hence, baseline schemes include the proposed system with discrete phase shifts (referred to as discrete phase), the STAR-RIS aided MISO SWIPT-NOMA buffer-less system (referred to as STAR-RIS-BL-NOMA), the RIS and energy buffer aided MISO SWIPT-NOMA system (referred to as RIS-EB-NOMA), and the STAR-RIS and energy buffer aided MISO SWIPT-TDMA system (referred to as STAR-RIS-EB-TDMA). It is noted that the proposed system and STAR-RIS-BL-NOMA have the same information transmission scheme, i.e., STAR-RIS aided NOMA. Hence, we only consider the proposed system, RIS- EB-NOMA, and the STAR-RIS-EB-TDMA when comparing the performance of the information outage probability and sum throughput.

Fig. 5 shows the power outage probability versus powersplitting factor θ of various systems, where N = 18, β_r = 0.65, and β_t = 0.35. It can be observed that the simulated curves well match with the theoretical ones, which verifies the correctness of the proposed analytical method. Moreover, it is observed that larger values of θ lead to higher power outage probabilities due to less power being allocated to energy collection. Furthermore, it is seen that the proposed system provides improved power outage probability performance compared to the STAR-RIS-

Fig. 5: Power outage probability versus power splitting factor θ of various systems, where N = 18, β_r = 0.65, and β_t = 0.35.

Fig. 6: Power outage probability versus the initial energy C for the proposed system with various values of N, where β_r = 0.65, β_t = 0.35, and θ = 0.5.

BL-NOMA, RIS-EB-NOMA, and STAR-RIS-EB-TDMA. For example, when θ = 0.3, the power outage probability of the proposed system at U_r is approximately 80% lower than that of the STAR-RIS-BL-NOMA. It is also seen that the proposed system yields an improved performance compared to the RIS-EB- NOMA. This is because the STAR-RIS can be configured for full-space electromagnetic propagation environments, whereas the conventional RIS requires both the transmitting-only RIS and the reflecting-only RIS to provide full-space coverage. It is shown that the proposed system outperforms the STAR-RIS- EB-TDMA. The reason is that U_r and U_t can utilize the same block of time-frequency resources in NOMA, thus achieving a multiplexing gain compared with the TDMA.

Fig. 6 illustrates the power outage probability versus the initial energy C for the proposed system with various values of N, where β_r = 0.65, β_t = 0.35, and θ = 0.5. It is observed that the increase in the number of STAR-RIS elements significantly improves the power outage probability performance^{11}. For example, when C = 15 mJ, the outage probability at U_r for N = 18 is approximately 85% lower than

11When the number of reflective elements becomes large, the circuit power consumption of STAR-RIS grows accordingly [64]. The study of minimizing reflective elements while meeting system performance constraints will be left for future work.

Fig. 7: Power outage probability versus power splitting factor θ of different energy levels, where N = 18, β_r = 0.65, and β_t = 0.35.

Fig. 8: Downlink information outage probability versus the transmit SNR of various systems, where N = 18, θ = 0.5, β_r = 0.6, β_t = 0.4, α_r = 0.6, α_t = 0.4, and R = 1.

that of N = 17 while the outage probability at U_r for N = 17 is approximately 60% lower than that case where N = 16. It is also observed that an increase in C yields a better power outage probability performance, especially when N is larger. For example, when N = 18, an increase in C from 20 to 25 reduces the outage probability of U_t from 10^{−3} to 10^{−4}.

Fig. 7 plots the power outage probability versus power splitting factor θ of different energy levels, where N = 18, β_r = 0.65, and β_t = 0.35. For the benchmark schemes, the energy buffer is discretized into 3 and 4 possible energy levels, respectively. It is observed that the benchmark schemes perform worse than the proposed system. The reason behind this is that the energy level of the energy buffer is rounded down to the closest discrete level [49], which causes a partial loss of energy. Moreover, it is seen that the performance of 4 energy levels is better than that of 3 energy levels due to the larger buffer capacity. Hence, unlike [48] which performs a residual energy-aware model to extend the lifetime of the node and [49] which schedules nodes to reduce packet loss based on their energy levels and data queue lengths, a two-state Markov chain is suitable for modeling power outage and achieving better performance.

Fig. 9: Downlink sum throughput versus transmit SNR of various systems, where N = 18, θ = 0.5, β_r = 0.65, β_t = 0.35, α_r = 0.95, α_t = 0.05, and R = 1.5.

Fig. 8 depicts the downlink information outage probability versus the transmit SNR of various systems, where N = 18, θ = 0.5, β_r = 0.6, β_t = 0.4, α_r = 0.6, α_t = 0.4, and R = 1. It can be seen that the STAR-RIS-EB-TDMA outperforms the proposed system in information outage probability. The reason is that there is no inter-user interference with STAR-RIS-EB- TDMA. Moreover, it can be seen that the proposed system outperforms the RIS-EB-NOMA. For example, for a target information outage probability of 10^{−3}, the proposed system shows a gain of 3.5 dB compared to RIS-EB-NOMA for U_r.

Fig. 9 shows the downlink sum throughput versus transmit SNR of various systems, where N = 18, θ = 0.5, β_r = 0.65, β_t = 0.35, α_r = 0.95, α_t = 0.05, and R = 1.5. It is observed that the proposed system can provide an improved sum throughput performance compared with baseline schemes. This is because compared to TDMA, the U_r and U_t can utilize the same block of time-frequency resources in NOMA to obtain a multiplexing gain. Moreover, in NOMA, the STAR-RIS adopts the energy-splitting protocol and exploit the proper energysplitting ratios to obtain an enhanced performance. At low SNR, the performance of the proposed system is slightly worse than that of STAR-RIS-EB-TDMA. The reason behind this is that the poor information outage performance of the proposed system at low SNR affects the sum throughput performance. Moreover, it is observed that an intersection exists between the curves of RIS-EB-NOMA and STAR-RIS-EB-TDMA. The reason lies that the beamforming gain of the STAR-RIS takes the lead and the multiplexing gain is not obvious at low SNR, whereas the multiplexing gain enhances and ultimately surpasses the beamforming gain as a leading factor at high SNR.

Fig. 10 illustrates the uplink information outage probability versus the transmit SNR of various systems, where N = 18, β_r = 0.6, β_t = 0.4, and R = 0.1. Similar to the downlink information outage probability, the uplink information outage performance of the STAR-RIS-EB-TDMA is better than that of the proposed system, while the proposed system outperforms the RIS-EB-NOMA. Fig. 11 depicts the uplink sum throughput versus transmit SNR of various systems, where N = 18, β_r = 0.3, β_t = 0.7, and R = 0.5. It can be observed

Fig. 10: Uplink information outage probability versus the transmit SNR of various systems, where N = 18, β_r = 0.6, β_t = 0.4, and R = 0.1.

Fig. 11: Uplink sum throughput versus transmit SNR of various systems, where N = 18, β_r = 0.3, β_t = 0.7, and R = 0.5.

Fig. 12: Downlink information outage probability versus the transmit SNR of various decoding orders, where N = 18, θ = 0.5, β_r = 0.6, β_t = 0.4, α_r = 0.6, α_t = 0.4, and R = 1.

Fig. 13: Downlink information outage probability versus the transmit SNR of imperfect SIC and imperfect CSI, where N = 18, θ = 0.5, β_r = 0.6, β_t = 0.4, α_r = 0.6, α_t = 0.4, and R = 1.

that NOMA schemes have better sum throughput performance compared to the TDMA scheme due to the multiplexing gain, and the proposed system provides superior performance over RIS-EB-NOMA.

Fig. 12 shows the downlink information outage probability versus the transmit SNR of various decoding orders, where N = 18, θ = 0.5, β_r = 0.6, β_t = 0.4, α_r = 0.6, α_t = 0.4, and R = 1. For the case of two users, four decoding orders are considered according to [57]. In the decoding order (i, j) of the legend, i denotes that U_i’s data will be decoded first by U_t, and j denotes that U_j ’s data will be decoded first by U_r, where i, j ∈ {t, r}. For example, the decoding order (r, r) means that U_t firstly decodes the signal of U_r, and U_r directly decodes the signal of U_r. It can be seen that for the decoding order (r, t), U_r firstly decodes the signal of U_t, resulting in constant outage. The reason is that due to the transmit power allocation α_r > α_t, if U_r firstly decodes the signal of U_t by treating the signal of U_r as interference, the decoding performance of U_r will become worse. It is also seen that for the decoding order (t, r), U_t cannot decode the signal of U_t first by treating the signal of U_r as interference. Hence, the decoding order (r, r) is the optimal decoding order.

Fig. 13 depicts the downlink information outage probability versus the transmit SNR of imperfect SIC and imperfect CSI, where N = 18, θ = 0.5, β_r = 0.6, β_t = 0.4, α_r = 0.6, α_t = 0.4, and R = 1. For imperfect SIC, there will be residual interference after performing the SIC. Thus, U_t cannot completely remove the interference from the signal of U_r. The SNR in (34) at U_t can be re-expressed as

γ^d_t = θβt | | | | L∑ ℓ=1 ( h^0_{t,ℓ} +^N ∑ i=1 h_{ℓ,i}gt,i )| | | 2 αtPAP εθβt | | | | L∑ ℓ=1 ( h^0_{t,ℓ} +^N ∑ i=1 h_{ℓ,i}gt,i )| | | 2 αr PAP + LN0 , (56)

where ε ∈ [0, 1] denotes the portion of residual interference. It is seen that the performance of U_t decreases due to the residual interference, and that of U_r is unchanged since no SIC is performed. This result is consistent with that from Fig. 13. For imperfect CSI, the complex channel coefficients are represented as ĥ^0_{k,ℓ} = h̃^0_{k,ℓ} + h̄^0_{k,ℓ}, ĥ_{ℓ,i} = h̃_{ℓ,i} + h̄_{ℓ,i}, and ĝ_{k,i} = g̃_{k,i} + ḡ_{k,i}, where h̃^0_{k,ℓ}, h̃_{ℓ,i}, g̃_{k,i} are the estimated channel coefficients, and

Fig. 14: Downlink joint outage probability versus power splitting factor θ of various systems, where N = 18, P_{AP}/N_0 = 25 dB, β_r = 0.6, β_t = 0.4, α_r = 0.7, and α_t = 0.3.

Fig. 15: Downlink joint outage probability versus powersplitting factor θ of the proposed system for various values of Q, where N = 17, P_{AP}/N_0 = 24 dB, β_r = 0.6, β_t = 0.4, α_r = 0.7, and α_t = 0.3.

h̄0_{k,ℓ}, h̄_{ℓ,i}, ḡ_{k,i} are the estimation errors [65], [66]. Hence, (1) can be re-expressed as

y_k = √ θβ_k L∑ ℓ=1 ( h̃^0_{k,ℓ} + h̄^0_{k,ℓ} ) e^{−jϖℓ} +^N ∑ i=1 ( h̃_{ℓ,i} + h̄_{ℓ,i} ) × ( g̃_{k,i} + ḡ_{k,i} ) e^j(^{φki −ϖℓ}) s + n_k

= √ θβ_k L∑ ℓ=1 ( h̃^0_{k,ℓ}e^{−jϖ}ℓ +^N ∑ i=1 h̃_{ℓ,i}g̃_{k,i}e^j(^{φk}i^{−ϖ}ℓ) ) s + √ θβ_kn̄_k + n_k , (57)

where

n̄_k = L∑ ℓ=1 ( h̄^0_{k,ℓ}e^{−jϖ}ℓ +^N ∑ i=1 (~ h_{ℓ,i}ḡ_{k,i} +h̄_{ℓ,i}g̃_{k,i} + h̄_{ℓ,i}ḡ_{k,i} ) e^j(^{φki −ϖℓ}) ) s (58)

is the error due to imperfect CSI. Since n̄_k is the sum of a large number of random variables, it can be approximated as a Gaussian-distributed random variable with variance N_0 by using the central limit theorem (CLT) [65]. Thus, there will be one interference term Lθβ_kN_0 in (33), (34), and (35). It is observed that different from the case of imperfect SIC, the performance of all users deteriorates due to the imperfect CSI. This result is also consistent with that from Fig. 13.

Fig. 14 plots the downlink joint outage probability versus

Fig. 16: Uplink joint outage probability versus power splitting factor θ of various systems, where N = 18, P_{AP}/N_0 = 24 dB, β_r = 0.65, and β_t = 0.35.

power splitting factor θ of various systems, where N = 18, P_{AP}/N_0 = 25 dB, β_r = 0.6, β_t = 0.4, α_r = 0.7, and α_t = 0.3. It is noticed that an optimal value of θ exists, which balances the power and information outage probabilities to minimize the joint outage probability. It is observed that the proposed system can obtain better joint outage probability performance compared with the baseline schemes. For example, when θ = 0.3, the joint outage probability of the proposed system at U_t is 10^{−3} while that of the STAR-RIS-BL-NOMA is 10^{−2}. It is also noticed that the optimal value of θ for U_t is larger than that for U_r. This is because U_t is a close user, which experiences better channel conditions than U_r and can allocate more power for information decoding. Moreover, the STAR-RIS-EB-TDMA slightly outperforms the proposed system for small values of θ. This is because the STAR-RIS- EB-TDMA has a better information outage probability than the proposed system. When θ is small, the poor information outage probability of the proposed system damages the joint outage probability performance. However, with the increase of θ and the improvement in the information outage probability performance, the proposed system is superior to the STAR- RIS-EB-TDMA scheme. There is a small performance gap between the proposed system with continuous phase shifts and the proposed system with discrete phase shifts. Hence, 4-bit quantization of discrete phase yields nearly the same performance as continuous phase shifts and phase errors can be neglected [67], which offers more insights into the practical deployment of the proposed system.

Fig. 15 shows the downlink joint outage probability versus power splitting factor θ of the proposed system for various values of Q, where N = 17, P_{AP}/N_0 = 24 dB, β_r = 0.6, β_t = 0.4, α_r = 0.7, and α_t = 0.3. It is observed that the joint outage probability performance decreases with the increase of Q. This is because as the number of continuous-time slots Q increases, both information outage and power outage increase. Moreover, it is observed that as Q increases, the performance degradation becomes smaller. For example, the gap between the curves of Q = 10 and Q = 15 is relatively small.

Fig. 16 depicts the uplink joint outage probability versus power splitting factor θ of various systems, where N = 18,

Fig. 17: Optimized uplink sum throughput versus the number of iterations, where P_{AP}/N_0 = 30 dB, θ = 0.1, R = 0.5, and JF I^{th} = 0.8.

Fig. 18: Optimized uplink sum throughput versus transmit SNR of the proposed system with various values of N, where θ = 0.1, R = 0.5, and JF I^{th} = 0.8.

P_{AP}/N_0 = 24 dB, β_r = 0.65, and β_t = 0.35. It can be observed that the performance of uplink joint outage probability deteriorates as θ increases, which is different from the downlink joint outage probability. The reason is that larger values of θ lead to higher power outage probability, while uplink information outage probability is independent of θ. It is seen that the proposed system achieves better performance than STAR-RIS- BL-NOMA. Since energy buffer is not considered for the STAR- RIS-BL-NOMA, it causes uplink information outage due to lack of energy, thus deteriorating the performance of uplink joint outage probability. The 4-bit quantization of discrete phase yields nearly the same performance as the proposed system in the uplink joint outage probability.

Fig. 17 shows the optimized uplink sum throughput versus the number of iterations, where P_{AP}/N_0 = 30 dB, θ = 0.1, R = 0.5, and JF I^{th} = 0.8. As can be seen in Fig. 17, the curves stabilize quickly with only a few iterations. When N goes large, convergence becomes faster, because it is easier to satisfy the constraints. This indicates that PSO-PA is an effective method that can converge faster to obtain a solution. Fig. 18 plots the optimized uplink sum throughput versus transmit SNR of the proposed system with various values of N, where θ = 0.1, R = 0.5, and JF I^{th} = 0.8. It is observed that the proposed PSO-

PA method can improve the sum throughput performance of the proposed system. For example, for a target sum throughput of 0.6 bits/s/Hz, the proposed system with the PSO-PA method and N = 19 can obtain a 1 dB gain compared with the proposed system without PSO-PA. As the transmit SNR increases, the PSO-PA method can optimize the uplink sum throughput and meet the uplink joint outage probability and JFI requirements by adjusting the transmit power allocation factors and the STAR- RIS’s energy-splitting ratios. VI. CONCLUSION In this paper, we have investigated a STAR-RIS and energy buffer aided MISO SWIPT-NOMA system, in which the power transfer and information transmission states are modeled using Markov chains. Moreover, the power outage probability, information outage probability, and sum throughput expressions for the proposed system were derived in closed-form over Nakagami-m fading channels. From the perspective of power and information outage, the downlink and uplink joint outage probabilities were analyzed to investigate the overall network performance. Both theoretical analysis and simulations showed that the proposed system yields an improved performance compared to the selected baseline schemes. Furthermore, the PSO-PA algorithm was designed to maximize the uplink sum throughput with a constraint on the uplink joint outage probability and JFI. Results showed that the proposed PSO-PA method significantly improves the uplink sum throughput performance of the proposed system. Thanks to the aforementioned advantages, the proposed system could offer a promising candidate for large-scale, low-power, and sustainable IoT applications. APPENDIX A Here, (23) is derived. The Bessel function of the first kind

can be expanded as I^q_{2 −1} (_s σ^2 √ x ) =^∞ ∑ ς=0 (^s_{2σ2}^√x)^{q2 −1+2ς} ς!Γ(^q_2 +ς) .

Thus, (23) can be expressed as P^k_{11} (q) = ∫_∞ L(qEs −C) η(1−θ)βk PAP Ts fT (x)dx

= ∫_∞ L(qEs−C) η(1−θ)βk PAP Ts 1 2σ^2 ( x s^2 ) q−2_4 e^{− s} 2 +x

2σ2 I q_{2 −1} ( s σ^2 √ x ) dx

= ∞∑ ς=0 e^{− s} 2 2σ2 s^{2ς} (2σ^2)^{q2 +2ς} ς!Γ (_q 2 + ς ) ∫_∞ L(qEs−C) η(1−θ)βk PAP Ts e^{− x}2σ^2 x^{q2 −1+ς} dx. (59)

From (3.351.2) in [68], one has ∞∫ ū x^{ω′} e^{−μ̄x}dx = e^{−ūμ̄} ω′∑ ℓ̄=0

ω^′! ℓ̄! ū^{ℓ̄} μ̄^{ω′−ℓ̄+1} . (60)

Using (60), (59) can be calculated as

P^k_{11} (q) = ∞∑ ς=0 e^{− s2}2σ^2 s^{2ς} (2σ^2)^{q2 +2ς} ς!Γ (_q 2 + ς ) e^− L(qEs −C) 2σ2 η(1−θ)βk PAP Ts

× q 2 −1+ς∑

p=0 (_q 2 − 1 + ς ) ! (_{L(qEs−C)} η(1−θ)βk PAPTs )_p p! (_1 2σ2 ) q_{2 +ς−p}

= ∞∑ ς=0

q 2 −1+ς ∑ p=0 s^{2ς} e^{− s2}2σ^2 (2σ^2)^{ς+p}ς! e^− L(qEs −C) 2σ2 η(1−θ)βk PAP Ts (_{L(qEs−C)} η(1−θ)βk PAPTs )_p p! . (61)

APPENDIX B Here, (46) is derived.

P^{t,io}_{10,u} = Pr (γ^u_s < γ_{th})

= Pr | | | L∑ ℓ=1 ( h^0_{t,ℓ} +^N ∑ i=1 h_{ℓ,i}gt,i )| | | 2 < Pr βr | | | | | L∑ ℓ=1 ( h0r,ℓ+ N∑ i=1 hℓ,igr,i )| | | | 2 γth +LN0 γth Pt βt = Pr ( Z^2_{l,t} < Prβr Z^2_{l,r} γ_{th} + LN0γ_{th} Ptβt ) . (62)

From (26) and (27), one has P^{t,io}_{10,u} = F_Z2_{l,t} ( Pr βr Z^2_{l,r} γ_{th} + LN0 γ_{th} Ptβt )

= ∞∫ 0 F_Z2_{l,t} ( Prβr xγ_{th} + LN0 γ_{th} Ptβt ) f_Z2_{l,r} (x) dx

= 1 − Lχ−1∑

m=0 ϕ^{Lχ+m} 2m! (Lχ − 1)! ∞∫ 0 e^{−ϕ} ( P r βr xγth +LN0γth Pt βt ) 1 2

× ( Pr βr xγ_{th} + LN0γ_{th} Ptβt ) m_2 e^{−ϕx} 1 2 x^{Lχ−22} dx. (63)

Equation (63) can be evaluated by leveraging the Gauss- Hermite quadrature approach. According to Table (25.10) in

[69], one has ∫_∞ −∞ g (x)dx =^W ∑ w=1 ψ_wg (x_w) exp ( x^2_w ) + O_W ,

where W denotes the number of sample points used for approximation, x_w is the w-th root of the Hermite polynomial H_W (x) (w = 1, 2, . . . W ), ψ_w is the w-th associated weight obtained from^{2W −1W !√π}

W^2 H^2_{W −1}(x_w ) and OW is the residual term that

tends to 0 when W tends to infinity.

Using variable substitution ln(x) = u to obtain the new limits with integral from −∞ to +∞ and after some mathematical operations, one obtains P^{t,io}_{10,u} ≈ 1− Lχ−1∑

m=0 ϕ^{Lχ+m} 2m! (Lχ − 1)! W∑ w=1 ψw e^{−ϕ} ( Pr βr euw γth+LN0γth Pt βt )1 2

× ( Prβr e^{uw} γ_{th} +LN0γ_{th} Ptβt )m_2 e^{−ϕe} uw 2 e^{uw Lχ−22} e^{uw +u2w} −OW . (64) Moreover, (47) is derived as: P^{r,io}_{10,u} = 1 − Pr (γ^u_s > γ_{th}, γ^u_r > γ_{th}) = 1 − Pr ( γ_{th}LN0 Pr βr < Z^2_{l,r} < PtβtZ^2_{l,t} − γ_{th}LN0 γ_{th}Prβr )

= 1 − F_Z2_{l,r} ( PtβtZ^2_{l,t} − γ_{th}LN0 γ_{th}Pr βr ) + F_Z2_{l,r} (B) , (65) where B =^{γth LN0}_{Pr βr} . Similar to (64), one has F_Z2_{l,r} ( PtβtZ^2_{l,t} − γ_{th}LN0 γ_{th}Pr βr )

= ∞∫ A F_Z2_{l,r} ( Ptβtx − γ_{th}LN0 γ_{th}Pr βr ) f_Z2_{l,t} (x) dx

= 1−F_Z2_{l,t} (A)− Lχ−1∑

m=0 ϕ^{Lχ+m} 2m! (Lχ − 1)! ∞∫ A e^{−ϕ} ( P t βt x−γthLN0 γth Pr βr ) 1 2

× ( Ptβtx − γ_{th}LN0 γ_{th}Prβr ) m_2 e^{−ϕx} 1 2 x^{Lχ−22} dx

≈ 1 − F_Z2_{l,t} (A) − Lχ−1∑

m=0 ϕ^{Lχ+m} 2m! (Lχ − 1)! W∑ w=1 ψw

×e^{−ϕ} ( Pt βt(euw +A)−γth LN0 γth Pr βr ) 1 2( Ptβt (e^{uw} + A) − γ_{th}LN0 γ_{th}Pr βr ) m_2

× e^{−ϕ(euw +A)} 1 2 (e^{uw} + A)^{Lχ−22} e^{uw+u2w} − OW , (66)

where A =^{γthLN0}_{Pt βt} . By combining (65) and (66), (47) is obtained.

REFERENCES

[1] T. Malik et al., “RL-IoT: Reinforcement learning-based routing approach for cognitive radio-enabled IoT communications,” IEEE Internet Things J., vol. 10, no. 2, pp. 1836–1847, Jan. 2023.

[2] L. Chai, L. Bai, T. Bai, J. Choi, and W. Zhang, “RIS-aided SCMA-based SWIPT systems: Design and optimization,” IEEE Trans. Veh. Technol., vol. 72, no. 5, pp. 6238–6252, May 2023.

[3] K. Choi et al., “Toward realization of long-range wireless-powered sensor networks,” IEEE Wireless Commun., vol. 26, no. 4, pp. 184–192, Aug. 2019.

[4] R. Zhang et al., “Energy efficiency maximization in RIS-assisted SWIPT networks with RSMA: A PPO-based approach,” IEEE J. Sel. Areas Commun., vol. 41, no. 5, pp. 1413–1430, May 2023.

[5] L. Dai et al., “Non-orthogonal multiple access for 5G: Solutions, challenges, opportunities, and future research trends,” IEEE Commun. Mag., vol. 53, no. 9, pp. 74–81, Sept. 2015.

[6] S. Islam et al., “Power-domain non-orthogonal multiple access (NOMA) in 5G systems: Potentials and challenges,” IEEE Commun. Surv. & Tut., vol. 19, no. 2, pp. 721–742, Oct. 2017.

[7] M. Hedayati and Il-Min Kim, “CoMP-NOMA in the SWIPT networks,” IEEE Trans. Wireless Commun., vol. 19, no. 7, pp. 4549–4562, Jul. 2020.

[8] T. Nguyen, V. Nguyen, D. Costa, and B. An, “Hybrid user pairing for spectral and energy efficiencies in multiuser MISO-NOMA networks with SWIPT,” IEEE Trans. Commun., vol. 68, no. 8, pp. 4874–4890, Aug. 2020.

[9] L. Dai et al., “Hybrid precoding-based millimeter-wave massive MIMO- NOMA with simultaneous wireless information and power transfer,” IEEE J. Sel. Areas Commun., vol. 37, no. 1, pp. 131–141, Jan. 2019.

[10] X. Lan, Y. Zhang, Q. Chen, and L. Cai, “Energy efficient bufferaided transmission scheme in wireless powered cooperative NOMA relay network,” IEEE Trans. Commun., vol. 68, no. 3, pp. 1432–1447, Mar. 2020.

[11] D. Bapatla et al., “Adaptive multiuser cooperative NOMA scheme with energy buffer-aided near-users for high spectral and energy efficiency,” IEEE Internet Things J., vol. 9, no. 17, pp. 16643–16662, Sept. 2022.

[12] J. Ren et al., “NOMA for wireless-powered communication networks with buffered sources,” IEEE Trans. Veh. Technol., vol. 70, no. 9, pp. 9088–9102, Sept. 2021.

[13] J. He, H. Wymeersch, and M. Juntti, “Channel estimation for RIS-aided mmWave MIMO systems via atomic norm minimization,” IEEE Trans. Wireless Commun., vol. 20, no. 9, pp. 5786–5797, Sept. 2021.

[14] A. Ranjha, and G. Kaddoum, “URLLC facilitated by mobile UAV relay and RIS: A joint design of passive beamforming, blocklength, and UAV positioning,” IEEE Internet Things J., vol. 8, no. 6, pp. 4618–4627, Mar. 2021.

[15] D. Ng and R. Schober, “Secure and green SWIPT in distributed antenna networks with limited backhaul capacity,” IEEE Trans. Wireless Commun., vol. 14, no. 9, pp. 5082–5097, Sept. 2015.

[16] R. Ma et al., “Energy efficiency optimization for mutual-coupling-aware wireless communication system based on RIS-enhanced SWIPT,” IEEE Internet Things J., vol. 10, no. 22, pp. 19399–19414, Nov. 2023.

[17] Q. Wu and R. Zhang, “Weighted sum power maximization for intelligent reflecting surface aided SWIPT,” IEEE Wireless Commun. Lett., vol. 9, no. 5, pp. 586–590, May 2020.

[18] J. Ren et al., “RIS-assisted cooperative NOMA with SWIPT,” IEEE Wireless Commun. Lett., vol. 12, no. 3, pp. 446–450, Mar. 2023.

[19] Q. Liu et al., “Joint beamforming and power splitting optimization for RIS-assited cooperative SWIPT NOMA system,” in Proc. 2022 IEEE Wireless Commun. Netw. Conf., Austin, TX, USA, pp. 351–356, Apr. 2022.

[20] G. Zhang, Y. Lu, Y. Lin, Z. Zhong, Z. Ding, and D. Niyato, “AoI minimization in RIS-aided SWIPT systems,” IEEE Trans. Veh. Technol., vol. 73, no. 2, pp. 2895-2900, Feb. 2024.

[21] Q. Zhai, L. Dong, C. Liu, Y. Li, and W. Cheng, “Resource management for active RIS aided multi-cluster SWIPT cooperative NOMA networks,” IEEE Trans. Netw. Serv. Manage., early access, doi: 10.1109/TNSM.2024.3395298.

[22] Y. Xu, B. Gu, Z. Gao, D. Li, Q. Wu, and C. Yuen, “Applying RIS in multi-user SWIPT-WPCN systems: A robust and environmentally-friendly design,” IEEE Trans. Cognit. Commun. Netw., vol. 10, no. 1, pp. 209-222, Feb. 2024.

[23] Z. Yang, L. Xia, J. Cui, Z. Dong, and Z. Ding, “Delay and energy minimization for cooperative NOMA-MEC networks with SWIPT aided by RIS,” IEEE Trans. Veh. Technol., vol. 73, no. 4, pp. 5321-5334, Apr. 2024.

[24] G. Zhang, X. Gu, W. Duan, M. Wen, J. Choi, F. Gao, and P. Ho, “Hybrid time-switching and power-splitting EH relaying for RIS-NOMA downlink,” IEEE Trans. Cogn. Commun. Netw., vol. 9, no. 1, pp. 146–158, Feb. 2023.

[25] Y. Liu, X. Mu, J. Xu, R. Schober, Y. Hao, H. Poor, and L. Hanzo, “STAR:

Simultaneous transmission and reflection for 360^o coverage by intelligent surfaces,” IEEE Wireless Commun., vol. 28, no. 6, pp. 102–109, Dec. 2021.

[26] Z. Zhang, J. Chen, Y. Liu, Q. Wu, B. He, and L. Yang, “On the secrecy design of STAR-RIS assisted uplink NOMA networks,” IEEE Trans. Wireless Commun., vol. 21, no. 12, pp. 11207–11221, Dec. 2022.

[27] X. Mu, Y. Liu, L. Guo, J. Lin, and R. Schober, “Simultaneously transmitting and reflecting (STAR) RIS aided wireless communications,” IEEE Trans. Wireless Commun., vol. 21, no. 5, pp. 3083–3098, May 2022.

[28] Z. Xie et al., “STAR-RIS aided NOMA in multicell networks: A general analytical framework with Gamma distributed channel modeling,” IEEE Trans. Commun., vol. 70, no. 8, pp. 5629–5644, Aug. 2022.

[29] C. Wu, X. Mu, Y. Liu, X. Gu, and X. Wang, “Resource allocation in STAR-RIS-aided networks: OMA and NOMA,” IEEE Trans. Wireless Commun., vol. 21, no. 9, pp. 7653–7667, Sept. 2022.

[30] J. Zuo et al., “Joint design for simultaneously transmitting and reflecting (STAR) RIS assisted NOMA systems,” IEEE Trans. Wireless Commun., vol. 22, no. 1, pp. 611–626, Jan. 2023.

[31] Y. Guo, F. Fang, D. Cai, and Z. Ding, “Energy-efficient design for a NOMA assisted STAR-RIS network with deep reinforcement learning,” IEEE Trans. Veh. Technol., vol. 72, no. 4, pp. 5424–5428, Apr. 2023.

[32] F. Fang et al., “Energy-efficient design of STAR-RIS aided MIMO-NOMA networks,” IEEE Trans. Commun., vol. 71, no. 1, pp. 498–511, Jan. 2023.

[33] X. Qin, Z. Song, T. Hou, W. Yu, J. Wang, and X. Sun, “Joint resource allocation and configuration design for STAR-RIS-enhanced wireless-powered MEC,” IEEE Trans. Commun., vol. 71, no. 4, pp. 2381–2395, Apr. 2023.

[34] W. Du et al., “STAR-RIS assisted wireless powered IoT networks,” IEEE Trans. Veh. Technol., vol. 72, no. 8, pp. 10644–10658, Aug. 2023.

[35] K. Xie, G. Cai, G. Kaddoum, and J. He, “Performance analysis and resource allocation of STAR-RIS aided wireless-powered NOMA system,” IEEE Trans. Commun., vol. 71, no. 10, pp. 5740–5755, Oct. 2023.

[36] P. Zhao, J. Zuo, and C. Wen, “Power allocation and beamforming vectors optimization in STAR-RIS assisted SWIPT,” in Proc. 2022 IEEE Int. Conf. Commun. Technol., Nanjing, China, pp. 1174–1178, Nov. 2022.

[37] X. Li, Y. Zheng, M. Zeng, Y. Liu, and O. Dobre, “Enhancing secrecy performance for STAR-RIS NOMA networks,” IEEE Trans. Veh. Technol., vol. 72, no. 2, pp. 2684–2688, Feb. 2023.

[38] P. Tran et al., “Exploiting multiple RISs and direct link for performance enhancement of wireless systems with hardware impairments,” IEEE Trans. Commun., vol. 70, no. 8, pp. 5599–5611, Aug. 2022.

[39] D. Selimis, K. Peppas, G. Alexandropoulos, and F. Lazarakis, “On the performance analysis of RIS-empowered communications over Nakagamim fading,” IEEE Commun. Lett., vol. 25, no. 7, pp. 2191–2195, Jul. 2022.

[40] M. B. Janjua, D. B. da Costa, and H. Arslan, “User pairing and power allocation strategies for 3D VLC-NOMA systems,” IEEE Wireless Commun. Lett., vol. 9, no. 6, pp. 866–870, Jun. 2020.

[41] L. Zhu, J. Zhang, Z. Xiao, X. Cao, and D. O. Wu, “Optimal user pairing for downlink non-orthogonal multiple access (NOMA),” IEEE Wireless Commun. Lett., vol. 8, no. 2, pp. 328–331, Apr. 2019.

[42] J. Lei, T. Zhang, and Y. Liu, “Hybrid NOMA for STAR-RIS enhanced communication,” IEEE Trans. Veh. Technol., vol. 73, no. 1, pp. 1497–1502, Jan. 2024.

[43] G. Chen, Q. Wu, C. He, W. Chen, J. Tang, and S. Jin, “Active IRS aided multiple access for energy-constrained IoT systems,” IEEE Trans. Wireless Commun., vol. 22, no. 3, pp. 1677–1694, Mar. 2023.

[44] Q. Wu and R. Zhang, “Intelligent reflecting surface enhanced wireless network via joint active and passive beamforming,” IEEE Trans. Wireless Commun., vol. 18, no. 11, pp. 5394–5409, Nov. 2019.

[45] I. Sohn, J. Lee, and S. Lee, “Low-energy adaptive clustering hierarchy using affinity propagation for wireless sensor networks,” IEEE Commun. Lett., vol. 20, no. 3, pp. 558–561, Mar. 2016.

[46] Y. Luo et al., “On the study of sustainability and outage of SWIPT-enabled wireless communications,” IEEE J. Sel. Topics Signal Process., vol. 15, no. 5, pp. 1159–1168, Aug. 2021.

[47] Y. Chen et al., “A low power software-defined-radio baseband processor for the internet of things,” in Proc. IEEE Int. Symp. High Perform. Comput. Architecture, Barcelona, Spain, pp. 40–51, Mar. 2016.

[48] Z. Ding, L. Shen, H. Chen, F. Yan, and N. Ansari, “Residual-energy aware modeling and analysis of time-varying wireless sensor networks,” IEEE Commun. Lett., vol. 25, no. 6, pp. 2082–2086, Jun. 2021.

[49] K. Li, W. Ni, L. Duan, M. Abolhasan, and J. Niu, “Wireless power transfer and data collection in wireless sensor networks,” IEEE Trans. Veh. Technol., vol. 67, no. 3, pp. 2686–2697, Mar. 2018.

[50] D. Costa, H. Ding, and J. Ge, “Interference-limited relaying transmissions in dual-hop cooperative networks over Nakagami-m fading,” IEEE Commun. Lett., vol. 15, no. 5, pp. 503–505, May 2011.

[51] S. Atapattu et al., “Reconfigurable intelligent surface assisted two-way communications: Performance analysis and optimization,” IEEE Trans. Commun., vol. 68, no. 10, pp. 6552–6567, Oct. 2020.

[52] T. Wang, M. Badiu, G. Chen, and J. Coon, “Outage probability analysis of STAR-RIS assisted NOMA network with correlated channels,” IEEE Commun. Lett., vol. 26, no. 8, pp. 1774–1778, Aug. 2022.

[53] B. Lu et al., “Learning-assisted partial offloading for dynamic NOMA- MEC systems with imperfect SIC and reconfiguration energy cost,” IEEE Internet Things J., vol. 10, no. 22, pp. 20134–20148, Nov. 2023.

[54] A. Jee and S. Prakriya, “Performance of energy and spectrally efficient AF relay-aided incremental CDRT NOMA-based IoT network with imperfect SIC for smart cities,” IEEE Internet Things J., vol. 10, no. 21, pp. 18766– 18781, Nov. 2023.

[55] C. Zhang, W. Yi, Y. Liu, Z. Ding, and L. Song, “STAR-IOS aided NOMA networks: Channel model approximation and performance analysis,” IEEE Trans. Wireless Commun., vol. 21, no. 9, pp. 6861–6876, Sept. 2022.

[56] X. Yue et al., “Simultaneously transmitting and reflecting reconfigurable intelligent surface assisted NOMA networks,” IEEE Trans. Wireless Commun., vol. 22, no. 1, pp. 189–204, Jan. 2023.

[57] S. Thapar, D. Mishra, and R. Saini, “Novel outage-aware NOMA protocol for secrecy fairness maximization among untrusted users,” IEEE Trans. Veh. Technol., vol. 69, no. 11, pp. 13259–13272, Nov. 2020.

[58] F. Kara et al., “Bit-interleaved multiple access: Improved fairness, reliability, and latency for massive IoT networks,” IEEE Internet Things J., vol. 10, no. 18, pp. 16006–16027, Sept. 2023.

[59] W. Xu et al., “Performance analysis and resource allocation for a relaying LoRa system considering random nodal distances,” IEEE Trans. Commun., vol. 70, no. 3, pp. 1638–1652, Mar. 2022.

[60] M. Shabanighazikelayeh and E. Koyuncu, “Optimal placement of UAVs for minimum outage probability,” IEEE Trans. Veh. Technol., vol. 71, no. 9, pp. 9558–9570, Sept. 2022.

[61] S. Shabir et al., “A comparative study of genetic algorithm and the particle swarm optimization,” Int. J. Electr. Eng, vol. 9, no. 2, pp. 215–223, 2016.

[62] Z. Zhang, Z. Wang, Y. Liu, B. He, L. Lv, and J. Chen, “Security enhancement for coupled phase-shift STAR-RIS networks,” IEEE Trans. Veh. Technol., vol. 72, no. 6, pp. 8210-8215, Jun. 2023.

[63] J. -C. Chen, “Designing STAR-RIS-assisted wireless systems with coupled and discrete phase shifts: A computationally efficient algorithm,” IEEE Trans. Veh. Technol., early access, doi: 10.1109/TVT.2024.3366888.

[64] D. Li, “How many reflecting elements are needed for energy- and spectralefficient intelligent reflecting surface-assisted communication,” IEEE Trans. Commun., vol. 70, no. 2, pp. 1320-1331, Feb. 2022.

[65] S. Dhok and P. K. Sharma, “Rate-splitting multiple access with STAR-RIS over spatially-correlated channels,” IEEE Trans. Commun., vol. 70, no. 10, pp. 6410–6424, Oct. 2022.

[66] A. Bansal et al., “RIS selection scheme for UAV-based multi-RIS-aided multiuser downlink network with imperfect and outdated CSI,” IEEE Trans. Commun., vol. 71, no. 8, pp. 4650–4664, Aug. 2023.

[67] D. Li, “Ergodic capacity of intelligent reflecting surface-assisted communication systems with phase errors,” IEEE Commun. Lett., vol. 24, no. 8, pp. 1646-1650, Aug. 2020.

[68] I. S. Gradshteyn and I. M. Ryzhik, Table of Integrals Series and Products.

Amsterdam, The Netherlands: Elsevier, 2007.

[69] M. Abramowitz et al., Handbook of mathematical functions with formulas graphs and mathematical tables. New York: NY, USA: Dover, 1965.