arXiv:2108.05056v1 [cs.IT] 11 Aug 2021

Group LCD and Group Reversible LCD Codes

Steven T. Dougherty Department of Mathematics University of Scranton Scranton, PA 18510 USA Joe Gildea Adrian Korban Adam M. Roberts University of Chester Chester, UK

August 12, 2021

Abstract

In this paper, we give a new method for constructing LCD codes. We employ group rings and a well known map that sends group ring elements to a subring of the n × n matrices to obtain LCD codes. Our construction method guarantees that our LCD codes are also group codes, namely, the codes are ideals in a group ring. We show that with a certain condition on the group ring element v, one can construct non-trivial group LCD codes. Moreover, we also show that by adding more constraints on the group ring element v, one can construct group LCD codes that are reversible. We present many examples of binary group LCD codes of which some are optimal and group reversible LCD codes with different parameters.

Key Words: Group rings; LCD codes; codes over rings.

1 Introduction

In this paper, we shall study Linear Complementary Dual codes (LCD codes), which are linear codes that have a trivial intersection with their orthogonal. LCD codes were first introduced by Massey in [16] and were used to give an optimum linear coding solution for the two user binary adder channel. These codes are also used in counter measures for passive and active side channel analyses on embedded crypto-systems. For a detailed description of this application please see [4]. LCD codes are asymptotically good, it is shown in [17] that they meet the asymptotic Gilbert-Varshamov bound. One of the main goals is to construct LCD codes over finite fields that also have good error correcting properties. A result of Carlet et al. in [5] gives that over any finite field of order q > 3, the existence of an [n, k, d]_q linear code implies the existence of an [n, k, d]_q LCD code. In general, the limits to error correction may be more restrictive for binary and ternary LCD codes than for linear codes, as LCD codes do satisfy extra conditions.

Finding methods for constructing LCD codes, classifying LCD [n, k] codes and determining the largest minimum weight among all LCD [n, k] codes are open problems in coding theory. Many researchers have employed different techniques to construct LCD codes. In [15], the authors consider k-covers to construct binary LCD codes with and they give a complete classification of these codes with the largest minimum weight for 1 ≤ k ≤ n ≤ 16. In the paper by D. Crnkovic et al. ([7]), LCD codes are constructed from weighing matrices and a connection between LCD codes and self-dual codes is drawn. In [18], M. Shi et al. construct LCD codes from tridiagonal Toeplitz matrices. In this paper, the authors construct optimal and quasi-optimal examples of binary and ternary LCD codes. Recently in [1], the authors determine the largest minimum weight of LCD [n, 4] codes for n ≡ 2, 3, 5, 6, 9, 10, 13 (mod 15) and the largest minimum weight of LCD [n, 5] codes for n ≡ 3, 4, 5, 7, 11, 19, 20, 22, 26 (mod 31). In another recent paper by S. Bouyuklieva ([3]), optimal binary LCD [n, k] codes are given for k ≤ 32 and n ≤ 40.

In this work, we present a new method for constructing LCD codes over any finite commutative ring. We employ group rings and a very well known matrix construction to study and construct LCD codes. In particular, we construct LCD codes that are group codes generated from group ring elements. We show that for a specific choice of a group element v in the group ring RG, one can obtain LCD codes. We specifically show that if we let the coefficient of the group element g_i be the same as the coefficient of the group element g^{-1}_i in the group ring element v, then one can construct a non-trivial group LCD code over any finite commutative ring R. Moreover, by further restricting the choice of the group in the group ring RG, and by fixing the listing of the elements of that group, we show that one can construct group reversible LCD codes. We give many examples of group LCD and group reversible LCD codes of different lengths.

The paper is organized as follows. In Section 2, we give the standard definitions and notations for linear codes, LCD codes, the alphabet that we use in this work, group rings and group codes. In Section 3, we present our main method for constructing group LCD codes. We also give an example of how our method works. Next, in Section 4, we describe generator matrices for various groups in the the group ring RG with the condition for obtaining group LCD codes with. In Section 5, we further amend our construction method so that one can construct group reversible LCD codes. Then, in Section 6, we give many examples of group LCD codes and group reversible LCD codes. We finish with concluding remarks and directions for possible future research.

2 Definitions and Notations

2.1 Linear codes and LCD codes

Our main aim in this paper is to construct binary LCD codes. However, we shall make use of linear codes over rings to construct such codes. Therefore, we shall make a very broad definition of linear codes. That is, we assume that the alphabet of a code can be any finite commutative ring. Note that we assume that a ring has a multiplicative unity. A code C, of length n, over a finite ring R is a subset of R^n. If the code is a submodule then the code is said to be linear. We attach to the ambient space the standard inner-product, namely [v, w] = � v_iw_i. The orthogonal is defined by C^⊥ = {v ∈ R^n | [v, w] = 0, ∀w ∈ C}. If the ring is Frobenius, then we have that for linear codes |C||C^⊥| = |R|^n. For a complete description of codes over rings and this fact about their cardinality, see [8].

The automorphism group of a code C, denoted by Aut(G), is the group of all permutations of the coordinates of the code that fix the code.

An LCD code satisfies C ∩ C^⊥ = {0}. The following are well known results. Let G be a generator matrix for a code over a finite field. If GG^T = I_n then G generates an LCD code. Let G be a generator matrix for a code over a field. Then det(GG^T ) ≠ 0 if and only if G generates an LCD code.

There is a particular family of finite commutative Frobenius rings that we shall use later in our work to prove some results with, which is a commutative ring with characteristic 2. The ring R_k is defined as R_k = F_2[u_1, u_2, . . . , u_k]/⟨u^2_i , u_iu_j - u_ju_i⟩. We have that R_k has size |R_k| = 2^{2k} and it is a non-chain ring which has characteristic 2 with maximal ideal M = ⟨u_1, u_2, . . . , u_k⟩ and Soc(R_k) = ⟨u_1u_2 · · · u_k⟩.

A linear Gray map from R_k to F^{2k}_2 is constructed as follows. Let ϕ_1 be the map defined on R_1, namely ϕ_1(a + bu) = (b, a + b). Then let c ∈ R. We can write c = c_1 + u_kc_2 where c_1, c_2 are elements of the ring R_{k-1} of order 2^{2k-1} , then we define

ϕ_k(c) = (ϕ_{k-1}(c_2), ϕ_{k-1}(c_1) + ϕ_{k-1}(c_2)). (1)

The map ϕ_k is a weight preserving map which we then expand coordinatewise to R^n.

In [12] it is shown that the map ϕ_k : R_k → F^{2k}_2 is a linear bijection and we have that ϕ(C^⊥) = ϕ(C)^⊥.

It follows immediately that if C is an LCD code of length n over R_k then ϕ(C) is a binary LCD code of length 2^kn. For a complete description of codes over R_k, see [12], [13] and [14].

2.2 Special Matrices and Group Rings

In this section, we recall the definitions of some special matrices that we use later in this work. We also give the basic definitions of group rings.

A circulant matrix is one where each row is shifted one element to the right relative to the preceding row. We label the circulant matrix as circ(α_1, α_2, . . . , α_n), where α_i are the ring elements appearing in the first row. A reverse-circulant matrix is one where each row is shifted one element to the left relative to the preceding row. We label the reverse-circulant matrix as revcirc(α_1, α_2, . . . , α_n), where α_i are ring elements appearing in the first row. The transpose of a matrix A, denoted by A^T , is a matrix whose rows are the columns of A, i.e., (A^T )_{ij} = A_{ji}.

Our interest is to construct codes that are not only LCD but also that are ideals inside of a group ring, where the ring is the alphabet of the code. We shall now give the definitions for group rings. We let G be a finite group or order n, the group ring RG consists of

�_n i=1 α_ig_i, α_i ∈ R, g_i ∈ G.

Addition in the group ring is done by coordinate addition, namely n� i=1 α_ig_i + n� i=1 β_ig_i = n� i=1 (α_i + β_i)g_i.

The product of two elements in a group ring is given by (_n � i=1 α_ig_i

) (_n � j=1 β_jg_j ) = � i,j α_iβ_jg_ig_j.

It follows immediately that the coefficient of g_k in the product is � g_ig_j=g_k αiβj.

When the ring is a field the group ring is generally referred to as a group algebra. While group rings are defined for groups and rings of arbitrary cardinality, we shall only consider when both the group and the ring are finite. Moreover, we shall assume that the ring R is commutative but we let G be an arbitrary group and make no assumption about its commutativity. Throughout this paper we use e to refer to the identity element of the group G. 2.3 Code construction

The following map was used in [9] to study group codes over a finite commutative Frobenius ring.

Let R be a finite commutative Frobenius ring and let G = {g_1, g_2, . . . , g_n} be a group of order n. Let v = α_{g1} g_1 + α_{g2} g_2 + · · · + α_{gn} g_n ∈ RG. Define the matrix σ(v) ∈ M_n(R) to be

σ(v) = α_g-1_{1 g1} α_g-1_{1 g2} α_g-1_{1 g3} . . . α_g-1_{1 gn} α_g-1_{2 g1} α_g-1_{2 g2} α_g-1_{2 g3} . . . α_g-1_{2 gn} . . . . . . . . . . α_g-1_{n g1} α_g-1_{n g2} α_g-1_{n g3} . . . α_g-1_{n gn}

. (2)

We note that the elements g^{-1}_1 , g^{-1}_2 , . . . , g^{-1}_n are simply the elements of the group G in some order.

Define the following code over the ring R for a given element v ∈ RG.

C(v) = ⟨σ(v)⟩. (3)

Specifically, the code is formed by taking the row space of σ(v) over the ring R. Given that it is the span of a set of vectors, the code is necessarily linear. Given the structure of the matrix it follows immediately that the code is held invariant by the action of the group G. Therefore, we have that C(v) is a G-code, namely a code that corresponds to an ideal in RG. We do not claim that the rows of the matrix σ(v) are necessarily linearly independent, in general, they will not be. If they are then the generated code is the ambient space.

Example 1. As a very simple example, let G be any finite group of odd order, R be a finite Frobenius ring with characterisitc 2, and let v = � g∈G v_g ∈ RG. Then C = ⟨σ(v)⟩ is the code generated by the all-one vector. Since the length is odd, this code has a trivial intersection with its orthogonal, giving that C is an LCD G-code.

For an element v = � α_ig_i ∈ RG, define the element v^T ∈ RG as v^T = � α_ig^{-1}_i . This is sometimes known as the canonical involution for the group ring.

In [12], the following is proven. Let R be a finite commutative Frobenius ring and let G be a group of order n. For an element v ∈ RG, we have that σ(v)^T = σ(v^T ).

From [12], we have the following. Let R be a finite commutative Frobenius ring and let G be a group of order n. Then the map σ : RG → M_n(R) is an injective ring homomorphism.

Given that we have the map σ : RG → M_n(R) is an injective ring homomorphism one may be tempted to find elements in RG that satisfy vv^T = 1, so that σ(v)σ(v^T ) = σ(v)σ(v)^T = I_n. However, in this case, given the structure of σ(v) this will only give trivial LCD codes. Therefore, the approach is that we need to find v so that σ(v) does not have a full rank but still produces an LCD code.

3 Construction of group LCD codes

In this section, we show what one needs in terms of the group ring element v, so that σ(v) does not have a full rank but still produces an LCD code.

Let Hull(v) = C(v) ∩ C(v)^⊥.

Lemma 3.1. Let v ∈ RG, then Hull(v) is a G-code.

Proof. We know from [9], that C(v)^⊥ is a G-code. Then if v ∈ C(v), then σv ∈ C(v) for all σ ∈ G and if v ∈ C(v)^⊥, then σv ∈ C(v)^⊥ for all σ ∈ G. This gives that if v ∈ Hull(v), then σv ∈ Hull(v) for all σ ∈ G

For an LCD code we have that Hull(v) = {0}.

Let I be an ideal in a group ring RG. Define R(I) = {w | vw = 0, ∀v ∈ I}. It follows immediately that R(I) is an ideal of RG.

Let v = a_{g1} g_1 + a_{g2} g_2 + · · · + a_{gn} g_n ∈ RG and C(v). Let Ψ : RG → R^n be the canonical map defined by Ψ(a_{g1} g_1 + a_{g2} g_2 + · · · + a_{gn} g_n) = (a_{g1} , a_{g2} , . . . , a_{gn} ).

It is shown in [9], that Ψ^{-1}(C(v)) is an ideal of RG.

Lemma 3.2. Let w = Ψ(w). Then w^T ∈ R(I(v)) if and only if w ∈ C(v)^⊥. Proof. Let I(v) be the ideal Ψ^{-1}(C(v)). Let w = (w_1, w_2, . . . , w_n) ∈ C^⊥. Then [(a_g-1_{j g1} , a_g-1_{j g2} , . . . , a_g-1_{j gn} ), (w_1, w_2, . . . , w_n)] = 0, ∀j. (4) This gives that_n � i=1 a_g-1_{j gi} w_i = 0, ∀j. (5) Then_n � i=1 a_g-1_{j gi} w_i = 0 =⇒ n� i=1 a_g-1_{j gi} b_g-1_i = 0. (6) Then g^{-1}_j g_ig^{-1}_i = g^{-1}_j , hence this is the coefficient of g^{-1}_j in the product of w^T and g^{-1}_j v. This gives that w^T ∈ R(I(v)) if and only if w ∈ C(v)^⊥.

Let R(I(v))^T = {w^t | w ∈ R(I(v)) and let H(v) = I(v) ∩ R(H(v))^T . Lemma 3.3. Let v ∈ RG, then Ψ(R(I(v))^T ) = C^⊥ and Ψ(H(v)) = Hull(v). Proof. Follows from a direct application of Lemma 3.2.

We have the following diagrams.

Hull(v)^⊥

C(v) C(v)^⊥

Hull(v)

R(H(v))

I(v) R(I(v))

H(v)

We now state our main result.

Theorem 3.4. Let v ∈ RG. If C(v) is a non-trivial LCD code then v = v^T .

Proof. Let R(I(v))^T = ⟨w^T_1 , w^T_2 , . . . , w^T_s ⟩. Assume C(v) is an LCD code. Then ⟨w^T_1 , w^T_2 , . . . , w^T_s ⟩ = RG. Hence no element divides v and each w^T_i . If w^T_i ∈ R(I)^T then w_i ∈ R(I) which gives that vw_i = 0 for all i. It follows that v^T w^T_i = 0 for all i.

If vw^T_i = α ≠ 0 then α ∈ I(v) and α ∈ R(I(v))^T which gives α ∈ calH(v) which is a contradiction since this ideal is trivial by Lemma 3.3. This gives that vw^T_i = 0 for all i.

Then we have that vw^T_i = v^T w^T_i which gives v(w^T_1 +w^T_2 +· · ·+w^T_s ) = v^T (w^T_1 +w^T_2 +· · ·+w^T_s ) and v and (w^T_1 + w^T_2 + · · · + w^T_s ) can have no common factor. This gives that v = v^T .

This result allows us to reduce the search for LCD codes significantly. Namely, we need only search through v with v = v^T .

It follows then that if C(v) is an LCD code then C(v) = C(v^T ).

We note that the theorem is not a biconditional. Consider the vector v = 1 + 1g_1 + 1g_2 + 1g_3 ∈ F_2C_4. Then v = v^T but Hull(v) = C(v) and so C(v) is not an LCD code.

We now present an example.

Example 2. Let v = α_11 + α_aa + α_a2 + α_bb + α_{ab}ab + α_a2_ba^2b ∈ F_2 D_6, where D_6 =

{1, a, a^a, b, ab, a^2b} is the dihedral group with 6 elements. Then

σ(v) = α_1 α_a α_a2 α_b α_{ab} α_a2_b α_a2 α_1 α_a α_a2_b α_b α_{ab} α_a α_a2 α_1 α_{ab} α_a2_b α_b α_b α_a2_b α_{ab} α_1 α_a2 α_a α_{ab} α_b α_a2_b α_a α_1 α_a2 α_a2_b α_{ab} α_b α_a2 α_a α_1

.

Now, if we add the condition v = v^T in, that is, we want the coefficient of the group element g_i to be the same as the coefficient of the group element g^{-1}_i , the above matrix becomes:

σ^′(v) = α_1 α_a α_a α_b α_{ab} α_a2_b α_a α_1 α_a α_a2_b α_b α_{ab} α_a α_a α_1 α_{ab} α_a2_b α_b α_b α_a2_b α_{ab} α_1 α_a α_a α_{ab} α_b α_a2_b α_a α_1 α_a α_a2_b α_{ab} α_b α_a α_a α_1

,

since 1^{-1} = 1, a^{-1} = a^2, (a^2)^{-1} = a, b^{-1} = b, (ab)^{-1} = ab and (a^2b)^{-1} = a^2b.

One can see that the search field in the matrix σ(v) is 2^6 and 2^5 in the matrix σ^′(v). We now search for dihedral LCD group codes of length 6 using both matrices; σ(v) and σ^′(v) and we obtain the following:

C_1 =

0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0

, C_2 =

0 0 0 0 0 1 0 0 0 1 0 0 0 0 0 0 1 0 0 1 0 0 0 0 0 0 1 0 0 0 1 0 0 0 0 0

, C_3 =

0 0 0 0 1 1 0 0 0 1 0 1 0 0 0 1 1 0 0 1 1 0 0 0 1 0 1 0 0 0 1 1 0 0 0 0 and

C_4 =

0 0 0 1 1 1 0 0 0 1 1 1 0 0 0 1 1 1 1 1 1 0 0 0 1 1 1 0 0 0 1 1 1 0 0 0

.

The same 4 dihedral LCD codes were obtained from both matrices; σ(v) and σ^′(v). Of course, there were fewer calculations needed with the second matrix σ^′(v) which highlights the importance of Theorem 3.4.

4 Construction of σ(v) with v = v^T for various groups

In this section, we want to generalize the forms of the matrices σ(v) with the condition v = v^T for various groups. That is, in this section, we present a number of matrices σ(v), where v = α_{g1} g_1 + α_{g2} g_2 + · · · + α_{gn} g_n ∈ RG with the coefficient of g_i being the same as the coefficient of g^{-1}_i . This will enable us to calculate group LCD codes of different lengths for different groups in less and more practical time.

1. Let C_n = ⟨a | a^n = e⟩ be the cyclic group of order n with n = 2k, for k ∈ Z^+. Let v = �_n i=1 α_ai-1 a^{i-1} ∈ RC_n. Then

σ(v) = circ(α_e, α_a, α_a2 , . . . , α_a n_2 , α_a n_2 -1 , α_a n_2 -2 , . . . , α_a2 , α_a). (7)

2. Let C_n = ⟨a | a^n = e⟩ be the cyclic group of order n with n = 2k + 1, for k ∈ Z^+. Let v = �_n i=1 α_ai-1 a^{i-1} ∈ RC_n. Then

σ(v) = circ(α_e, α_a, α_a2 , . . . , α_a n-1_2 , α_a n-1_2 , α_a n-1_{2 -1} , α_a n-1_{2 -2} , . . . , α_a2 , α_a). (8)

3. Let D_{2n} = ⟨a, b | a^n = b^2 = e, a^b = a^{-1}⟩ be the dihedral group of order 2n with n = 2k, for k ∈ Z^+. Let v =

�_n i=0 �_1 j=0 α_ai_bj a^ib^j ∈ RD_{2n}. Then

σ(v) = ( A B B^T A^T ) , (9)

where A = circ(α_e, α_a, α_a2 , . . . , α_a n_2 , α_a n_2 -1 , α_a n_2 -2 , . . . , α_a2 , α_a),

B = circ(α_b, α_{ab}, α_a2_b, . . . , α_an-1_b).

4. Let D_{2n} = ⟨a, b | a^n = b^2 = e, a^b = a^{-1}⟩ be the dihedral group of order 2n with n = 2k + 1, for k ∈ Z^+. Let v =

�_n i=0 �_1

j=0 α_ai_bj a^ib^j ∈ RD_{2n}. Then

σ(v) = ( A B B^T A^T ) , (10)

where

A = circ(α_e, α_a, α_a2 , . . . , α_a n-1_2 , α_a n-1_2 , α_a n-1_{2 -1} , α_a n-1_{2 -2} , . . . , α_a2 , α_a),

B = circ(α_b, α_{ab}, α_a2_b, . . . , α_an-1_b).

5. Let D_{2n} = ⟨a, b | a^n = b^2 = e, a^b = a^{-1}⟩ be the dihedral group of order 2n with n = 2k, for k ∈ Z^+. Let v =

�_n i=0 �_1 j=0 α_bj_ai b^ja^i ∈ RD_{2n}. Then

σ(v) = ( A B B A ) , (11)

where A = circ(α_e, α_a, α_a2 , . . . , α_a n_2 , α_a n_2 -1 , α_a n_2 -2 , . . . , α_a2 , α_a), B = revcirc(α_b, α_{ba}, α_{ba}2 , . . . , α_{ba}n-1 ).

6. Let D_{2n} = ⟨a, b | a^n = b^2 = e, a^b = a^{-1}⟩ be the dihedral group of order 2n with n = 2k + 1, for k ∈ Z^+. Let v =

�_n i=0 �_1

j=0 α_bj_ai b^ja^i ∈ RD_{2n}. Then

σ(v) = ( A B B A ) , (12)

where

A = circ(α_e, α_a, α_a2 , . . . , α_a n-1_2 , α_a n-1_2 , α_a n-1_{2 -1} , α_a n-1_{2 -2} , . . . , α_a2 , α_a),

B = revcirc(α_b, α_{ba}, α_{ba}2 , . . . , α_{ba}n-1 ).

5 Construction of group reversible LCD codes

In this section, we show that for certain groups and with a fixed listing of their elements in the group ring RG, one can construct group reversible LCD codes with our method. We start with a definition from [6].

Definition 1. A code C is said to be reversible of index α if a_i is a vector of length α and c^α = (a_0, a_1, . . . , a_{s-1}) ∈ C implies that (c^α)^r = (a_{s-1}, a_{s-2}, . . . , a_1, a_0) ∈ C.

Also in [6], the following is shown.

Theorem 5.1. Let R be a finite ring. Let G be a finite group of order n = 2ℓ and let H = {e, h_1, h_2, . . . , h_{ℓ-1}} be a subgroup of index 2 in G. Let β /∈ H be an element in G with β^{-1} = β. List the elements of G as

{e, h_1, . . . , h_{ℓ-1}, βh_{ℓ-1}, βh_{ℓ-2}, βh_2, βh_1, β},

then any linear G-code in R^n (a left ideal in RG) is a reversible code of index 1.

Combining the above result with Theorem 3.4, we get the following

Theorem 5.2. Let R be a finite ring. Let G be a finite group of order n = 2ℓ and let H = {e, h_1, h_2, . . . , h_{ℓ-1}} be a subgroup of index 2 in G. Let β /∈ H be an element in G with β^{-1} = β. Let v ∈ RG with v = v^T such that the elements of G in v are listed as

{e, h_1, . . . , h_{ℓ-1}, βh_{ℓ-1}, βh_{ℓ-2}, βh_2, βh_1, β}.

Then C(v) is a non-trivial reversible LCD code of index 1.

Proof. The reversibility follows from Theorem 3.4 and the second part follows from Theorem 5.1.

The above result shows that with a careful selection of the element v in the group ring RG, one can construct a group code that is both, reversible and LCD.

Theorem 5.3. Let G be a finite group of order n = 2ℓ and let H = {e, h_1, h_2, . . . , h_{ℓ-1}} be a subgroup of index 2 in G. Let β /∈ H be an element in G with β^{-1} = β. Let v ∈ RG with v = v^T such that the elements of G in v are listed as

{e, h_1, . . . , h_{ℓ-1}, βh_{ℓ-1}, βh_{ℓ-2}, βh_2, βh_1, β}.

If C(v) is a linear G-code in R^n_k (a left ideal in R_kG), then ϕ(C(v)) is a non-trivial reversible LCD code of index 2^k.

Proof. By Theorem 5.2, we have that C is a non-trivial reversible LCD code of index 1. Therefore, if (c_0, c_1, . . . , c_{n-1}) ∈ C(v) we have that (c_{n-1}, c_{n-2}, . . . , c_1, c_0) ∈ C(v), where c_i ∈ R_k. Then ϕ(c_i) is a vector of length 2^k. This gives that

(ϕ(c_0), ϕ(c_1), . . . , ϕ(c_{n-1})) ∈ ϕ(C)

and then (ϕ(c_{n-1}), ϕ(c_{n-2}), . . . , ϕ(c_1), ϕ(c_0)) ∈ ϕ(C).

This gives the result.

6 Computational Results

In this section, we construct many group LCD and group reversible LCD codes using the code construction ⟨σ(v)⟩, given in Equation (2), where σ(v) are some of the n × n matrices described in Section 4. The searches are performed in the software package MAGMA ([2]). We only tabulate the lengths, dimensions and the largest minimum distance of the codes that we construct. Codes with the largest minimum distance that are optimal (according to [3]) are written in bold. The generator matrices of these codes and their corresponding weight enumerators can be found at [10].

6.1 Group LCD Codes

In this section we search for group LCD codes using the code construction ⟨σ(v)⟩, given in Equation (2), where σ(v) are some of the n × n matrices described in Section 4.

1. Let v ∈ F_2 C_n and let G_1 = ⟨σ(v)⟩, where σ(v) is the matrix given in Equation (7).

We set n to be 28, 30, 34, 36 and 38. We list the results in Table 1, Table 2, Table 3, Table 4 and Table 5 respectively.

Table 1: Group LCD Codes from G_1 (n = 28) over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [28, 4, 7] C_2 [28, 24, 2]

Table 2: Group LCD Codes from G_1 (n = 30) over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [30, 2, 15] C_8 [30, 16, 4] C_2 [30, 4, 10] C_9 [30, 18, 4] C_3 [30, 6, 5] C_{10} [30, 20, 2] C_4 [30, 8, 6] C_{11} [30, 22, 2] C_5 [30, 10, 3] C_{12} [30, 24, 2] C_6 [30, 12, 6] C_{13} [30, 26, 2] C_7 [30, 14, 3] C_{14} [30, 28, 2]

Table 3: Group LCD Codes from G_1 (n = 34) over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [34, 2, 17] C_3 [34, 18, 5] C_2 [34, 16, 6] C_4 [34, 32, 2]

Table 4: Group LCD Codes from G_1 (n = 36) over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [36, 4, 9] C_4 [36, 24, 2] C_2 [36, 8, 6] C_5 [36, 28, 2] C_3 [36, 12, 3] C_6 [36, 32, 2]

Table 5: Group LCD Codes from G_1 (n = 38) over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [38, 2, 19] C_2 [38, 36, 2]

2. Let v ∈ F_2 C_n and let G_2 = ⟨σ(v)⟩, where σ(v) is the matrix given in Equation (8). We set n to be 29, 31, 33, 35, 37 and 39. We list the results in Table 6, Table 7, Table 8, Table 9, Table 10 and Table 11 respectively.

Table 6: Group LCD Codes from G_2 (n = 29) over F_2 C_i [n, k, d] C_1 [29, 28, 2]

Table 7: Group LCD Codes from G_2 (n = 31) over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [31, 10, 10] C_4 [31, 21, 5] C_2 [31, 11, 10] C_5 [31, 30, 2] C_3 [31, 20, 6]

Table 8: Group LCD Codes from G_2 (n = 33) over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [33, 2, 22] C_{12} [33, 20, 6] C_2 [33, 3, 11] C_{13} [33, 21, 3] C_3 [33, 10, 6] C_{14} [33, 21, 4] C_4 [33, 10, 12] C_{15} [33, 22, 2] C_5 [33, 11, 3] C_{16} [33, 22, 6] C_6 [33, 11, 11] C_{17} [33, 23, 2] C_7 [33, 12, 6] C_{18} [33, 23, 3] C_8 [33, 12, 10] C_{19} [33, 30, 2] C_9 [33, 13, 3] C_{20} [33, 31, 2] C_{10} [33, 13, 10] C_{21} [33, 32, 2] C_{11} [33, 20, 4]

Table 9: Group LCD Codes from G_2 (n = 35) over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [35, 4, 14] C_8 [35, 25, 4] C_2 [35, 5, 7] C_9 [35, 28, 2] C_3 [35, 6, 10] C_{10} [35, 29, 2] C_4 [35, 7, 5] C_{11} [35, 30, 2] C_5 [35, 10, 10] C_{12} [35, 31, 2] C_6 [35, 11, 5] C_{13} [35, 34, 2] C_7 [35, 24, 4]

Table 10: Group LCD Codes from G_2 (n = 37) over F_2 C_i [n, k, d] C_1 [37, 36, 2]

Table 11: Group LCD Codes from G_2 (n = 39) over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [39, 2, 26] C_8 [39, 25, 4] C_2 [39, 3, 13] C_9 [39, 26, 2] C_3 [39, 12, 6] C_{10} [39, 27, 2] C_4 [39, 13, 3] C_{11} [39, 36, 2] C_5 [39, 14, 6] C_{12} [39, 37, 2] C_6 [39, 15, 3] C_{13} [39, 38, 2] C_7 [39, 24, 4]

3. Let v ∈ F_2 D_{24} and let G_3 = ⟨σ(v)⟩, where σ(v) is the matrix given in Equation (11).

We list our results in Table 12.

Table 12: Group LCD Codes from G_3 over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [24, 8, 3] C_2 [24, 16, 2]

4. Let v ∈ F_2 D_{30} and let G_4 = ⟨σ(v)⟩, where σ(v) is the matrix given in Equation (12).

We list our results in Table 13.

Table 13: Group Reversible LCD Codes from G_4 over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [30, 2, 15] C_8 [30, 16, 4] C_2 [30, 4, 10] C_9 [30, 18, 4] C_3 [30, 6, 5] C_{10} [30, 20, 2] C_4 [30, 8, 6] C_{11} [30, 22, 2] C_5 [30, 10, 3] C_{12} [30, 24, 2] C_6 [30, 12, 6] C_{13} [30, 26, 2] C_7 [30, 14, 3] C_{14} [30, 28, 2]

6.2 Group Reversible LCD Codes

In this section we search for group reversible LCD codes using Theorem 5.2. In particular, we employ the matrices σ(v) given in Equation (9) and Equation (10) but with the listing of the group elements in the group ring element v as given in Theorem 5.2. That is, since the group used in the group ring element v in both equations; Equation (9) and Equation (10), is the dihedral group of even order, we list the elements of this group (according to Theorem 5.2) as follow:

{e, a, a^2, . . . , a^{n-1}, ba^{n-1}, ba^{n-2}, . . . , ba, b}. (13) This approach, as shown in Theorem 5.2 guarantees that the codes are group reversible LCD codes.

1. Let v ∈ F_2 D_{22} and let G_5 = ⟨σ(v)⟩, where σ(v) is the matrix given in Equation (10).

We list our results in Table 14.

Table 14: Group Reversible LCD Codes from G_5 over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [22, 2, 11] C_2 [22, 20, 2]

2. Let v ∈ F_2 D_{24} and let G_6 = ⟨σ(v)⟩, where σ(v) is the matrix given in Equation (9).

We list our results in Table 15.

Table 15: Group Reversible LCD Codes from G_6 over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [24, 8, 3] C_2 [24, 16, 2]

3. Let v ∈ F_2 D_{30} and let G_7 = ⟨σ(v)⟩, where σ(v) is the matrix given in Equation (10).

We list our results in Table 16.

Table 16: Group Reversible LCD Codes from G_7 over F_2 C_i [n, k, d] C_i [n, k, d] C_1 [30, 2, 15] C_8 [30, 16, 4] C_2 [30, 4, 10] C_9 [30, 18, 4] C_3 [30, 6, 5] C_{10} [30, 20, 2] C_4 [30, 8, 6] C_{11} [30, 22, 2] C_5 [30, 10, 3] C_{12} [30, 24, 2] C_6 [30, 12, 6] C_{13} [30, 26, 2] C_7 [30, 14, 3] C_{14} [30, 28, 2]

7 Conclusion

In this work, we presented a new method for constructing LCD codes over any finite commutative ring. We showed that the LCD codes constructed with our method are ideals in a group ring RG, i.e., our LCD codes are also group codes. We proved that with a certain condition on the group ring element v, one can construct non-trivial group LCD codes with our method. Moreover, we also proved that under some more restrictions on the group ring element v, one can construct group reversible LCD codes with our method. We presented many examples of group LCD codes and group reversible LCD codes with different parameters. A possible direction for future research is to consider our approach but with groups of orders higher than we used in this paper to obtain more group LCD and group reversible LCD codes of lengths greater than we constructed in this paper.

References

[1] M. Araya, M, Harada, On the minimum weights of binary linear complementary dual codes, Cryptography and Communications, 12, (2020), 285–300.

[2] W. Bosma, J. Cannon and C. Playoust, “The Magma algebra system. I. The user language”, J. Symbolic Comput., 24, (1997), 235–265.

[3] S. Bouyuklieva, Optimal Binary LCD Codes, arXiv:2010.13399.

[4] C. Carlet and S. Guilley, Complementary dual codes for counter-measures to sidechannel attacks, Proceedings of the 4th ICMCTA Meeting, Palmela, Portugal, (2014).

[5] C. Carlet, S. Mesnager, C. Tang, Y. Qi, Linear codes over F_q are equivalent to LCD codes for q > 3, IEEE Trans. Inform. Theory, 64, (2018), 3010–3017.

[6] Y. Cengellenmis, A. Dertli, S.T. Dougherty, A. Korban and S. Sahinkaya, “Reversible G-Codes over the Ring F_{j,k} with Applications to DNA Codes”, in submission.

[7] D. Crnkovic, R. Egan, B. G. Rodrigues, A. Svob, LCD codes from weighing matrices, Applicable Algebra in Engineering, Communication and Computing, 32, (2021), 175– 189.

[8] Dougherty, S.T., Algebraic Coding Theory Over Finite Commutative Rings, Springer- Verlag, Springer Briefs in Mathematics (ISBN 978-3-319-59805-5), (2017).

[9] Dougherty, S.T., Gildea, J., Taylor, R., Tylshchak, A., Group Rings, G-Codes and Constructions Of Self-Dual and Formally Self-Dual Codes, Designs, Codes and Cryptography, 10.1007/s10623-017-0440-7.

[10] S.T. Dougherty, J. Gildea, A. Korban, A. M. Roberts, Generator Matrices for the manuscript entitled “Group LCD and Group Reversible LCD Codes”, available at https://sites.google.com/view/adriankorban/generator-matrices.

[11] S.T. Dougherty, J. L. Kim, B. Ozkaya, L. Sok, P. Sole, The combinatorics of LCD codes: linear programming bound and orthogonal matrices. Int. J. Inf. Coding Theory, 4, (2017), 116–128.

[12] S. T. Dougherty, B. Yildiz, S. Karadeniz, Codes over R_k, Gray maps and their Binary Images, Finite Fields and their Applications, 17, (2011), 205–219.

[13] S. T. Dougherty, B. Yildiz, S. Karadeniz, Cyclic Codes over R_k, Designs, Codes and Cryptography, 63, (2012), 113–126.

[14] S. T. Dougherty, B. Yildiz, S. Karadeniz, Self-dual codes over R_k and binary self-dual codes. Eur. J. Pure Appl. Math. 6, (2013), 89– 106.

[15] M. Harada, K. Saito, Binary linear complementary dual codes, Cryptography and Communications, 11, (2019), 677–696.

[16] J.L. Massey, Linear codes with complementary duals, Discrete Mathematics, 106/107, (1992), 337–342.

[17] N. Sendrier, Linear codes with complementary duals meet the Gilbert-Varshamov bound, Discrete Math., 304, (2004), 345–347.

[18] M. Shi, F. Ozbudak, L. Xu, P. Sole, LCD codes from tridiagonal Toeplitz matrices, Finite Fields and Their Applications, (2021).