arXiv:2305.01442v1 [cs.IT] 2 May 2023

A Direct Construction of Optimal Symmetrical Z-Complementary Code Sets of Prime Power Lengths

Praveen Kumar^∗, Sudhan Majhi^†, Subhabrata Paul^∗ ∗Department of Mathematics, IIT Patna, India {praveen_2021ma03, subhabrata}@iitp.ac.in †Department of Electrical Communication Engineering, IISC Bangalore, India, smajhi@iisc.ac.in

Abstract—This paper presents a direct construction of an optimal symmetrical Z-complementary code set (SZCCS) of prime power lengths using a multi-variable function (MVF). SZCCS is a natural extension of the Z-complementary code set (ZCCS), which has only front-end zero correlation zone (ZCZ) width. SZCCS has both front-end and tail-end ZCZ width. SZCCSs are used in developing optimal training sequences for broadband generalized spatial modulation systems over frequency-selective channels because they have ZCZ width on both the front and tail ends. The construction of optimal SZCCS with large set sizes and prime power lengths is presented for the first time in this paper. Furthermore, it is worth noting that several existing works on ZCCS and SZCCS can be viewed as special cases of the proposed construction.

I. INTRODUCTION

The idea of Z-complementary pairs (ZCPs) was introduced by Fan et al. [1]. The sum of the aperiodic auto-correlation function (AACF) of the two sequences in a ZCP is zero within a particular zone, which is referred to as the zero-correlation zone (ZCZ). When this ZCZ width Z is equal to the sequence length N, ZCP becomes a Golay complementary pair (GCP). Unlike GCPs, ZCPs are available in arbitrary lengths with various ZCZ widths [2]–[6].

The idea of ZCPs introduced in [1] was generalized to a Zcomplementary code set (ZCCS) by Feng et al. in [7]. ZCCS only considers the front-end ZCZ of the AACFs and aperiodic cross-correlation functions (ACCFs). Several generalized Boolean functions (GBFs) based constructions of ZCCSs of non-power-of-two lengths are proposed in the literature [8]– [13]. A ZCCS with K codes, with each code having M sequences each of length N and ZCZ width Z is denoted by (K, M, N, Z)-ZCCS. For the special case, K = M and N = Z, it is known as a complete complementary code (CCC) and is denoted by (K, K, N)-CCC. Recently, Li et al. proposed a direct construction of multiple CCC of prime power length and with inter set ZCZ width using a multivariable function (MVF) [14]. After combining these multiple CCC, optimal (p^{n+v}, p^n, p^m, p^{m−v})-ZCCS are obtained [14].

Recently, the idea of ZCCS has been extended to symmetrical-ZCCS (SZCCS), which exhibits ZCZ properties for the front-end and the tail-end [15]. The authors in [15] have presented a GBF based construction of (8, 2, 2^m, 2^{m−2} − 1)- SZCCS. In practice, a front-end ZCZ and a tail-end ZCZ have a particular role in mitigating interference with small and large delays, respectively. SZCCSs with larger set sizes are used in designing training sequences for broadband generalized spatial modulation (GSM) systems over frequency-selective channels [15]. The fact that SZCCS is being widely applied in the GSM systems and also the unavailability of constructions with flexible parameters in terms of set size, flock size, and length have inspired the authors to propose a direct construction of SZCCSs of prime power lengths in this paper.

The proposed MVF-based construction of SZCCS has a set size p^{k+δ} , which is much larger than the flock size of p^k, where m ≥ 3, 0 ≤ δ < m, 1 ≤ k ≤ m−δ. Also, the proposed SZCCS has large ZCZ width of p^{m−δ} − 1, and it achieves the optimality condition. Many of the existing constructions of ZCCS and SZCCS appear as special cases of the proposed construction.

The rest of the paper is structured as follows: preliminary work is covered in Section II, and the proposed SZCCS construction based on MVF is presented in Section III. Section IV of the paper presents a comprehensive comparison between the proposed constructions and the existing works, providing detailed insights. Following that, Section V concludes the paper.

II. PRELIMINARIES

The essential concepts, notations, and previously established findings necessary for the proposed construction are explained in this section.

Definition 1: Let u = (u_0, u_1, . . . , u_{N−1}) and v = (v_0, v_1, . . . , v_{N−1}) be two sequences of length N over Z_q. At a shift τ, the ACCF is defined as

C(u, v)(τ) = ∑_{N−1−τ} i=0 ω^{ui−vi+τ} q , 0 ≤ τ ≤ N − 1, ∑_{N−1+τ} i=0 ω^{ui−τ −vi} q , −N + 1 ≤ τ ≤ −1, 0, |τ| ≥ N, (1) where q is a positive integer greater than 2, and ω_q = exp(2π √ −1/q). For the special case, u = v, C(u, v)(τ) is referred to as the AACF of u and is denoted by A(u)(τ). Consider a set C = { C^0, C^1, . . . , C^{K−1} } , where each set C^e consists of M sequences, i.e., C^e = { c^e_0, c^e_1, . . . , c^e_{M−1} } , and length of each sequence c^e_l is N, where 0 ≤ e ≤ K − 1 and 0 ≤ l ≤ M − 1.

Definition 2: The set C defined above is called a ZCCS, denoted by (K, M, N, Z)-ZCCS, if the ACCF of C^e and C^{e′} satisfies C ( C^e, C^{e′} ) (τ) = M−1∑ l=0 C ( c^e_l , c^{e′}_l ) (τ)

= MN, τ = 0, e = e^′, 0, 0 < |τ| < Z, e = e^′, 0, |τ| < Z, e ≠ e^′, (2)

where 0 ≤ e, e^′ ≤ K − 1. For a general (K, M, N, Z)-ZCCS, K ≤ M⌊N/Z⌋, whereas for the special case, K = M⌊N/Z⌋, it becomes an optimal ZCCS [16]. Again, for the special case, K = M and Z = N, the ZCCS is called a CCC of order K and length N, and is denoted by (K, K, N)-CCC.

Definition 3: The set C defined above is known as a SZCSS, denoted by (K, M, N, Z)-SZCCS, if for T_1 = {1, 2, · · · , Z} and T_2 = {N − Z, N− Z + 1, · · · , N − 1} with Z ≤ N, it satisfies the following properties

P 1 : M−1∑ i=0 A(c^e_i )(τ) = 0, for all |τ| ∈ (T_1 ∪ T_2) ∩ T ;

P 2 : M−1∑ i=0 C(c^e_i , c^{e′}_i )(τ) = 0, for all |τ| ∈ {0} ∪ T_1 ∪ T_2;

(3) where T = {1, 2, . . . , N −1} and e ≠ e^′. For a (K, M, N, Z)- SZCCS, K, M, N and Z are known as the set size, flock size, sequence length, and ZCZ width, respectively.

For a MVF f : {0, 1, . . . , p − 1}^m → Z_q in m p-ary variables x_1, x_2, . . . , x_m, corresponding Z_q-valued sequence is denoted by f, and calculated as f = (f_0, f_1, . . . , f_pm_{−1}) , where f_r = f(r_1, r_2, . . . , r_m), and r = (r_1, r_2, . . . , r_m) is the p-ary representation of the integer r, i.e., r = ∑_m i=1 r_ip^{i−1}.

The complex-valued sequence associated with f is produced as Ψ(f) = ( ω^{f0}_q , ω^{f1}_q , . . . , ω^{fpm−1}_q ) , where ω_q is the q-th (q ≥ 2) root of unity [14].

Lemma 1 ( [15], [16]): Any unimodular (K, M, N, Z)- SZCCS satisfies K ≤ M ⌊_N Z+1 ⌋ , when K = M ⌊_N Z+1 ⌋ , it is known as an optimal (K, M, N, Z)-SZCCS.

III. PROPOSED CONSTRUCTION

This section explains a MVF based construction of optimal (p^{k+δ} , p^k, p^m, p^{m−δ} − 1)-SZCCS.

Theorem 1: For any positive integer m ≥ 3 and 0 ≤ δ < m, we let the set {1, 2, . . . , m − δ} be partitioned into k sets, S_1, S_2, . . . , S_k, where 1 ≤ k ≤ m − δ. Let the cardinality of the set S_β be m_β, and π_β be a one-one and onto mapping from {1, 2, . . . , m_β } to S_β for β = 1, 2, . . . , k. Let us define a MVF g : {0, 1, . . . , p − 1}^m → Z_q by g = q p k∑ β=1 m_β −1∑

γ=1 x_{πβ (γ)}x_{πβ (γ+1)} + m∑ l=1 λ_lx_l + λ_0, (4) where p is a prime and p | q, λ_l ∈ Z_q, 0 ≤ l ≤ m. Then the set A = { A^0, A^1, . . . , A^{pk+δ −1} } is a (p^{k+δ} , p^k, p^m, p^{m−δ} − 1)- SZCCS, where A^t = {a^t_0, a^t_1, . . . , a^t_{pk −1}} and

a^t_σ = g + q p k∑ β=1 σ_β x_{πβ (1)} + k∑ β=1 t_βx_{πβ (mβ )}

+ δ∑ β=1 t_{k+β} x_{m−δ+β} , (5)

for σ = 0, 1, . . . , p^k − 1 and t = 0, 1, . . . , p^{k+δ} − 1 with p-ary vector representation (σ_1, σ_2, . . . , σ_k ) and (t_1, t_2, . . . , t_k, . . . , t_{k+δ} ), respectively.

Proof: We will prove that the set A = { A^0, A^1, . . . , A^{pk+δ −1} } obtained from Theorem 1 satisfies two conditions P 1 and P 2 given in Definition 3, with K = p^{k+δ} , M = p^k, N = p^m, and Z = p^{m−δ} − 1, and hence a (p^{k+δ} , p^k, p^m, p^{m−δ} − 1)-SZCCS. Let the p-ary representations of 0 ≤ r, s < p^m be (r_1, r_2, . . . , r_m) and (s_1, s_2, . . . , s_m), respectively. Let a^t_σ = (a^t_{σ,0}, a^t_{σ,1}, . . . , a^t_{σ,p}m_{−1}). First, we prove the property P 1 of Definition 3, i.e., for T_1 = {1, 2, . . . , p^{m−δ} − 1} and T_2 = {p^m − p^{m−δ} − 1, p^m − p^{m−δ}, . . . , p^m − 1} the AACF for every A^t zero, i.e., p^k −1∑

σ=0 A(a^t_σ )(τ) = p^m −τ −1 ∑ r=0 p^k −1∑

σ=0 ω (a^t_{σ,r} −a^t_{σ,r+τ} ) q = 0, (6)

for all |τ| ∈ (T_1 ∪ T_2) ∩ T , where T = {1, 2, . . . , p^m − 1}. Let s = r + τ for any integer r. Then we consider the two cases listed below.

Case I: r_{πβ (1)} ≠ s_{πβ (1)} for some β ∈ {1, 2, . . . , k}. Then there exist a^t_{σj} = (a^t_{σj ,0}, a^t_{σj ,1}, . . . , a^t_{σj ,pm−1}) = a^t_σ + (jq/p)x_{πβ (1)} ∈ A^t, where 1 ≤ j ≤ p − 1, such that a^t_σj_{,r} − a^t_{σ,r} = jq p r_{πβ (1)}, (7) and a^t_σj_{,s} − a^t_{σ,s} = jq p s_{πβ (1)}. (8)

So from the above two equations, we get ( a^t_σj_{,r} − a^t_σj_{,s} ) − ( a^t_{σ,r} − a^t_{σ,s} ) = jq p ( r_{πβ (1)} − s_{πβ (1)} ) . (9)

Raising to the power of q-th root of unity and then taking sum over 1 ≤ j ≤ p − 1, we get p−1∑ j=1 ω ( a^t_{σj ,r} −a^t_{σj ,s} ) −(a^t_{σ,r} −a^t_{σ,s}) q = p−1∑ j=1 ω^j ( r_{πβ (1)} −s_{πβ (1)} ) p = −1. (10) Hence, ω(^{atσ,r −atσ,s}) q + p−1∑ j=1 ω ( a^t_{σj ,r} −a^t_{σj ,s} ) q = 0. (11)

So, the sum AACF is zero. i.e., p^k −1∑

σ=0 A(a^t_σ )(τ) = 0. (12)

Case II: r_{πβ (1)} = s_{πβ (1)} for all β ∈ {1, 2, . . . , k}. Then, there exist integers β̂ and γ̂ such that β̂ is the largest integer satisfying r_{πβ (γ)} = s_{πβ (γ)} for all β = 1, 2, . . . , β̂ − 1, and γ = 1, 2, . . . , m_α, and γ̂ is the least integer satisfying r_{πβ̂ (γ̂)} ≠ s_{πβ̂ (γ̂)} . If the above statement doesn’t hold, then we have r_i = s_i for i = 1, 2, . . . , m − δ since ⋃_k α=1 I_α = {1, 2, . . . , m − δ}. Hence the lower bound of τ is estimated as, τ = s − r = m∑ i=m−δ+1 (s_i − r_i)p^{i−1} ≥ p^{m−δ}, (13) also the upper bound of τ is estimated as, τ =s − r = m∑ i=m−δ+1 (s_i − r_i)p^{i−1} ≤ p^{m−δ} + p^{m−δ+1} + . . . + p^{m−1} = p^m − p^{m−δ}. (14)

The above two equations (13) and (14) contradict the assumption that τ ∈ (T_1 ∪ T_2)∩T . So this guarantees the existence of integers β̂ and γ̂ with the above-mentioned conditions. Let r^j and s^j be two integer which differs from r and s, respectively, in only one position π_{β̂} (γ̂ − 1) of their p-ary representation, i.e., r^j_{πβ̂ (γ̂−1)} = r_{πβ̂ (γ̂−1)} − j and s^j_{πβ̂ (γ̂−1)} = s_{πβ̂ (γ̂−1)} − j, where 1 ≤ j ≤ p − 1. Since s = r + τ, we get s^j = r^j + τ. The difference between the terms a^t_{σ,r} − a^t_{σ,rj} is calculated below as a^t_{σ,r} − a^t_{σ,r}j = g_r − g_rj = j ( q p r_{πβ̂ (γ̂−2)} + q p r_{πβ̂ (γ̂)} + λ_{πβ̂ (γ̂−1)} ) . (15)

Similarly, it can be calculated that a^t_{σ,s} − a^t_{σ,s}j = j ( q p s_{πβ̂ (γ̂−2)} + q p s_{πβ̂ (γ̂)} + λ_{πβ̂ (γ̂−1)} ) . (16)

From the above two equations and using r_{πβ̂ (γ̂−2)} ≠ s_{πβ̂ (γ̂−2)}, we get the following equality a^t_{σ,r}j − a^t_{σ,s}j − ( a^t_{σ,r} − a^t_{σ,s} ) = j q p ( s_{πβ̂ (γ̂)} − r_{πβ̂ (γ̂)} ) . (17)

Raising to the power of q-th root of unity and then taking sum over 1 ≤ j ≤ p − 1, we get the following expression p−1∑ j=1 ω ( a^t_{σ,rj} −a^t_{σ,sj} ) −(a^t_{σ,r} −a^t_{σ,s}) q = p−1∑ j=1 ω^j ( s_{πβ̂ (γ̂)} −r_{πβ̂ (γ̂)} ) p = −1. (18) Hence, ω (a^t_{σ,r} −a^t_{σ,s}) q + p−1∑ j=1 ω ( a^t_{σ,rj} −a^t_{σ,sj} ) q = 0. (19)

So, the AACF is zero. Combining Cases I and II, we get AACF of A^t is zero for τ ∈ (T_1 ∪ T_2) ∩ T .

Next, in the following part, we will demonstrate that any two distinct sets A^{t1} and A^{t2} have zero ACCF for all |τ| ∈ {0} ∪ T_1 ∪ T_2, i.e., p^k −1∑

σ=0 C(a^{t1}_σ , a^{t2}_σ )(τ) = p^m−τ −1 ∑ r=0 p^k −1∑

σ=0 ω (a^{t1}_{σ,r} −a^{t2}_{σ,r+τ} ) q = 0. (20) Similar to the first part, we let s = r + τ for any integer r and consider two cases.

Case I: Suppose r_{πβ (1)} ≠ s_{πβ (1)} for some β ∈ {1, 2, . . . , k}. In the same manner as Case I in the first part there exist a^t_{σj} = (a^t_{σj ,0}, a^t_{σj ,1}, . . . , a^t_{σj ,pm−1}) = a^t_σ + (jq/p)x_{πβ (1)} ∈ A^t, for t = t_1, t_2, where 1 ≤ j ≤ p − 1, such that p−1∑ j=1 ω ( a^{t1}_{σj ,r} −a^{t2}_{σj ,s} ) −(a^{t1}_{σ,r} −a^{t2}_{σ,s}) q = p−1∑ j=1 ω^j ( r_{πβ (1)} −s_{πβ (1)} ) p = −1. (21) Hence, similar to the first part, the ACCF becomes zero, i.e., p^k −1∑

σ=0 ω (a^{t1}_{σ,r} −a^{t2}_{σ,s}) q = 0. (22)

Case II: Suppose we have r_{πβ (1)} = s_{πβ (1)} for all β ∈ {1, 2, . . . , k}. As argued in Case II in the first part, a similar result can be obtained, i.e., ω (a^{t1}_{σ,r} −a^{t2}_{σ,s}) q + p−1∑ j=1 ω ( a^{t1}_{σ,rj} −a^{t2}_{σ,sj} ) q = 0. (23)

So, from Case I and Case II, we get ∑_pk_{−1} σ=0 C(a^{t1}_σ , a^{t2}_σ )(τ) = 0, for |τ| ∈ T_1 ∪ T_2. It only suffices to show that p^k −1∑

σ=0 C(a^{t1}_σ , a^{t2}_σ )(0) = p^k −1∑

σ=0 p^m−1∑

r=0 ω(^{at1σ,r −at2σ,r}) q = 0. (24)

Let ⊕ denotes modulo-p addition; let (t_{11}, t_{12}, . . . , t_{1k+δ} ) and (t_{21}, t_{22}, . . . , t_{2k+δ} ) denote the p-ary representations of t_1 and t_2, respectively. Then, for σ = 0, 1, . . . , p^k − 1, we have a^{t1}_σ − a^{t2}_σ ≡ (q/p)d (mod q) where d = (t_{11} ⊕ t_{21})x_{π1(m1 )} ⊕ (t_{12} ⊕ t_{22})x_{π2 (m2)} ⊕ · · · ⊕ (t_{1k} ⊕ t_{2k})x_{πk (mk )}⊕ (t_{1k+1} ⊕ t_{1k+1})x_{m−δ+1} ⊕ · · · ⊕ (t_{1k+δ} ⊕ t_{2k+δ} )x_m. For every 1 ≤ β ≤ k, x_{πβ (mβ )} takes each value from {0, 1, . . . , p − 1} exactly p^{m−1} times. Also for 1 ≤ β ≤ δ, x_{m−δ+β} takes each value from {0, 1, . . . , p − 1} exactly p^{m−1} times. So, d also takes each value from {0, 1, . . . , p − 1} exactly p^{m−1} times, i.e., it is balanced. So, p^m−1∑

r=0 ω(^{at1σ,r −at2σ,r} ) q = p^m−1∑

r=0 ω^{dr}_p = 0. (25)

Therefore, from (24) and (25) the ACCF at shift τ = 0 is zero, i.e.,_{pk −1} ∑ σ=0 C(a^{t1}_σ , a^{t2}_σ )(0) = 0. (26)

The proposed SZCCS in Theorem 1, is optimal since K = p^{k+δ} = p^k(p^m/p^{m−δ}) = M(N/(Z + 1)).

Remark 1: For δ = 0, the proposed construction generates (p^k, p^k, p^m)-CCC. So, the construction of (p^k, p^k, p^m)-CCC, in [17], [18] become particular cases of the proposed construction.

Remark 2: For p = 2, the proposed construction generates (2^{k+δ} , 2^k, 2^m, 2^{m−δ})-ZCCS, so the available construction of ZCCS provided in [19] is a special case of the proposed construction.

Remark 3: In [20], direct construction of (p^{δ+1}, p, p^m, p^{m−δ})-ZCCS is provided, the proposed construction with k = 1 generates the ZCCS with the same parameter.

Remark 4: Since every SZCCS is a ZCCS, the construction of (p^{n+v} , p^n, p^m, p^{m−v})-ZCCS in [14] occurs as a special case of the proposed construction in Theorem 1.

Remark 5: The construction of (8, 2, 2^m, 2^{m−2} −1)-SZCCS is given is [15], which appears as a special case of the proposed construction when p = 2, δ = 2, k = 1.

We provide the following example to illustrate how optimal SZCCS is obtained from Theorem 1.

Example 1: For m = 3, δ = 1, let π_1 = π is the identity permutation of {1, 2}, i.e. π(1) = 1 and π(2) = 2. Further let us take p = 3 and q = 3 and define the MVF g : {0, 1, 2}^3 → Z_3 as g(x_1, x_2, x_3) = x_1x_2. Also let us define the sets A^t = {f +σ_1x_1 +t_1x_2 +t_2x_3 : σ_1 ∈ {0, 1, 2}}, for t = 0, 1, . . . , 8 with p-ary representation (t_1, t_2). So, from Theorem 1, A = {A^0, A^1, . . . , A^8} is a (9, 3, 27, 8)-SZCCS. The codes A^0, A^1, . . . , A^8 are listed in Table I explicitly, where by integer i, we mean ω^i where ω = exp(2π √ −1/3), and AACF graph of A^0 is plotted in Fig. 1, and ACCF graph of A^2 and A^8 in Fig. 2.

TABLE I: Different codes of the SZCSS obtained from Example 1

A^0 A^1 000012021000012021000012021 000120210000120210000120210 000201102000201102000201102

012021000012021000012021000 012102222012102222012102222 012210111012210111012210111 A^2 A^3 021000012021000012021000012 021111201021111201021111201 021222120021222120021222120

000012021111120102222201210 000120210111201021222012102 000201102111012210222120021 A^4 A^5 012021000120102111201210222 012102222120210000201021111 012210111120021222201102000

021000012102111120210222201 021111201102222012210000120 021222120102000201210111012 A^6 A^7 000012021222201210111120102 000120210222012102111201021 000201102222120021111012210

012021000201210222120102111 012102222201021111120210000 012210111201102000120021222 A^8 021000012210222201102111120 021111201210000120102222012 021222120210111012102000201

Fig. 1: AACF of A^0.

Fig. 2: ACCF of A^2 and A^8.

IV. COMPARISON WITH EXISTING WORKS

In the literature, research on SZCCS is relatively recent, with only constructions available for (8, 2, 2^m, 2^{m−2} − 1)- SZCCS [15] and (2, 2, 2^{m−1} + 2^v, 2^v − 1)-SZCCS [21]. Optimal SZCCS are utilized in the design of optimal training sequences for GSM systems, which can achieve superior channel estimation performance compared to other sequence classes [15], [21]. The proposed construction in Theorem 1 produces optimal SZCCS with variable set size (p^{k+δ} ), flock size (p^k), sequence length (p^m), and ZCZ width (p^{m−δ} − 1). Thus, due to the flexibility of parameters, the proposed SZCCS offers adaptability in generating optimal training matrices for GSM systems with multiple active transmit antennas [21].

Based on definitions 2 and 3, it is clear that a ZCCS can be regarded as a particular case of an SZCCS, where T_2 = ϕ and T_1 = {1, 2, . . . , Z − 1}. Moreover, according to Lemma 1, optimality of SZCCS implies optimality of ZCCS. Consequently, as detailed in Remark 1-4, the existing constructions of CCC in [17], [18] and ZCCS in [14], [19], [20] can be viewed as special cases of the proposed construction.

V. CONCLUSION

An optimal SZCCS of prime power length has been constructed directly using MVF in this paper. Since SZCCS have both front-end and tail-end ZCZ width, they are used in designing optimal training sequences for broadband GSM systems over frequency-selective channels. The proposed MVFbased construction generates optimal (p^{k+δ} , p^k, p^m, p^{m−δ} − 1)-SZCCS, which generalizes many of the existing works of ZCCS and SZCCS.

REFERENCES

[1] P. Fan, W. Yuan, and Y. Tu, “Z-complementary binary sequences,” IEEE Signal Process. Lett., vol. 14, no. 8, pp. 509–512, Aug. 2007.

[2] C.-Y. Pai, S.-W. Wu, and C.-Y. Chen, “Z-complementary pairs with flexible lengths from generalized Boolean functions,” IEEE Commun. Lett., vol. 24, no. 6, pp. 1183–1187, 2020.

[3] C.-Y. Chen, “A novel construction of Z-complementary pairs based on generalized Boolean functions,” IEEE Signal Process. Lett., vol. 24, no. 7, pp. 987–990, 2017.

[4] A. R. Adhikary, P. Sarkar, and S. Majhi, “A direct construction of q-ary even length Z-complementary pairs using generalized Boolean functions,” IEEE Signal Process. Lett., vol. 27, pp. 146–150, 2020.

[5] A. R. Adhikary, S. Majhi, Z. Liu, and Y. L. Guan, “New sets of optimal odd-length binary Z-complementary pairs,” IEEE Trans. Inf. Theory, vol. 66, no. 1, pp. 669–678, 2020.

[6] P. Kumar, P. Sarkar, S. Majhi, and S. Paul, “A direct construction of even length ZCPs with large ZCZ ratio,” Cryptogr. Commun., vol. 15, pp. 85–94, 2023.

[7] L. Feng, P. Fan, X. Tang, and K. K. Loo, “Generalized pairwise Zcomplementary codes,” IEEE Signal Process. Lett., vol. 15, pp. 377–380, 2008.

[8] S.-W. Wu, A. Şahin, Z.-M. Huang, and C.-Y. Chen, “Z-complementary code sets with flexible lengths from generalised Boolean functions,” IEEE Access, vol. 9, pp. 4642–4652, 2021.

[9] P. Sarkar, S. Majhi, and Z. Liu, “Optimal Z-complementary code set from generalized Reed-Muller codes,” IEEE Trans. Commun., vol. 67, no. 3, pp. 1783–1796, 2019.

[10] B. Shen, Y. Yang, P. Fan, and Z. Zhou, “New Zcomplementary/complementary sequence sets with non-power-of-two length and low PAPR,” Cryptogr. Commun., 2022.

[11] G. Ghosh, S. Majhi, P. Sarkar, and A. K. Upadhaya, “Direct construction of optimal Z-complementary code sets with even lengths by using generalized Boolean functions,” IEEE Signal Process. Lett., vol. 29, pp. 872–876, 2022.

[12] C. Xie, Y. Sun, and Y. Ming, “Constructions of optimal binary Zcomplementary sequence sets with large zero correlation zone,” IEEE Signal Process. Lett., vol. 28, pp. 1694–1698, 2021.

[13] L. Tian, Y. Li, Z. Zhou, and C. Xu, “Two classes of Z-complementary code sets with good cross-correlation subsets via paraunitary matrices,” IEEE Trans. Commun., vol. 69, no. 5, pp. 2935–2947, 2021.

[14] X. Men and Y. Li, “New construction of multiple complete complementary codes with inter-set zero cross-correlation zone,” IEEE Signal Process. Lett., vol. 29, pp. 1958–1962, 2022.

[15] Y. Zhou, Z. Zhou, Z. Liu, Y. Yang, P. Yang, and P. Fan, “Symmetrical Zcomplementary code sets for optimal training in generalized spatial modulation,” in 10th Int. Workshop Signal Des. Appl. Commun. (IWSDA), 2022, pp. 1–5.

[16] L. Feng, P. Fan, and X. Zhou, “Lower bounds on correlation of Zcomplementary code sets.” Wireless Pers Commun, p. 1475–1488, 2013.

[17] P. Sarkar, Z. Liu, and S. Majhi, “Multivariable function for new complete complementary codes with arbitrary lengths,” 2021. [Online]. Available: https://arxiv.org/abs/2102.10517 [18] N. Kumar, S. Majhi, and A. K. Upadhyay, “A direct construction of complete complementary code with zero correlation zone property for prime-power length,” 2022. [Online]. Available: https://arxiv.org/abs/ 2207.13642 [19] S.-W. Wu and C.-Y. Chen, “Optimal Z-complementary sequence sets with good peak-to-average power-ratio property,” IEEE Signal Process. Lett., vol. 25, no. 10, pp. 1500–1504, 2018.

[20] B. Shen, H. Meng, Y. Yang, and Z. Zhou, “New constructions of Z-complementary code sets and mutually orthogonal complementary sequence sets,” Des. Codes Cryptogr., 2022.

[21] Y. Zhou, Z. Zhou, Z. Liu, Y. Yang, P. Yang, and P. Fan, “Symmetrical z-complementary code sets for optimal training in generalized spatial modulation,” Signal Processing, vol. 208, p. 108990, 2023. [Online]. Available: https://www.sciencedirect.com/science/article/pii/ S0165168423000646